{"text_format":"1","workbook":"xls","n_sheets":3,"sheets":["PLANILHA","Reparo Profundo","Plan3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PLANILHA","index":0,"n_rows":13084,"n_cols":19,"rows_kept":4500,"cut":true,"hidden":false,"merged":[[0,0,0,7],[1,0,1,7],[2,1,2,7],[3,1,3,7],[4,1,4,7],[5,0,5,7],[6,0,6,7],[7,0,7,7],[8,0,8,3],[8,4,8,7],[9,0,10,0],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,10,4],[9,5,10,5],[9,6,10,6],[9,7,10,7],[11,1,11,4],[12,1,12,4],[62,1,62,4],[117,1,117,4],[145,1,145,4]],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0},"flags":["formulas_cached_only"]}
[" "]
[null,null,null,null,null,null,null,null,null,1.259]
[null,"PREFEITURA DO MUNICÍPIO DE MAUÁ"]
[null,"Secretaria de Obras"]
[null,null,null,null,null,null,null,null,null,""]
["PLANILHA DE QUANTIDADES E PREÇOS"]
[]
["Objeto: Revitalização e Reurbanização da Região do Bairro Capuava."]
[null,null,null,null,"BASE: SET/2014"]
["ITEM","DESCRIÇÃO","UNIDADE ","QUANTIDADE","PREÇO UNITÁRIO (R$)","PREÇO TOTAL (R$)","FONTE","CÓDIGO"]
[null,null,null,null,null,null,"FONTE","CÓDIGO"]
[null,"REVITALIZAÇÃO E REURBANIZAÇÃO DA REGIÃO DO BAIRRO CAPUAVA"]
[null,"PRAÇA - AVENIDA DO ESTADO (CAPUAVA)",null,null,null,0]
[1,"PAISAGISMO",null,null,null,0]
["1.1","LIMP.TERRENO C/DEST.ARV.PERIMETRO<=78CM","m²",3031.13,null,0,"DER","22.01.02",null,null,null,null,null,null,null,null,null,null,0.69]
["1.2","CARGA DE MATERIAL LIMPEZA","m³",5181.34,null,0,"DER","22.02.06",null,null,null,null,null,null,null,null,null,null,2.24]
["1.3","TRANSPORTE MATERIAL DE LIMPEZA ATE 1 KM","m³*km",5181.34,null,0,"DER","22.03.11",null,null,null,null,null,null,null,null,null,null,4.12]
["1.4","TRANSPORTE MATERIAL DE LIMP.ALEM DE 1 KM","m³*km",46632.05,null,0,"DER","22.03.12",null,null,null,null,null,null,null,null,null,null,2.58]
["1.5","ESPALHAMENTO/REGULARIZACAO/COMPACTACAO DE MATERIAL EM BOTA-FORA.","m³",5181.34,null,0,"DER","22.02.09",null,null,null,null,null,null,null,null,null,null,2.22]
["1.6","GRAMA PLACA COM ADUBO","m²",5821.67,null,0,"DER","30.01.02",null,null,null,null,null,null,null,null,null,null,7.64]
["1.7","MARANTA FOLHA DE PRATA - PLANTIO DE GRAMINEAS SEMENTE TELA BIODEG","m²",155.66,null,0,"DER","30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.8","ONZE HORAS - PLANTIO DE GRAMINEAS SEMENTE TELA BIODEG","m²",451.59,null,0,"DER","30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.9","SANGUE DE ADÃO - PLANTIO DE GRAMINEAS SEMENTE TELA BIODEG","m²",150.31,null,0,"DER","30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.10","VEDÉLIA - PLANTIO DE GRAMINEAS SEMENTE TELA BIODEG","m²",232.68,null,0,"DER","30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.11","ESPONJA - PLANTIO DE ARBUSTOS","un",169,null,0,"DER","30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.12","LANTANA BRANCA - PLANTIO DE ARBUSTOS","un",286,null,0,"DER","30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.13","GUAIMBÊ - PLANTIO DE ARBUSTOS","un",42,null,0,"DER","30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.14","MULUNGU DO LITORAL - PLANTIO DE ÁRVORES","un",8,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.15","MANDUIRANA - PLANTIO DE ÁRVORES","un",6,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.16","ALELUIA - PLANTIO DE ÁRVORES","un",10,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.17","JERIVÁ - PLANTIO DE ÁRVORES","un",7,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.18","IPÊ AMARELO - PLANTIO DE ÁRVORES","un",10,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.19","QUARESMEIRA - PLANTIO DE ÁRVORES","un",4,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.20","MANACÁ DA SERRA - PLANTIO DE ÁRVORES","un",5,null,0,"DER","30.01.22",null,null,null,null,null,null,null,null,null,null,43.18]
["1.21","ENROCAMENTO PEDRA JOGADA","m³",506.852,null,0,"DER","24.09.03",null,null,null,null,null,null,null,null,null,null,135.39]
[2,"PAVIMENTAÇÃO, PASSEIOS E GUIAS",null,null,null,0]
["2.1","FRESAGEM CONTINUA DE PAV., INDEPENDENTE DA ESPESSURA","m³",27.96,null,0,"DER","23.10.01",null,null,null,null,null,null,null,null,null,null,143.78]
["2.2","CAMADA ROLAMENTO - CBUQ - GRAD.C - COM DOP","m³",27.96,null,0,"DER","23.08.03.03",null,null,null,null,null,null,null,null,null,null,541.99]
["2.3",0,0,932,null,0,0,"23.05.02",null,null,null,null,null,null,null,null,null,null,1.33]
["2.4",0,0,53.5,null,0,0,"24.19.03.01",null,null,null,null,null,null,null,null,null,null,47.02]
["2.5",0,0,349.8,null,0,0,"22.02.01",null,null,null,null,null,null,null,null,null,null,4.5600000000000005]
["2.6",0,0,3498,null,0,0,"22.03.04",null,null,null,null,null,null,null,null,null,null,1.47]
["2.7",0,0,145.75,null,0,0,"23.04.03.02",null,null,null,null,null,null,null,null,null,null,134.28]
["2.8",0,0,204.05,null,0,0,"26.09.05",null,null,null,null,null,null,null,null,null,null,471.74]
["2.9",0,0,651,null,0,0,"21.03.08",null,null,null,null,null,null,null,null,null,null,17.97]
[3,"ILUMINAÇÃO",null,null,null,0]
["3.1",0,0,3,null,0,0,"042114"]
["3.2",0,0,6,null,0,0,"411024"]
[4,"DRENAGEM",null,null,null,0]
["4.1",0,0,3,null,0,0,"21.03.07",null,null,null,null,null,null,null,null,null,null,69.95]
["4.2",0,0,4,null,0,0,"21.05.02",null,null,null,null,null,null,null,null,null,null,154.1]
["4.3",0,0,5,null,0,0,"22.02.09",null,null,null,null,null,null,null,null,null,null,2.22]
["4.4",0,0,6,null,0,0,"24.02.01",null,null,null,null,null,null,null,null,null,null,45.76]
["4.5",0,0,7,null,0,0,"24.05.01",null,null,null,null,null,null,null,null,null,null,75.54]
["4.6",0,0,8,null,0,0,"24.06.02",null,null,null,null,null,null,null,null,null,null,8.37]
["4.7",0,0,9,null,0,0,"24.07.01",null,null,null,null,null,null,null,null,null,null,386.56]
["4.8",0,0,10,null,0,0,"24.07.02",null,null,null,null,null,null,null,null,null,null,428.4]
["4.9",0,0,11,null,0,0,"24.07.05",null,null,null,null,null,null,null,null,null,null,471.74]
["4.10",0,0,12,null,0,0,"24.11.05",null,null,null,null,null,null,null,null,null,null,442.99]
["4.11",0,0,13,null,0,0,"24.11.07",null,null,null,null,null,null,null,null,null,null,31.93]
["4.12",0,0,14,null,0,0,"24.19.03.01",null,null,null,null,null,null,null,null,null,null,47.02]
["4.13",0,0,15,null,0,0,"27.01.04",null,null,null,null,null,null,null,null,null,null,1.29]
[null,"PRAÇA  ESTAÇÃO CAPUAVA",null,null,null,0]
[1,"PAISAGISMO",null,null,null,0]
["1.1",0,0,342.68,null,0,0,"22.01.02",null,null,null,null,null,null,null,null,null,null,0.69]
["1.2",0,0,102.804,null,0,0,"22.02.06",null,null,null,null,null,null,null,null,null,null,2.24]
["1.3",0,0,102.8,null,0,0,"22.03.11",null,null,null,null,null,null,null,null,null,null,4.12]
["1.4",0,0,925.24,null,0,0,"22.03.12",null,null,null,null,null,null,null,null,null,null,2.58]
["1.5",0,0,102.8,null,0,0,"22.02.09",null,null,null,null,null,null,null,null,null,null,2.22]
["1.6",0,0,342.68,null,0,0,"30.01.02",null,null,null,null,null,null,null,null,null,null,7.64]
["1.7","CORAÇÃO DE JESUS - PLANTIO DE GRAMINEAS",0,31.54,null,0,0,"30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.8","MARANTA-BICOLOR - PLANTIO DE GRAMINEAS",0,21.35,null,0,0,"30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.9","SANGUE DE ADÃO - PLANTIO DE GRAMINEAS",0,10.73,null,0,0,"30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.10","VEDÉLIA - PLANTIO DE GRAMINEAS",0,7.52,null,0,0,"30.01.30",null,null,null,null,null,null,null,null,null,null,12.14]
["1.11","CALATÉIA-ZEBRA - PLANTIO DE ARBUSTOS",0,16,null,0,0,"30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.12","ESPONJA - PLANTIO DE ARBUSTOS",0,19,null,0,0,"30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.13","MARIANINHA - PLANTIO DE ARBUSTOS",0,31,null,0,0,"30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.14","LANTANA BRANCA - PLANTIO DE ARBUSTOS",0,6,null,0,0,"30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["1.15","LÍRIO-ROXO-DAS-PEDRAS - PLANTIO DE ARBUSTOS",0,16,null,0,0,"30.01.21",null,null,null,null,null,null,null,null,null,null,15.55]
["2","PISOS, GUIAS E PASSEIOS",null,null,null,0]
["2.1",0,0,295,null,0,0,"24.19.03.01",null,null,null,null,null,null,null,null,null,null,47.02]
["2.2",0,0,17.33,null,0,0,"27.01.03",null,null,null,null,null,null,null,null,null,null,287.75]
["2.3",0,0,5940,null,0,0,"27.01.04",null,null,null,null,null,null,null,null,null,null,1.29]
["2.4",0,0,29.71,null,0,0,"22.02.01",null,null,null,null,null,null,null,null,null,null,4.5600000000000005]
["2.5",0,0,297.1,null,0,0,"22.03.04",null,null,null,null,null,null,null,null,null,null,1.47]
["2.6",0,0,12.38,null,0,0,"23.04.03.02",null,null,null,null,null,null,null,null,null,null,134.28]
["2.7",0,0,17.33,null,0,0,"26.09.05",null,null,null,null,null,null,null,null,null,null,471.74]
["2.8",0,0,697.15,null,0,0,"540404"]
["2.9",0,0,697.15,null,0,0,"540405"]
["2.10",0,0,257.13,null,0,0,"170304"]
["2.11",0,0,27,null,0,0,"21.03.08",null,null,null,null,null,null,null,null,null,null,17.97]
["3","ILUMINAÇÃO",null,null,null,0]
["3.1",0,0,16,null,0,0,"411043"]
["3.2",0,0,3,null,0,0,"411024"]
["4","DRENAGEM",null,null,null,0]
["4.1",0,0,43.29,null,0,0,"22.02.09",null,null,null,null,null,null,null,null,null,null,2.22]
["4.2",0,0,41.22,null,0,0,"24.02.01",null,null,null,null,null,null,null,null,null,null,45.76]
["4.3",0,0,4.61,null,0,0,"24.02.08",null,null,null,null,null,null,null,null,null,null,56.62]
["4.4",0,0,7.68,null,0,0,"24.03.07",null,null,null,null,null,null,null,null,null,null,61.49]
["4.5",0,0,60.55,null,0,0,"24.05.01",null,null,null,null,null,null,null,null,null,null,75.54]
["4.6",0,0,523.6,null,0,0,"24.06.02",null,null,null,null,null,null,null,null,null,null,8.37]
["4.7",0,0,2.11,null,0,0,"24.07.01",null,null,null,null,null,null,null,null,null,null,386.56]
["4.8",0,0,54.04,null,0,0,"24.07.02",null,null,null,null,null,null,null,null,null,null,428.4]
["4.9",0,0,4.9,null,0,0,"24.07.05",null,null,null,null,null,null,null,null,null,null,471.74]
["4.10",0,0,6.69,null,0,0,"24.11.05",null,null,null,null,null,null,null,null,null,null,442.99]
["4.11",0,0,33.44,null,0,0,"24.11.07",null,null,null,null,null,null,null,null,null,null,31.93]
["4.12",0,0,0.98,null,0,0,"24.12.01.01",null,null,null,null,null,null,null,null,null,null,101.31]
["4.13",0,0,2.54,null,0,0,"24.12.08",null,null,null,null,null,null,null,null,null,null,21.65]
["4.14",0,0,6,null,0,0,"24.16.02",null,null,null,null,null,null,null,null,null,null,139.22]
["4.15",0,0,5,null,0,0,"24.19.03.01",null,null,null,null,null,null,null,null,null,null,47.02]
["4.16",0,0,8.99,null,0,0,"24.19.04.01",null,null,null,null,null,null,null,null,null,null,592.09]
["4.17",0,0,1,null,0,0,"24.19.06",null,null,null,null,null,null,null,null,null,null,441.62]
["4.18",0,0,5,null,0,0,"24.19.08",null,null,null,null,null,null,null,null,null,null,412.81]
["5","DIVERSOS",null,null,null,0]
["5.1",0,0,8.55,null,0,0,"24.11.05",null,null,null,null,null,null,null,null,null,null,442.99]
["5.2",0,0,17.1,null,0,0,"170222"]
["5.3",0,0,17.1,null,0,0,"37.01.24",null,null,null,null,null,null,null,null,null,null,23.28]
[null,"RECAPEAMENTO DA RUA MANOEL DA NÓBREGA",null,null,null,0]
["1","DEMOLIÇÃO E REMOÇÃO",null,null,null,0]
["1.1",0,0,259.88,null,0,0,"21.05.01",null,null,null,null,null,null,null,null,null,null,287.75]
["1.2",0,0,1582.46,null,0,0,"21.03.08",null,null,null,null,null,null,null,null,null,null,17.97]
["1.3","DEMOLICAO DE CONCRETO SIMPLES (SARJETA)",0,712.11,null,0,0,"21.05.02",null,null,null,null,null,null,null,null,null,null,154.1]
["1.4",0,0,11556.77,null,0,0,"27.01.04",null,null,null,null,null,null,null,null,null,null,1.29]
["1.5",0,0,492.91,null,0,0,"22.02.09",null,null,null,null,null,null,null,null,null,null,2.22]
["2","PAVIMENTAÇÃO",null,null,null,0]
["2.1","RECAPEAMENTO",null,null,null,0]
["2.1.1",0,0,58.62,null,0,0,"23.10.01",null,null,null,null,null,null,null,null,null,null,143.78]
["2.1.2",0,0,6703.61,null,0,0,"23.05.02",null,null,null,null,null,null,null,null,null,null,1.33]
["2.1.3",0,0,335.18,null,0,0,"23.08.02.02",null,null,null,null,null,null,null,null,null,null,581.55]
["2.2","REPARO PROFUNDO",null,null,null,0]
["2.1",0,0,110.64,null,0,0,"21.05.07",null,null,null,null,null,null,null,null,null,null,28.57]
["2.2",0,0,15.81,null,0,0,"23.08.02.02",null,null,null,null,null,null,null,null,null,null,581.55]
["2.3",0,0,31.61,null,0,0,"23.08.01",null,null,null,null,null,null,null,null,null,null,468.98]
["2.4",0,0,63.22,null,0,0,"24.07.02",null,null,null,null,null,null,null,null,null,null,428.4]
["2.5",0,0,316.11,null,0,0,"23.05.01",null,null,null,null,null,null,null,null,null,null,3.49]
["2.6",0,0,632.22,null,0,0,"23.05.02",null,null,null,null,null,null,null,null,null,null,1.363]
["2.3","PASSEIOS, GUIAS E SARJETAS",null,null,null,0]
["2.3.1",0,0,21,null,0,0,"24.10.02",null,null,null,null,null,null,null,null,null,null,595.94]
["2.3.2",0,0,15,null,0,0,"24.12.01.02",null,null,null,null,null,null,null,null,null,null,108.1]
["2.3.3",0,0,27,null,0,0,"24.19.04.01",null,null,null,null,null,null,null,null,null,null,592.09]
["2.3.4",0,0,400,null,0,0,"24.19.03.01",null,null,null,null,null,null,null,null,null,null,47.02]
["2.3.5","LEVANTAMENTO OU REBAIXAMENTO DE TAMPÃO DE POÇO DE VISITA","un",18,null,0,"SIURB","06-21-00"]
["3","URBANISMO E PAISAGISMO",null,null,null,0]
["3.1","FORRAÇÕES",null,null,null,0]
["3.1.1",0,0,307.51,null,0,0,"37.06.02",null,null,null,null,null,null,null,null,null,null,7.67]
[null,"TOTAL (R$)",null,null,null,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1000,1.35]
[null,null,null,null,null,null,null,null,null,null,"Subitem","Nome","unidade","Preço unitário","Preço unitário Sem BDI","Fonte"]
[null,null,null,null,null,null,null,null,null,null,"21.01.01","SONDAGEM A PERCUSSAO ATE 15M","m",122.84,90.99259259259259,"DER",122840]
[null,null,null,null,null,null,null,null,null,null,"21.01.02","SONDAGEM A PERC. ATE 15M LOC. ALAG.<50CM","m",181.96,134.78518518518518,"DER",181960]
[null,null,null,null,null,null,null,null,null,null,"21.01.03","SONDAGEM A  PERCUSSAO DE 15 A 30M","m",144.56,107.08148148148148,"DER",144560]
[null,null,null,null,null,null,null,null,null,null,"21.01.04","SONDAGEM A PERC.15A30M LOC.ALAG.<50CM","m",222.4,164.74074074074073,"DER",222400]
[null,null,null,null,null,null,null,null,null,null,"21.01.05","SONDAGEM PERCUSSAO SUPERIOR A 30M","m",166.8,123.55555555555556,"DER",166800]
[null,null,null,null,null,null,null,null,null,null,"21.01.06","SONDAGEM PERC.+30M LOC.ALAG.<50CM","m",252.73,187.20740740740737,"DER",252730]
[null,null,null,null,null,null,null,null,null,null,"21.01.07","TAXA FIXA INSTALACAO SONDAGEM PERCUSSAO","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.047,490"]
[null,null,null,null,null,null,null,null,null,null,"21.01.08","TAXA FIXA INSTALACAO SONDAGEM ROTATIVA","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.557,970"]
[null,null,null,null,null,null,null,null,null,null,"21.01.09","TRANSPORTE DE EQUIPAMENTO DE SONDAGEM","km*equip",10.65,7.888888888888888,"DER",10650]
[null,null,null,null,null,null,null,null,null,null,"21.01.10","DESLOCAMENTO DE EQUIPAMENTO DE SONDAGEM","m",7.6,5.629629629629629,"DER",7600]
[null,null,null,null,null,null,null,null,null,null,"21.01.11","PLATAFORMA OU BANQUETA SOND.PERCUSSAO","equip",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.651,360"]
[null,null,null,null,null,null,null,null,null,null,"21.01.12","PLATAFORMA OU BANQUETA P/ SOND. ROTATIVA","equip",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.819,690"]
[null,null,null,null,null,null,null,null,null,null,"21.01.14","FLUTUANTE PARA SONDAGEM","obra",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","10.548,310"]
[null,null,null,null,null,null,null,null,null,null,"21.01.15","INSTAL.SONDAGEM PERCUSSAO S/ FLUTUANTE","sond",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.228,390"]
[null,null,null,null,null,null,null,null,null,null,"21.01.16","INSTALACAO SONDAGEM ROTATIVA S/FLUTUANTE","sond",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.275,710"]
[null,null,null,null,null,null,null,null,null,null,"21.01.17","SONDAGEM ROTATIVA SOLO 57,10MM (AX)","m",276.39,204.73333333333332,"DER",276390]
[null,null,null,null,null,null,null,null,null,null,"21.01.18","SONDAGEM ROTATIVA SOLO 73,00MM (BX)","m",281.5,208.5185185185185,"DER",281500]
[null,null,null,null,null,null,null,null,null,null,"21.01.19","SONDAGEM ROTATIVA SOLO 88,90MM (NX)","m",378.74,280.54814814814813,"DER",378740]
[null,null,null,null,null,null,null,null,null,null,"21.01.20","SONDAGEM ROTATIVA SOLO 114,30MM (HX)","m",409.47,303.31111111111113,"DER",409470]
[null,null,null,null,null,null,null,null,null,null,"21.01.21","SONDAGEM ROTATIVA ROCHA ALT.57,1MM (AX)","m",657.09,486.73333333333335,"DER",657090]
[null,null,null,null,null,null,null,null,null,null,"21.01.22","SONDAGEM ROTATIVA ROCHA ALT.73,0MM (BX)","m",697.52,516.6814814814815,"DER",697520]
[null,null,null,null,null,null,null,null,null,null,"21.01.23","SONDAGEM ROTATIVA ROCHA ALT.88,9MM (NX)","m",712.68,527.911111111111,"DER",712680]
[null,null,null,null,null,null,null,null,null,null,"21.01.24","SONDAGEM ROTATIVA ROCHA ALT.114,3MM (HX)","m",731.92,542.1629629629629,"DER",731920]
[null,null,null,null,null,null,null,null,null,null,"21.01.25","SONDAGEM ROTATIVA ROCHA SA 57,10MM (AX)","m",706.32,523.2,"DER",706320]
[null,null,null,null,null,null,null,null,null,null,"21.01.26","SONDAGEM ROTATIVA ROCHA SA 73,00MM (BX)","m",726.8,538.3703703703703,"DER",726800]
[null,null,null,null,null,null,null,null,null,null,"21.01.27","SONDAGEM ROTATIVA ROCHA SA 88,9MM (NX)","m",839.4,621.7777777777777,"DER",839400]
[null,null,null,null,null,null,null,null,null,null,"21.01.28","SONDAGEM ROTATIVA ROCHA SA 114,30MM (HX)","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.120,910"]
[null,null,null,null,null,null,null,null,null,null,"21.01.29","SONDAGEM A TRADO PROFunDIDADE ATE 5M","m",116.25,86.1111111111111,"DER",116250]
[null,null,null,null,null,null,null,null,null,null,"21.01.30","SONDAGEM A TRADO PROFunDIDADE 5 A 10M","m",141.53,104.83703703703704,"DER",141530]
[null,null,null,null,null,null,null,null,null,null,"21.02.01.01","DETER. COORDENADAS COM GPS2 (CONTROLE BASICO) PRECISAO MINIMA DE 2","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.060,590"]
[null,null,null,null,null,null,null,null,null,null,null,"ORDEM.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.01.02","DETER. COORDENADAS COM GPS3 (CONTROLE BASICO) PRECISAO MINIMA DE 2","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.185,340"]
[null,null,null,null,null,null,null,null,null,null,null,"ORDEM.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.02.01","TRANSPORTE COORDENADAS ATRAVES DE POLIGONAIS CLASSE II P DA NBR","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.014,280"]
[null,null,null,null,null,null,null,null,null,null,null,13.133,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.03.01","IMPLANTACAO DE POLIGONAIS CLASSE III P DA NBR 13.133.","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.603,450"]
[null,null,null,null,null,null,null,null,null,null,"21.02.04.01","TRANSPORTE DE REFERENCIA DE NIVEL ATRAVES NIVELAMENTO GEOMETRICO","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.706,040"]
[null,null,null,null,null,null,null,null,null,null,null,"4 MM K.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.05.01","TRANSPORTE DE REFERENCIA DE NIVEL ATRAVES NIVELAMENTO GEOMETRICO","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.395,810"]
[null,null,null,null,null,null,null,null,null,null,null,"CLASSE IN.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.06.01","LEV. PLANIALTIMETRICO E CADASTRAL, POLIGONAL CLASSE II PAC ESC. 1:500","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","4.676,430"]
[null,null,null,null,null,null,null,null,null,null,null,"ATE 1 HA.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.06.02","LEV. PLANIALTIMETRICO E CADASTRAL, POLIGONAL CLASSE II PAC ESC. 1:1000","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","4.320,660"]
[null,null,null,null,null,null,null,null,null,null,null,"ATE 1HA.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.07.01","LEV. PLANIALTIMETRICO E CADASTRAL, POLIGONAL CLASSE II PAC ESC. 1:500","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.891,850"]
[null,null,null,null,null,null,null,null,null,null,null,"ALEM 1HA.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.07.02","LEV. PLANIALTIMETRICO E CADASTRAL, POLIGONAL CLASSE II PAC ESC.1:1000","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.637,160"]
[null,null,null,null,null,null,null,null,null,null,null,"ALEM 1HA",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.08.01","LEV. PLANIALTIMETRICO DE FAVELAS COM AREA ATE 2000 m² C/POLIG.","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","7.659,560"]
[null,null,null,null,null,null,null,null,null,null,null,"AUXILIAR",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.09.01","LEV. PLANIALTIMETRICO DE FAVELAS COM AREA ALEM 2000 m²","m²",3.02,2.237037037037037,"DER",3020]
[null,null,null,null,null,null,null,null,null,null,null,"C/POLIG.AUXILIAR",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.10.01","LEV. PLANIALT. SECOES TRANSV. A PARTIR DE LINHA BASE EXISTENTE NIV.","m",4.97,3.681481481481481,"DER",4970]
[null,null,null,null,null,null,null,null,null,null,null,"GEOMETRICO.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.11.01","LEVANT. PLANIALTIMETRICO CADASTRAL FAIXAS ATE 30M CLASSE II PAC DA","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","8.266,540"]
[null,null,null,null,null,null,null,null,null,null,null,"NBR 13.133",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.12.01","LEVANT. PLANIALTIMETRICO CADASTRAL FAIXAS DE 30 A 60 M CLASSE II PAC","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","12.168,180"]
[null,null,null,null,null,null,null,null,null,null,null,"NBR 13.133",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.13.01","LEVANT. PLANIALTIMETRICO CADASTRAL FAIXAS ALEM 60M CLASSE II PAC DA","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.387,650"]
[null,null,null,null,null,null,null,null,null,null,null,"NBR 13.133",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.14.01","MATERIALIZACAO DE LINHA BASE PROJETADA C/ ESTAQUEAMENTO DE 20 EM","m",4.56,3.3777777777777773,"DER",4560]
[null,null,null,null,null,null,null,null,null,null,null,"20 M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.15.01","IMPL. E CADASTRO PLANIALT. LINHA BASE VIA EXISTENTE ESTAQUEAMENTO DE","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.815,700"]
[null,null,null,null,null,null,null,null,null,null,null,"20 EM 20 M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.16.01","CADASTRO DE PVA, PVE, BL E TL","un",213.37,158.05185185185184,"DER",213370]
[null,null,null,null,null,null,null,null,null,null,"21.02.17.01","CADASTRO DE OBRA DE ARTE CORRENTE (GALERIA E BUEIRO) E","m",7.29,5.3999999999999995,"DER",7290]
[null,null,null,null,null,null,null,null,null,null,null,"INTERFERENCIAS",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.18.01","LEV.CAD.ESTRUT. EM CONCRETO, PONTES E VIADUTOS, DETALHADO PECAS","tramo",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.223,000"]
[null,null,null,null,null,null,null,null,null,null,null,"ESTRUTURAIS",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.19.01","CADASTRO DE PROPRIEDADE PARA DESAPROPRIACAO URBANA.","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.991,660"]
[null,null,null,null,null,null,null,null,null,null,"21.02.20.01","CADASTRO DE PROPRIEDADE PARA DESAPROPRIACAO RURAL ATE 5000 m².","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.879,660"]
[null,null,null,null,null,null,null,null,null,null,"21.02.20.02","CADASTRO DE PROPRIEDADE PARA DESAPROPRIACAO RURAL ALEM 5000 m².","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","8.373,930"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.21.01","ABERTURA DE PICADA COM LARGURA SUFICIENTE PARA LEVANTAMENTO","m",2.67,1.9777777777777776,"DER",2670]
[null,null,null,null,null,null,null,null,null,null,null,"TOPOGRAFICO.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.22.01","LEVANTAMENTO DE SECOES TOPOBATIMETRICOS.","m",9.45,6.999999999999999,"DER",9450]
[null,null,null,null,null,null,null,null,null,null,"21.02.22.02","LEVANTAMENTO TOPOBATIMETRICO, MODO CONTINUO COM ECOBATIMETRO,","m",8.46,6.266666666666667,"DER",8460]
[null,null,null,null,null,null,null,null,null,null,null,"POSIC.COM GPS",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.23.01","LEVANTAMENTO DE BATIMETRIA ESPECIAL","equipe.dia",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","4.699,740"]
[null,null,null,null,null,null,null,null,null,null,"21.02.24.01","FORN. EQUIP.TOP., 1 TECN., 2 AUX., 1 NIVEL. C/ NIVEL AUT. ESTACAO TOTAL E","equipe.mes",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","49.868,140"]
[null,null,null,null,null,null,null,null,null,null,null,"VEIC.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.25.01","MARC.CONC. TRONCO PIR. DE 10X10CM T/ 30X30CM B/ 40CM H, PINO/CHAPA","un",110.77,82.05185185185185,"DER",110770]
[null,null,null,null,null,null,null,null,null,null,null,"COLADA TOPO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.26.01","MOBILIZACAO / DESMOBILIZACAO - DE EQUIPE E EQUIP. DE TOPOGRAFIA A 50 E","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.140,620"]
[null,null,null,null,null,null,null,null,null,null,null,"150KM",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.26.02","MOBILIZACAO / DESMOBILIZACAO - EQUIPE E EQUIP. DE TOPOGRAFIA ENTRE","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.821,470"]
[null,null,null,null,null,null,null,null,null,null,null,"151E300KM",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.26.03","MOBILIZACAO / DESMOBILIZACAO - EQUIPE E EQUIP. TOPOGRAFIA ENTRE","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.904,040"]
[null,null,null,null,null,null,null,null,null,null,null,"301E600KM",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.27.01","MOBILIZACAO DE AERONAVE DENTRO DO ESTADO.","global",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","37.484,330"]
[null,null,null,null,null,null,null,null,null,null,"21.02.28.01","COBERTURA FOTOGRAFICA POR AREA FOTOGRAFADA, VOO NA ESCALA","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.304,170"]
[null,null,null,null,null,null,null,null,null,null,null,"1:20.000",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.28.02","COBERTURA FOTOGRAFICA POR AREA FOTOGRAFADA, VOO NA ESCALA 1:5.000","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.730,670"]
[null,null,null,null,null,null,null,null,null,null,"21.02.29.01","REVELACAO DE FOTOS AEREAS INCLUSIVE ARQUIVO DIGITAL E FOTOINDICE.","un",256.03,189.65185185185183,"DER",256030]
[null,null,null,null,null,null,null,null,null,null,"21.02.30.01","RESTITUICAO VOO AEROFOTOGRAMETRICO ESC. ATE 5X SUPERIOR AO DO VOO,","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","8.888,390"]
[null,null,null,null,null,null,null,null,null,null,null,"ESC.1:5.000",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.30.02","RESTITUICAO VOO AEROFOTOGRAMETRICO ESC. ATE 5X SUPERIOR AO DO VOO,","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","42.601,420"]
[null,null,null,null,null,null,null,null,null,null,null,"ESC. 1:1.000",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.31.01","ORTOFOTOCARTA VOO AEROFOTOGRAMETRICO ESC. ATE 5X SUPERIOR AO DO","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.802,860"]
[null,null,null,null,null,null,null,null,null,null,null,"VOO, ESC.1:5000",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.31.02","ORTOFOTOCARTA VOO AEROFOTOGRAMETRICO ESC. ATE 5X SUPERIOR AO DO","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","20.657,780"]
[null,null,null,null,null,null,null,null,null,null,null,"VOO, ESC.1:1000",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.02.32.01","APOIO CAMPO AEROF. DETERM. NUM. DE PONTOS P/ RESIST. EM ESC. ATE 5X","km²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.965,640"]
[null,null,null,null,null,null,null,null,null,null,null,"MAIOR.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.03.01","REMOCAO CERCA ARAME,INCL.TRANSPORTE","m",12.03,8.91111111111111,"DER",12030]
[null,null,null,null,null,null,null,null,null,null,"21.03.02","REMOCAO DE DEFENSA METALICA SIMPLES","m",43.91,32.52592592592592,"DER",43910]
[null,null,null,null,null,null,null,null,null,null,"21.03.03","REMOCAO DE DEFENSA METALICA DUPLA","m",61.47,45.53333333333333,"DER",61470]
[null,null,null,null,null,null,null,null,null,null,"21.03.04","REMOCAO DEFENSA MET.SIMPLES P/ REINST.","m",115.1,85.25925925925925,"DER",115100]
[null,null,null,null,null,null,null,null,null,null,"21.03.05","REMOCAO DEFENSA METALICA DUPLA P/ REINST","m",138.12,102.3111111111111,"DER",138120]
[null,null,null,null,null,null,null,null,null,null,"21.03.06","REMOCAO CANALIZACAO D>=0,60M","m",79.87,59.162962962962965,"DER",79870]
[null,null,null,null,null,null,null,null,null,null,"21.03.07","REMOCAO CANALIZACAO D<0,60M","m",68.46,50.7111111111111,"DER",68460]
[null,null,null,null,null,null,null,null,null,null,"21.03.08","REMOCAO E TRANSPORTE DE GUIA PRE-MOLDADA","m",17.64,13.066666666666666,"DER",17640]
[null,null,null,null,null,null,null,null,null,null,"21.03.09","REMOCAO DE ESTACA DE EUCALIPTO","m",11.16,8.266666666666666,"DER",11160]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.03.10","REMOCAO DE TACHA REFLETIVA","un",7.01,5.192592592592592,"DER",7010]
[null,null,null,null,null,null,null,null,null,null,"21.03.11.01","REMOCAO DE PINTURA ACRIL.  DEMARC.DE VIA POR PROCESSO MANUAL","m²",50.87,37.68148148148148,"DER",50870]
[null,null,null,null,null,null,null,null,null,null,"21.04.01","CERCA DE ARAME FARPADO C/ 4 FIOS","m",44.4,32.888888888888886,"DER",44400]
[null,null,null,null,null,null,null,null,null,null,"21.04.02","CERCA DE ARAME FARPADO C/ 6 FIOS","m",49.75,36.85185185185185,"DER",49750]
[null,null,null,null,null,null,null,null,null,null,"21.04.03","CERCA ARAME FARPADO POR REAPROVEITAMENTO","m",21.18,15.688888888888888,"DER",21180]
[null,null,null,null,null,null,null,null,null,null,"21.05.01","DEMOLICAO DE CONCRETO ARMADO","m³",298.95,221.44444444444443,"DER",298950]
[null,null,null,null,null,null,null,null,null,null,"21.05.02","DEMOLICAO DE CONCRETO SIMPLES","m³",158.86,117.67407407407407,"DER",158860]
[null,null,null,null,null,null,null,null,null,null,"21.05.04","DEMOLICAO PAV.RIG.INCL.TRANSP. ATE 1 KM","m³",154.8,114.66666666666667,"DER",154800]
[null,null,null,null,null,null,null,null,null,null,"21.05.05","DEMOLICAO DE EDIFICACAO EM ALVENARIA","m²",43.2,32,"DER",43200]
[null,null,null,null,null,null,null,null,null,null,"21.05.06","DEMOLICAO DE EDIFICACAO EM MADEIRA","m²",17.84,13.214814814814813,"DER",17840]
[null,null,null,null,null,null,null,null,null,null,"21.05.07","DEMOLICAO PAVIMENTOFLEXIVEL C/TRANSPORT","m³",27.85,20.62962962962963,"DER",27850]
[null,null,null,null,null,null,null,null,null,null,"21.07.01","ABERTURA DE POCO DE INSPECAO ATE 1,5M DE PROFunDIDADE","m",799.46,592.1925925925926,"DER",799460]
[null,null,null,null,null,null,null,null,null,null,"21.07.02","ENSAIO DE UMIDADE NATURAL","un",37.31,27.637037037037036,"DER",37310]
[null,null,null,null,null,null,null,null,null,null,"21.07.03","ENSAIO DE DENSIDADE NATURAL","un",79.95,59.22222222222222,"DER",79950]
[null,null,null,null,null,null,null,null,null,null,"21.07.04","ANALISE GRANULOMETRICA POR PENEIRAMENTO E SEDIMENTACAO.","un",207.86,153.97037037037038,"DER",207860]
[null,null,null,null,null,null,null,null,null,null,"21.07.05","ENSAIO DE CBR 5 PONTOS E.N.","un",287.81,213.19259259259258,"DER",287810]
[null,null,null,null,null,null,null,null,null,null,"21.07.06","ENSAIO DE CBR 5 PONTOS E.I.","un",319.78,236.87407407407403,"DER",319780]
[null,null,null,null,null,null,null,null,null,null,"21.07.07","CLASSIFICACAO MCT (PERDA POR IMERSAO E MINI MCV).","conjunto",405.06,300.0444444444444,"DER",405060]
[null,null,null,null,null,null,null,null,null,null,"21.07.12","CLASSIFICACAO MCT - METODO PASTILHA","un",143.9,106.5925925925926,"DER",143900]
[null,null,null,null,null,null,null,null,null,null,null,"ENSAIO DE CBR 1 PONTO MOLDADO NA UMIDADE OTIMA DE COMPACTACAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"21.07.13","(E.N.)","un",234.51,173.71111111111108,"DER",234510]
[null,null,null,null,null,null,null,null,null,null,"21.07.14","ENSAIO DE COMPACTACAO - PROCTOR.","un",138.57,102.64444444444443,"DER",138570]
[null,null,null,null,null,null,null,null,null,null,"21.07.15","GRANULOMETRIA POR PENEIRAMENTO SIMPLES (SEM SEDIMENTACAO).","un",106.59,78.95555555555555,"DER",106590]
[null,null,null,null,null,null,null,null,null,null,"21.08.01","LIMPEZA DE DRENAGEM DA PLATAFORMA","m",1.05,0.7777777777777778,"DER",1050]
[null,null,null,null,null,null,null,null,null,null,"21.08.02","LIMPEZA DE BUEIROS DIAMETRO ATE 80CM","m",50.02,37.05185185185185,"DER",50020]
[null,null,null,null,null,null,null,null,null,null,"21.08.03","LIMPEZA DE BUEIROS DIAMETRO ATE 100CM","m",52.28,38.72592592592592,"DER",52280]
[null,null,null,null,null,null,null,null,null,null,"21.08.04","LIMPEZA DE BUEIROS DIAMETRO ATE 120CM","m",55.88,41.39259259259259,"DER",55880]
[null,null,null,null,null,null,null,null,null,null,"21.08.05","LIMPEZA DE BUEIROS DIAMETRO ATE 150CM","m",59.14,43.8074074074074,"DER",59140]
[null,null,null,null,null,null,null,null,null,null,"21.08.06","LIMPEZA DE GALERIA","m",52.62,38.977777777777774,"DER",52620]
[null,null,null,null,null,null,null,null,null,null,"21.08.08","DEMOLICAO E RETIRADA DE GUARDA-CORPO","m³",272.54,201.88148148148147,"DER",272540]
[null,null,null,null,null,null,null,null,null,null,"21.08.09","LIMPEZA DE BUEIROS DIAMETRO ATE 60CM","m",39.13,28.985185185185184,"DER",39130]
[null,null,null,null,null,null,null,null,null,null,"21.08.11","LIMPEZA DE DRENAGEM FORA DA PLATAFORMA","m",1.26,0.9333333333333332,"DER",1260]
[null,null,null,null,null,null,null,null,null,null,"22.01.01","LIMP.TERRENO SEM DESTOCAMENTO DE ARVORES","m²",0.28,0.2074074074074074,"DER","0,280"]
[null,null,null,null,null,null,null,null,null,null,"22.01.02","LIMP.TERRENO C/DEST.ARV.PERIMETRO<=78CM","m²",0.68,0.5037037037037037,"DER","0,680"]
[null,null,null,null,null,null,null,null,null,null,"22.01.03","LIMP. MANUAL TERRENO AMONT. DE MATERIAL","m²",2.99,2.214814814814815,"DER",2990]
[null,null,null,null,null,null,null,null,null,null,"22.01.04","DERRUBADA E DEST.ARV.C/PERIMETRO>78CM","un",67.65,50.111111111111114,"DER",67650]
[null,null,null,null,null,null,null,null,null,null,"22.01.05","DEST.ARV.COM PERIMETRO MAIOR QUE 78CM","un",22.86,16.933333333333334,"DER",22860]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.01.06","RASPAGEM DO TERRENO","m²",0.63,0.4666666666666666,"DER","0,630"]
[null,null,null,null,null,null,null,null,null,null,"22.02.01","ESCAVACAO E CARGA DE MATERIAL DE 1/2A CATEGORIA","m³",4.9,3.6296296296296298,"DER",4900]
[null,null,null,null,null,null,null,null,null,null,"22.02.02","ESCAV.CARGA MATERIAL DE 2 CAT. C/ RIPPER","m³",5.44,4.029629629629629,"DER",5440]
[null,null,null,null,null,null,null,null,null,null,"22.02.03","ESCAV.CARGA MATERIAL 2 CAT.C/EXPLOSIVO","m³",19.85,14.703703703703704,"DER",19850]
[null,null,null,null,null,null,null,null,null,null,"22.02.04","ESCAVACAO E CARGA MATERIAL  3 CATEGORIA","m³",31.63,23.429629629629627,"DER",31630]
[null,null,null,null,null,null,null,null,null,null,"22.02.05","ESCAV.CARGA SOLO MOLE SOB LAMINA D´AGUA","m³",10.66,7.8962962962962955,"DER",10660]
[null,null,null,null,null,null,null,null,null,null,"22.02.06","CARGA DE MATERIAL LIMPEZA","m³",2.26,1.6740740740740738,"DER",2260]
[null,null,null,null,null,null,null,null,null,null,"22.02.07","ESCAV.,CARGA E DESC.MAT.SIL-ARG.NO CORTE","m³",4.62,3.422222222222222,"DER",4620]
[null,null,null,null,null,null,null,null,null,null,"22.02.08","AQUIS.MAT.ESPAL.CONF.ROLAGEM MAT.SIL.ARG","m³",3.77,2.7925925925925923,"DER",3770]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.02.09","ESPALHAMENTO/REGULARIZACAO/COMPACTACAO DE MATERIAL EM BOTA-FORA.","m³",2.21,1.6370370370370368,"DER",2210]
[null,null,null,null,null,null,null,null,null,null,"22.03.01","TRANSPORTE DE 1/2 CATEGORIA ATE 1 KM","m³*km",3.74,2.77037037037037,"DER",3740]
[null,null,null,null,null,null,null,null,null,null,"22.03.02","TRANSPORTE DE 1/2 CATEGORIA ATE 2 KM","m³*km",2.2,1.6296296296296298,"DER",2200]
[null,null,null,null,null,null,null,null,null,null,"22.03.03","TRANSPORTE DE 1/2 CATEGORIA ATE 5 KM","m³*km",1.71,1.2666666666666666,"DER",1710]
[null,null,null,null,null,null,null,null,null,null,"22.03.04","TRANSPORTE DE 1/2 CATEGORIA ATE 10 KM","m³*km",1.43,1.0592592592592591,"DER",1430]
[null,null,null,null,null,null,null,null,null,null,"22.03.05","TRANSPORTE DE 1/2 CATEGORIA ATE 15 KM","m³*km",1.26,0.9333333333333332,"DER",1260]
[null,null,null,null,null,null,null,null,null,null,"22.03.06","TRANSPORTE DE 1/2 CATEGORIA ALEM DE 15KM","m³*km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,990"]
[null,null,null,null,null,null,null,null,null,null,"22.03.07","TRANSPORTE DE 3 CATEGORIA ATE 1 KM","m³*km",4.84,3.585185185185185,"DER",4840]
[null,null,null,null,null,null,null,null,null,null,"22.03.08","TRANSPORTE DE 3 CATEGORIA ALEM 1 KM","m³*km",3.53,2.6148148148148147,"DER",3530]
[null,null,null,null,null,null,null,null,null,null,"22.03.09","TRANSPORTE DE SOLO MOLE ATE 2 KM","m³*km",3.5,2.5925925925925926,"DER",3500]
[null,null,null,null,null,null,null,null,null,null,"22.03.10","TRANSPORTE DE SOLO MOLE ALEM 2 KM","m³*km",2.41,1.7851851851851852,"DER",2410]
[null,null,null,null,null,null,null,null,null,null,"22.03.11","TRANSPORTE MATERIAL DE LIMPEZA ATE 1 KM","m³*km",4,2.962962962962963,"DER",4000]
[null,null,null,null,null,null,null,null,null,null,"22.03.12","TRANSPORTE MATERIAL DE LIMP.ALEM DE 1 KM","m³*km",2.5,1.8518518518518516,"DER",2500]
[null,null,null,null,null,null,null,null,null,null,"22.04.01","COMPACTACAO DE ATERRO MAIOR/IGUAL 95% PS","m³",3.01,2.2296296296296294,"DER",3010]
[null,null,null,null,null,null,null,null,null,null,"22.04.02","RETALUDAMENTO MANUAL","m³",132.63,98.24444444444444,"DER",132630]
[null,null,null,null,null,null,null,null,null,null,"22.06.01","FunDACAO DE ATERRO C/AREIA LAVADA","m³",131.19,97.17777777777776,"DER",131190]
[null,null,null,null,null,null,null,null,null,null,"22.06.04","FunDACAO DE ATERRO C/PED.RACHAO","m³",101.3,75.03703703703702,"DER",101300]
[null,null,null,null,null,null,null,null,null,null,"22.06.05","ESPALH.ADENS.MATERIAL DE FunD.DE ATERRO","m³",2.21,1.6370370370370368,"DER",2210]
[null,null,null,null,null,null,null,null,null,null,"22.07.01","VALETA DE PROTECAO MANUAL","m",7.1,5.259259259259259,"DER",7100]
[null,null,null,null,null,null,null,null,null,null,"22.08.01","GEOGRELHA POLIETILENO RESIST. TRANSV. 5 KN/M - RESIST. LONGIT. 30 KN/M","m²",19.87,14.718518518518518,"DER",19870]
[null,null,null,null,null,null,null,null,null,null,"22.08.02","GEOGRELHA POLIETILENO RESIST. TRANSV. 5 KN/M - RESIST. LONGIT. 50 KN/M","m²",22.77,16.866666666666664,"DER",22770]
[null,null,null,null,null,null,null,null,null,null,"22.08.03","GEOGRELHA POLIETILENO RESIST. TRANSV. 5 KN/M - RESIST. LONGIT. 80 KN/M","m²",25.69,19.02962962962963,"DER",25690]
[null,null,null,null,null,null,null,null,null,null,"22.08.04","GEOGRELHA POLIETILENO RESIST. TRANSV. 5 KN/M - RESIST. LONGIT. 100 KN/M","m²",28.58,21.170370370370367,"DER",28580]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.05","GEOGRELHA POLIETILENO RESIST. TRANSV. 5 KN/M - RESIST. LONGIT. 150 KN/M","m²",32.94,24.399999999999995,"DER",32940]
[null,null,null,null,null,null,null,null,null,null,"22.08.06","GEOGRELHA POLIETILENO RESIST. TRANSV. 5 KN/M - RESIST. LONGIT. 200 KN/M","m²",36.6,27.11111111111111,"DER",36600]
[null,null,null,null,null,null,null,null,null,null,"22.08.07","GEOGRELHA POLIETILENO RESIST. TRANSV. 15 KN/M - RESIST. LONGIT. 30 KN/M","m²",20.99,15.548148148148146,"DER",20990]
[null,null,null,null,null,null,null,null,null,null,"22.08.08","GEOGRELHA POLIETILENO RESIST. TRANSV. 15 KN/M - RESIST. LONGIT. 50 KN/M","m²",24.07,17.82962962962963,"DER",24070]
[null,null,null,null,null,null,null,null,null,null,"22.08.09","GEOGRELHA POLIETILENO RESIST. TRANSV. 15 KN/M - RESIST. LONGIT. 80","m²",27.12,20.08888888888889,"DER",27120]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.10","GEOGRELHA POLIETILENO RESIST. TRANSV. 15 KN/M - RESIST. LONGIT. 100","m²",30.21,22.377777777777776,"DER",30210]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.11","GEOGRELHA POLIETILENO RESIST. TRANSV. 15 KN/M - RESIST. LONGIT. 150","m²",34.81,25.785185185185185,"DER",34810]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.12","GEOGRELHA POLIETILENO RESIST. TRANSV. 15 KN/M - RESIST. LONGIT. 200","m²",38.65,28.629629629629626,"DER",38650]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.13","GEOGRELHA POLIETILENO RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 30","m²",22.1,16.37037037037037,"DER",22100]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.14","GEOGRELHA POLIETILENO RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 50","m²",25.35,18.77777777777778,"DER",25350]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.15","GEOGRELHA POLIETILENO RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 80","m²",28.58,21.170370370370367,"DER",28580]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.16","GEOGRELHA POLIETILENO RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 100","m²",31.83,23.577777777777776,"DER",31830]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.17","GEOGRELHA POLIETILENO RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 150","m²",36.69,27.177777777777774,"DER",36690]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.18","GEOGRELHA POLIETILENO RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 200","m²",40.78,30.207407407407405,"DER",40780]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.19","GEOGRELHA POLIETILENO RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 30","m²",23.2,17.185185185185183,"DER",23200]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.20","GEOGRELHA POLIETILENO RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 50","m²",26.63,19.725925925925925,"DER",26630]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.21","GEOGRELHA POLIETILENO RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 80","m²",30.02,22.237037037037034,"DER",30020]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.22","GEOGRELHA POLIETILENO RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 100","m²",33.44,24.77037037037037,"DER",33440]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.23","GEOGRELHA POLIETILENO RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 150","m²",38.57,28.57037037037037,"DER",38570]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.24","GEOGRELHA POLIETILENO RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 200","m²",42.83,31.72592592592592,"DER",42830]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.25","GEOGRELHA POLIETILENO RESIST. TRANSV. 50 KN/M - RESIST. LONGIT. 50 KN/M","m²",30.45,22.555555555555554,"DER",30450]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.26","GEOGRELHA POLIETILENO RESIST. TRANSV. 50 KN/M - RESIST. LONGIT. 80 KN/M","m²",34.38,25.46666666666667,"DER",34380]
[null,null,null,null,null,null,null,null,null,null,"22.08.27","GEOGRELHA POLIETILENO RESIST. TRANSV. 50 KN/M - RESIST. LONGIT. 100","m²",38.3,28.370370370370367,"DER",38300]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.28","GEOGRELHA POLIETILENO RESIST. TRANSV. 50 KN/M - RESIST. LONGIT. 150","m²",44.2,32.74074074074074,"DER",44200]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.29","GEOGRELHA POLIETILENO RESIST. TRANSV. 50 KN/M - RESIST. LONGIT. 200","m²",49.15,36.407407407407405,"DER",49150]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.30","GEOGRELHA POLIETILENO RESIST. TRANSV. 100 KN/M - RESIST. LONGIT. 100","m²",65.88,48.79999999999999,"DER",65880]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.31","GEOGRELHA POLIETILENO RESIST. TRANSV. 100 KN/M - RESIST. LONGIT. 150","m²",72.68,53.837037037037035,"DER",72680]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.32","GEOGRELHA POLIETILENO RESIST. TRANSV. 100 KN/M - RESIST. LONGIT. 200","m²",77.81,57.63703703703703,"DER",77810]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.33","GEOGRELHA POLIETILENO RESIST. TRANSV. 150 KN/M - RESIST. LONGIT. 150","m²",76.1,56.37037037037036,"DER",76100]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.34","GEOGRELHA POLIETILENO RESIST. TRANSV. 150 KN/M - RESIST. LONGIT. 200","m²",82.91,61.41481481481481,"DER",82910]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.35","GEOGRELHA POLIETILENO RESIST. TRANSV. 200 KN/M - RESIST. LONGIT. 200","m²",86.34,63.955555555555556,"DER",86340]
[null,null,null,null,null,null,null,null,null,null,null,"KN/M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"22.08.36","GEOGRELHA PVC RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 40 KN/M.","m²",22.1,16.37037037037037,"DER",22100]
[null,null,null,null,null,null,null,null,null,null,"22.08.37","GEOGRELHA PVC RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 60 KN/M.","m²",25.35,18.77777777777778,"DER",25350]
[null,null,null,null,null,null,null,null,null,null,"22.08.38","GEOGRELHA PVC RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 90 KN/M.","m²",28.58,21.170370370370367,"DER",28580]
[null,null,null,null,null,null,null,null,null,null,"22.08.39","GEOGRELHA PVC RESIST. TRANSV. 20 KN/M - RESIST. LONGIT. 120 KN/M.","m²",31.83,23.577777777777776,"DER",31830]
[null,null,null,null,null,null,null,null,null,null,"22.08.40","GEOGRELHA PVC RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 40 KN/M.","m²",23.2,17.185185185185183,"DER",23200]
[null,null,null,null,null,null,null,null,null,null,"22.08.41","GEOGRELHA PVC RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 60 KN/M.","m²",26.63,19.725925925925925,"DER",26630]
[null,null,null,null,null,null,null,null,null,null,"22.08.42","GEOGRELHA PVC RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 90 KN/M.","m²",30.02,22.237037037037034,"DER",30020]
[null,null,null,null,null,null,null,null,null,null,"22.08.43","GEOGRELHA PVC RESIST. TRANSV. 30 KN/M - RESIST. LONGIT. 120 KN/M.","m²",33.44,24.77037037037037,"DER",33440]
[null,null,null,null,null,null,null,null,null,null,"23.02.01","MELH/PREPARO SUB-LEITO - 100% EN","m²",1.14,0.8444444444444443,"DER",1140]
[null,null,null,null,null,null,null,null,null,null,"23.02.02","MELH/PREPARO SUB-LEITO - 100% EI","m²",1.36,1.0074074074074073,"DER",1360]
[null,null,null,null,null,null,null,null,null,null,"23.03.01","REFORCO SUB-LEITO ESCAV. SOLO ESCOLHIDO","m³",4.79,3.548148148148148,"DER",4790]
[null,null,null,null,null,null,null,null,null,null,"23.03.02.01","REFORCO DO SUB-LEITO - TRANSPORTE ATE 1 KM","m³*km",3.91,2.8962962962962964,"DER",3910]
[null,null,null,null,null,null,null,null,null,null,"23.03.02.02","REFORCO DO SUB-LEITO - TRANSPORTE ATE 2 KM","m³*km",2.74,2.0296296296296297,"DER",2740]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.03.02.03","REFORCO DO SUB-LEITO - TRANSPORTE ATE 5KM","m³*km",2.14,1.5851851851851853,"DER",2140]
[null,null,null,null,null,null,null,null,null,null,"23.03.02.04","REFORCO DE SUB-LEITO - TRANSPORTE ATE 10 KM","m³*km",1.79,1.325925925925926,"DER",1790]
[null,null,null,null,null,null,null,null,null,null,"23.03.02.05","REFORCO DO SUB-LEITO - TRANSPORTE ATE 15 KM","m³*km",1.58,1.1703703703703703,"DER",1580]
[null,null,null,null,null,null,null,null,null,null,"23.03.02.06","REFORCO DOE SUB-LEITO - TRANSPORTE + 15KM","m³*km",1.24,0.9185185185185184,"DER",1240]
[null,null,null,null,null,null,null,null,null,null,"23.03.03","REFORCO DE SUB-LEITO COMPACTACAO 100% EI","m³",4.1,3.0370370370370368,"DER",4100]
[null,null,null,null,null,null,null,null,null,null,"23.03.04","REFORCO DE SUB-LEITO COMPACT 100% EN","m³",3.69,2.733333333333333,"DER",3690]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.01","SUB-BASE OU BASE SOLO CIM 3% - USINA","m³",56.64,41.955555555555556,"DER",56640]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.02","SUB-BASE OU BASE SOLO CIM 4% - USINA","m³",69.18,51.24444444444445,"DER",69180]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.03","SUB-BASE OU BASE SOLO CIM 5% - USINA","m³",81.72,60.53333333333333,"DER",81720]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.04","SUB-BASE OU BASE SOLO CIM 6% - USINA","m³",94.26,69.82222222222222,"DER",94260]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.05","SUB-BASE OU BASE SOLO CIM 7% - USINA","m³",106.81,79.11851851851851,"DER",106810]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.06","SUB-BASE OU BASE SOLO CIM 8% - USINA","m³",119.35,88.40740740740739,"DER",119350]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.07","SUB-BASE OU BASE SOLO CIM 9% - USINA","m³",131.89,97.69629629629628,"DER",131890]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.08","SUB-BASE OU BASE SOLO CIM 10% - USINA","m³",144.43,106.98518518518519,"DER",144430]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.09","SUB-BASE OU BASE SOLO CIM 11% - USINA","m³",156.97,116.27407407407406,"DER",156970]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.10","SUB-BASE OU BASE SOLO CIM 12% - USINA","m³",169.52,125.57037037037037,"DER",169520]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.11","SUB-BASE OU BASE SOLO CIM 3% - PULVEMISTURADOR","m³",47.85,35.44444444444444,"DER",47850]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.12","SUB-BASE OU BASE SOLO CIM 4% - PULVEMISTURADOR","m³",60.39,44.733333333333334,"DER",60390]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.13","SUB-BASE OU BASE SOLO CIM 5% - PULVEMISTURADOR","m³",72.94,54.029629629629625,"DER",72940]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.14","SUB-BASE OU BASE SOLO CIM 6% - PULVEMISTURADOR","m³",85.48,63.318518518518516,"DER",85480]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.15","SUB-BASE OU BASE SOLO CIM 7% - PULVEMISTURADOR","m³",91.1,67.48148148148147,"DER",91100]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.16","SUB-BASE OU BASE SOLO CIM 8% - PULVEMISTURADOR","m³",98.09,72.65925925925926,"DER",98090]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.17","SUB-BASE OU BASE SOLO CIM 9% - PULVEMISTURADOR","m³",108.97,80.71851851851851,"DER",108970]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.18","SUB-BASE OU BASE SOLO CIM 10% - PULVEMISTURADOR","m³",120.95,89.5925925925926,"DER",120950]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.19","SUB-BASE OU BASE SOLO CIM 11% - PULV.","m³",131.65,97.51851851851852,"DER",131650]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.20","SUB-BASE OU BASE SOLO CIM 12% - PULVEMISTURADOR","m³",143.28,106.13333333333333,"DER",143280]
[null,null,null,null,null,null,null,null,null,null,"23.04.01.26","SUB-BASE OU BASE DE SOLO-CAL 4% - PULVEMISTURADOR","m³",53.72,39.79259259259259,"DER",53720]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.01","SUB-BASE OU BASE SOLO BRITA C/ CIM.3%","m³",142.23,105.35555555555554,"DER",142230]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.02","SUB-BASE OU BASE SOLO BRITA C/ CIM.4%","m³",159.97,118.4962962962963,"DER",159970]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.03","SUB-BASE OU BASE SOLO BRITA C/ CIM.5%","m³",170.43,126.24444444444444,"DER",170430]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.04","SUB-BASE OU BASE SOLO BRITA C/ CIM.6%","m³",180.89,133.9925925925926,"DER",180890]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.05","SUB-BASE OU BASE DE SOLO BRITA 50% BRITA","m³",88.29,65.4,"DER",88290]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.05.01","SUB-BASE OU BASE DE SOLO LATERITICO-BRITA 50% BRITA","m³",88.29,65.4,"DER",88290]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.07","SUB-BASE OU BASE DE SOLO BRITA 60% BRITA","m³",90.44,66.99259259259259,"DER",90440]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.09","SUB-BASE OU BASE DE SOLO BRITA 70% BRITA","m³",117.78,87.24444444444444,"DER",117780]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.11","SUB-BASE OU BASE DE SOLO BRITA 80% BRITA","m³",132.52,98.16296296296296,"DER",132520]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.04.02.13","SUB-BASE OU BASE SE SOLO BRITA 90% BRITA","m³",145.77,107.97777777777777,"DER",145770]
[null,null,null,null,null,null,null,null,null,null,"23.04.03.01","SUB-BASE OU BASE BRITA GRAD. SIMPLES","m³",168.38,124.72592592592592,"DER",168380]
[null,null,null,null,null,null,null,null,null,null,"23.04.03.02","SUB-BASE OU BASE DE PEDRA BRITADA","m³",130.4,96.5925925925926,"DER",130400]
[null,null,null,null,null,null,null,null,null,null,"23.04.03.03","SUB-BASE OU BASE DE BICA CORRIDA","m³",147.81,109.48888888888888,"DER",147810]
[null,null,null,null,null,null,null,null,null,null,"23.04.03.04","SUB-BASE OU BASE DE PEDRA RACHAO, CONF. ET-POO/042 (DERSA)","m³",168.04,124.47407407407405,"DER",168040]
[null,null,null,null,null,null,null,null,null,null,"23.04.04.01","SUB-BASE OU BASE BRITA GRAD. C/CIM 1%VOL","m³",168.82,125.05185185185184,"DER",168820]
[null,null,null,null,null,null,null,null,null,null,"23.04.04.02","SUB-BASE OU BASE BRITA GRA. C/CIM 2%VOL","m³",181.93,134.76296296296297,"DER",181930]
[null,null,null,null,null,null,null,null,null,null,"23.04.04.03","SUB-BASE OU BASE BRITA GRAD. C/CIM 3%VOL","m³",195.04,144.47407407407405,"DER",195040]
[null,null,null,null,null,null,null,null,null,null,"23.04.04.04","SUB-BASE OU BASE BRITA GRAD. C/CIM 4%VOL","m³",208.16,154.19259259259258,"DER",208160]
[null,null,null,null,null,null,null,null,null,null,"23.04.04.05","SUB-BASE OU BASE BRITA GRAD. C/CIM 5%","m³",232.27,172.05185185185184,"DER",232270]
[null,null,null,null,null,null,null,null,null,null,"23.04.05.01","SUB-BASE OU BASE ESTABILIZADA GRANULOMETRICAMENTE","m³",128.41,95.11851851851851,"DER",128410]
[null,null,null,null,null,null,null,null,null,null,"23.04.06.01","SUB-BASE OU BASE MACADAME HIDRAULICO","m³",156.63,116.02222222222221,"DER",156630]
[null,null,null,null,null,null,null,null,null,null,"23.04.06.02","SUB-BASE OU BASE MACADAME BETUMINOSO","m³",393.92,291.7925925925926,"DER",393920]
[null,null,null,null,null,null,null,null,null,null,"23.04.06.03","SUB-BASE OU BASE DE MACADAME SECO","m³",161.13,119.35555555555554,"DER",161130]
[null,null,null,null,null,null,null,null,null,null,"23.04.07.01","SUB-BASE OU BASE SOLO AREN. FINO 95% PI","m³",19.06,14.118518518518517,"DER",19060]
[null,null,null,null,null,null,null,null,null,null,"23.04.07.03","BASE SOLO ESTABILIZADO QUIMICAMENTE PARA SOLO ARENOSO","m³",43.93,32.54074074074074,"DER",43930]
[null,null,null,null,null,null,null,null,null,null,"23.05.01","IMPRIMADURA BETUMINOSA IMPERMEABILIZANTE","m²",3.42,2.533333333333333,"DER",3420]
[null,null,null,null,null,null,null,null,null,null,"23.05.01.01","IMPRIMADURA BETUMINOSA IMPERMEABILIZANTE (SEM MATERIAIS","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,210"]
[null,null,null,null,null,null,null,null,null,null,null,"ASFALTICOS)",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.05.02","IMPRIMADURA BETUMINOSA LIGANTE","m²",1.32,0.9777777777777777,"DER",1320]
[null,null,null,null,null,null,null,null,null,null,"23.05.02.01","IMPRIMADURABETUMINOSA LIGANTE (SEM MATERIAIS ASFALTICOS)","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,150"]
[null,null,null,null,null,null,null,null,null,null,"23.05.03","IMPRIMADURA BET. AUXILIAR DE LIGACAO","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,730"]
[null,null,null,null,null,null,null,null,null,null,"23.05.04","IMPRIM. BET. LIGANTE MODIF. POLIMERO","m²",1.71,1.2666666666666666,"DER",1710]
[null,null,null,null,null,null,null,null,null,null,"23.06.01","TRATAMENTO SUPERFICIAL SIMPLES","m²",3.6,2.6666666666666665,"DER",3600]
[null,null,null,null,null,null,null,null,null,null,"23.06.02","TRATAMENTO SUPERFICIAL DUPLO","m³",330.83,245.05925925925922,"DER",330830]
[null,null,null,null,null,null,null,null,null,null,"23.06.03","TRATAMENTO SUPERFICIAL TRIPLO","m³",412.88,305.837037037037,"DER",412880]
[null,null,null,null,null,null,null,null,null,null,"23.06.04","MICROPAVIMENTO C/POLIMERO COM FIBRA","m²",10.57,7.829629629629629,"DER",10570]
[null,null,null,null,null,null,null,null,null,null,"23.06.04.01","MICROPAVIMENTO COM POLIMERO SEM FIBRA","m²",10.01,7.4148148148148145,"DER",10010]
[null,null,null,null,null,null,null,null,null,null,"23.06.05","TRATAMENTO SUPERF. C/ LAMA ASFALTICA","m²",4.52,3.3481481481481477,"DER",4520]
[null,null,null,null,null,null,null,null,null,null,"23.06.06","TRAT.SUP.CAM. LAMA ASFALTICA GROSSA","m²",5.8,4.296296296296296,"DER",5800]
[null,null,null,null,null,null,null,null,null,null,"23.06.07","TRATAMENTO SUPERFICIAL SIMPLES MODIFICADO POR POLIMEROS","m²",4.48,3.3185185185185184,"DER",4480]
[null,null,null,null,null,null,null,null,null,null,"23.06.08","TRATAMENTO SUPERFICIAL DUPLO MODIFICADO POR POLIMEROS","m³",460.05,340.77777777777777,"DER",460050]
[null,null,null,null,null,null,null,null,null,null,"23.06.09","TRATAMENTO SUPERFICIAL TRIPLO MODIFICADO POR POLIMEROS","m³",531.57,393.7555555555556,"DER",531570]
[null,null,null,null,null,null,null,null,null,null,"23.07.01","PRE-MISTURADO A FRIO","m³",442.63,327.87407407407403,"DER",442630]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.07.01.01","CAMADA BASE PRE-MISTURADO A FRIO (SEM MATERIAIS ASFALTICOS)","m³",200.71,148.67407407407407,"DER",200710]
[null,null,null,null,null,null,null,null,null,null,"23.07.01.02","APLICACAO CAMADA DE PRE-MISTURADO A FRIO COM TRANSPORTE (EXCLUSO","m³",74.05,54.85185185185185,"DER",74050]
[null,null,null,null,null,null,null,null,null,null,null,"MATERIAL)",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.08.01","CONC.ASF.US.QUENTE - BINDER GRAD.A C/DOP","m³",473.18,350.5037037037037,"DER",473180]
[null,null,null,null,null,null,null,null,null,null,null,"CONC.ASF.US.QUENTE - BINDER GRAD.A S/DOP","m³",454.57,336.71851851851847,"DER",454570]
[null,null,null,null,null,null,null,null,null,null,"23.08.02","CONC.ASF.US.QUENTE - BINDER GRAD.B C/DOP","m³",488.89,362.1407407407407,"DER",488890]
[null,null,null,null,null,null,null,null,null,null,"23.08.02.01","CONC.ASF.US.QUENTE - BINDER GRAD.B S/DOP","m³",467.25,346.1111111111111,"DER",467250]
[null,null,null,null,null,null,null,null,null,null,"23.08.02.02","CONCRETO ASFALTICO GRADUACAO I","m³",563.58,417.4666666666667,"DER",563580]
[null,null,null,null,null,null,null,null,null,null,"23.08.03.01","CAMADA ROLAMENTO-CBUQ GRADUACAO C-S/DOP","m³",503.26,372.7851851851851,"DER",503260]
[null,null,null,null,null,null,null,null,null,null,"23.08.03.03","CAMADA ROLAMENTO - CBUQ - GRAD.C - COM DOP","m³",526.62,390.08888888888885,"DER",526620]
[null,null,null,null,null,null,null,null,null,null,"23.08.04.02","CAMADA DE ROLAMENTO - CBUQ - GRAD. D - SEM DOP","m³",485.79,359.84444444444443,"DER",485790]
[null,null,null,null,null,null,null,null,null,null,"23.08.04.03","CAMADA ROLANTE CBUQ - GRAD. D - COM DOP","m³",510.88,378.4296296296296,"DER",510880]
[null,null,null,null,null,null,null,null,null,null,"23.08.04.04","CAMADA DE ROLAMENTO CBUQ - GRADUACAO D, MODIFICADA POR POLIMERO","m³",627.7,464.962962962963,"DER",627700]
[null,null,null,null,null,null,null,null,null,null,"23.08.05","CONC. ASF. MODIFICADO P/POLIMERO","m³",637.36,472.1185185185185,"DER",637360]
[null,null,null,null,null,null,null,null,null,null,"23.08.05.01.01","CONCRETO ASFALTICO MODIFICADO POR POLIMERO - GRAD. II","m³",572.96,424.4148148148148,"DER",572960]
[null,null,null,null,null,null,null,null,null,null,"23.08.06","CONCRETO ASFALTICO MODIFICADO COM 15% EM PESO DE BORRACHA","m³",618.62,458.237037037037,"DER",618620]
[null,null,null,null,null,null,null,null,null,null,null,"(CONTINUO)",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.08.06.04","CONCRETO ASFALTICO COM ASFALTO-BORRACHA, GRADUACAO IV","m³",607.87,450.27407407407406,"DER",607870]
[null,null,null,null,null,null,null,null,null,null,"23.08.06.05","CONCRETO ASFALTO BORRACHA MORNO COM 15% DE BORRACHA.","m³",636.82,471.7185185185185,"DER",636820]
[null,null,null,null,null,null,null,null,null,null,"23.08.06.06","CONCRETO ASFALTO BORRACHA GRAD. IV, MORNO COM 15% BORRACHA","m³",627.11,464.5259259259259,"DER",627110]
[null,null,null,null,null,null,null,null,null,null,"23.09.01","CAPA SELANTE TIPO 2","m²",2.51,1.859259259259259,"DER",2510]
[null,null,null,null,null,null,null,null,null,null,"23.09.02","CAPA SELANTE TIPO 3","m²",4.11,3.0444444444444443,"DER",4110]
[null,null,null,null,null,null,null,null,null,null,"23.10.01","FRESAGEM CONTINUA DE PAV., INDEPENDENTE DA ESPESSURA","m³",139.28,103.17037037037036,"DER",139280]
[null,null,null,null,null,null,null,null,null,null,"23.11.04.01","PAVIMENTO DE CONCRETO - APLICACAO COM FORMAS DESLIZANTES","m³",575.07,425.97777777777776,"DER",575070]
[null,null,null,null,null,null,null,null,null,null,"23.11.09","PAVIMENTO DE CONCRETO SOBRE OBRA DE ARTE ESPECIAL-MANUAL.","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.039,180"]
[null,null,null,null,null,null,null,null,null,null,null,"PAVIMENTO DE CONCRETO SOBRE OBRA DE ARTE ESPECIAL-MECANICO(PP-DE-",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.11.10","P00/010)","m³",749.33,555.0592592592593,"DER",749330]
[null,null,null,null,null,null,null,null,null,null,"23.11.11","PAVIMENTO DE CONCRETO POBRE PARA BASE DE PAVIMENTO RIGIDO.","m³",229.86,170.26666666666665,"DER",229860]
[null,null,null,null,null,null,null,null,null,null,"23.12.01","PAVIMENTO CONCRETO INTERTRAVADO - E=6CM","m²",75.25,55.74074074074074,"DER",75250]
[null,null,null,null,null,null,null,null,null,null,"23.12.02","PAVIMENTO CONCRETO INTERTRAVADO - E=8CM","m²",86.81,64.3037037037037,"DER",86810]
[null,null,null,null,null,null,null,null,null,null,"23.12.03","PAV CONCRETO INTERTRAVADO - E=10CM","m²",91.94,68.1037037037037,"DER",91940]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"23.13.07.01","RECICLAGEM CAPA/BASE COM ADICAO DE 4% DE CIMENTO","m³",113.92,84.38518518518518,"DER",113920]
[null,null,null,null,null,null,null,null,null,null,"23.13.07.02","RECICLAGEM DE PAVIMENTO COM ADICAO DE 30% DE BRITA E 4% DE CIMENTO","m³",157.32,116.53333333333332,"DER",157320]
[null,null,null,null,null,null,null,null,null,null,"23.13.07.03","RECICLAGEM DE PAVIMENTO COM ADICAO DE 20% DE BRITA E 4% DE CIMENTO","m³",144.19,106.8074074074074,"DER",144190]
[null,null,null,null,null,null,null,null,null,null,"23.13.07.04","RECICLAGEM DE PAVIMENTO COM ADICAO DE 20% DE BRITA E 6% DE CIMENTO","m³",172.2,127.55555555555554,"DER",172200]
[null,null,null,null,null,null,null,null,null,null,"23.13.07.05","RECICLAGEM DE PAVIMENTO COM ADICAO DE 20% BRITA.","m³",88.18,65.31851851851852,"DER",88180]
[null,null,null,null,null,null,null,null,null,null,"24.01.01","ATERRO DE ACESSO","m³",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"24.02.01","ESCAVACAO MANUAL PARA OBRAS S/ EXPLOSIVO","m³",50.17,37.162962962962965,"DER",50170]
[null,null,null,null,null,null,null,null,null,null,"24.02.02","ESCAVACAO MECANICA P/ OBRAS S/EXPLOSIVO","m³",10.92,8.088888888888889,"DER",10920]
[null,null,null,null,null,null,null,null,null,null,"24.02.03","ESCAVACAO MECANICA P/ OBRAS C/EXPLOSIVO","m³",43.09,31.918518518518518,"DER",43090]
[null,null,null,null,null,null,null,null,null,null,"24.02.04","CORTA-RIO ESCAVACAO SEM EXPLOSIVO","m³",10.92,8.088888888888889,"DER",10920]
[null,null,null,null,null,null,null,null,null,null,"24.02.05","CORTA-RIO ESCAVACAO COM EXPLOSIVO","m³",43.09,31.918518518518518,"DER",43090]
[null,null,null,null,null,null,null,null,null,null,"24.02.08","ESCAV.FUND.BUEIRO OU DRENO S/EXPL.ATE 2M","m³",62.83,46.54074074074074,"DER",62830]
[null,null,null,null,null,null,null,null,null,null,"24.02.09","ACRESC.P/ESCAV.1,5M PROFunDIDADE,ALEM 2M","m³",13.05,9.666666666666666,"DER",13050]
[null,null,null,null,null,null,null,null,null,null,"24.02.10","ESCAV.FunD.BUEIRO OU DRENO C/EXPL.ATE 2M","m³",199.61,147.85925925925926,"DER",199610]
[null,null,null,null,null,null,null,null,null,null,"24.02.11","ACRESC.ESC.ENS.EXPL.C/1,5M PROF.ALEM 2M","m³",18.94,14.02962962962963,"DER",18940]
[null,null,null,null,null,null,null,null,null,null,"24.02.12","ESCAV.FunD.DENTRO ENSEC.SEM EXPL. ATE 3M","m³",53.8,39.85185185185185,"DER",53800]
[null,null,null,null,null,null,null,null,null,null,"24.02.13","ACR.P/ESCAV.ENSEC.P/CADA 1M  PROF.ALEm³M","m³",10.78,7.985185185185184,"DER",10780]
[null,null,null,null,null,null,null,null,null,null,"24.02.14","ESCAV.FunD.DENTRO ENSEC.C/EXPL.ATE 3M","m³",166.18,123.09629629629629,"DER",166180]
[null,null,null,null,null,null,null,null,null,null,"24.02.15","ACRESC.P/ESC.ENSEC.C/EXPL.C/1,5M ALEM 3M","m³",18.94,14.02962962962963,"DER",18940]
[null,null,null,null,null,null,null,null,null,null,"24.03.01","PAREDE ENSECADEIRA COM PRANCHA-ESP.0,05M","m²",199.49,147.77037037037036,"DER",199490]
[null,null,null,null,null,null,null,null,null,null,"24.03.02","PAREDE ENSECADEIRA C/PRANCHA-ESP.0,075M","m²",280.41,207.7111111111111,"DER",280410]
[null,null,null,null,null,null,null,null,null,null,"24.03.03","PAREDE ENSECADEIRA COM PERFIL METALICO","m²",388.21,287.56296296296296,"DER",388210]
[null,null,null,null,null,null,null,null,null,null,"24.03.04","ARGILA ENCH.ENSECADEIRA,INCL.APILOAMENTO","m³",51.11,37.859259259259254,"DER",51110]
[null,null,null,null,null,null,null,null,null,null,"24.03.05","ESGOTAMENTO CONTINUO AGUA","m³",2.02,1.4962962962962962,"DER",2020]
[null,null,null,null,null,null,null,null,null,null,"24.03.06","ESCORAMENTO DE VALAS/CAVAS P/FunD.CONT.","m²",96,71.1111111111111,"DER",96000]
[null,null,null,null,null,null,null,null,null,null,"24.03.07","ESCORAMENTO DE VALAS/CAVAS P/FUND.DESC.","m²",64.68,47.91111111111111,"DER",64680]
[null,null,null,null,null,null,null,null,null,null,"24.03.08","ESCORAMENTO PARA FORMAS","m²",35.8,26.518518518518515,"DER",35800]
[null,null,null,null,null,null,null,null,null,null,"24.04.01","CIMB.DE PASSAGEM SECunD. E GALERIA RET.","m³",34.78,25.762962962962963,"DER",34780]
[null,null,null,null,null,null,null,null,null,null,"24.04.02","CIMBRAMENTO DE GALERIA EM ABOBODA","m³",49.59,36.733333333333334,"DER",49590]
[null,null,null,null,null,null,null,null,null,null,"24.04.03","ANDAIME DE MADEIRA","m³",12.63,9.355555555555556,"DER",12630]
[null,null,null,null,null,null,null,null,null,null,"24.04.04","ANDAIME TUBULAR","m³",18.12,13.422222222222222,"DER",18120]
[null,null,null,null,null,null,null,null,null,null,"24.05.01","FORMA PLANA PARA CONCRETO COMUM","m²",80.07,59.3111111111111,"DER",80070]
[null,null,null,null,null,null,null,null,null,null,"24.05.02","FORMA PLANA PARA CONCRETO APARENTE","m²",90.3,66.88888888888889,"DER",90300]
[null,null,null,null,null,null,null,null,null,null,"24.06.01","BARRA DE ACO CA-25","kg",8.78,6.503703703703703,"DER",8780]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.06.02","BARRA DE ACO CA-50","kg",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"24.06.03","BARRA DE ACO CA-60","kg",9.2,6.814814814814814,"DER",9200]
[null,null,null,null,null,null,null,null,null,null,"24.06.04","TELA METALICA","kg",7.38,5.466666666666666,"DER",7380]
[null,null,null,null,null,null,null,null,null,null,"24.07.01","CONCRETO FCK 10 MPA","m³",386.3,286.14814814814815,"DER",386300]
[null,null,null,null,null,null,null,null,null,null,"24.07.02","CONCRETO FCK 15 MPA","m³",426.19,315.6962962962963,"DER",426190]
[null,null,null,null,null,null,null,null,null,null,"24.07.03","CONCRETO FCK 18 MPA","m³",435.69,322.7333333333333,"DER",435690]
[null,null,null,null,null,null,null,null,null,null,"24.07.04","CONCRETO FCK 20 MPA","m³",455.28,337.2444444444444,"DER",455280]
[null,null,null,null,null,null,null,null,null,null,"24.07.05","CONCRETO FCK 25 MPA","m³",467.63,346.39259259259256,"DER",467630]
[null,null,null,null,null,null,null,null,null,null,"24.07.07","CONCRETO FCK 30 MPA","m³",483.41,358.0814814814815,"DER",483410]
[null,null,null,null,null,null,null,null,null,null,"24.07.08","CONCRETO CICLOPICO","m³",390.4,289.18518518518516,"DER",390400]
[null,null,null,null,null,null,null,null,null,null,"24.07.09","BOMBEAMENTO P/ CONCRETO QUALQUER RESIST.","m³",42.12,31.199999999999996,"DER",42120]
[null,null,null,null,null,null,null,null,null,null,"24.07.12","CONCRETO FCK 35 MPA","m³",493.31,365.4148148148148,"DER",493310]
[null,null,null,null,null,null,null,null,null,null,"24.07.13","CONCRETO FCK 40 MPA","m³",522.21,386.82222222222225,"DER",522210]
[null,null,null,null,null,null,null,null,null,null,"24.07.14","CONCRETO FCK 45 MPA","m³",590.18,437.1703703703703,"DER",590180]
[null,null,null,null,null,null,null,null,null,null,"24.07.15","CONCRETO FCK 50 MPA","m³",609.64,451.58518518518514,"DER",609640]
[null,null,null,null,null,null,null,null,null,null,"24.08.01","JunTA ELASTICA EM PVC TIPO O-12","m",68.94,51.06666666666666,"DER",68940]
[null,null,null,null,null,null,null,null,null,null,"24.08.02","JunTA ELASTICA EM PVC TIPO O-22","m",82.51,61.11851851851852,"DER",82510]
[null,null,null,null,null,null,null,null,null,null,"24.09.01","ENROCAMENTO PEDRA ARRUMADA","m³",210.83,156.17037037037036,"DER",210830]
[null,null,null,null,null,null,null,null,null,null,"24.09.02","ENROCAMENTO PEDRA ARRUMADA E REJunTADA","m³",324.57,240.4222222222222,"DER",324570]
[null,null,null,null,null,null,null,null,null,null,"24.09.03","ENROCAMENTO PEDRA JOGADA","m³",136.02,100.75555555555556,"DER",136020]
[null,null,null,null,null,null,null,null,null,null,"24.09.04","GABIAO TIPO CAIXA LARGURA 50CM - TELA GALVANIZADA","m³",382.7,283.48148148148147,"DER",382700]
[null,null,null,null,null,null,null,null,null,null,"24.09.04.01","GABIAO TIPO CAIXA ALTURA DE 50 CM - REVSTIDO DE PVC","m³",441.23,326.837037037037,"DER",441230]
[null,null,null,null,null,null,null,null,null,null,"24.09.04.02","GABIAO TIPO CAIXA REVESTIDO DE PVC ALTURA DE 1,00M","m³",422.7,313.1111111111111,"DER",422700]
[null,null,null,null,null,null,null,null,null,null,"24.09.04.03","GABIAO TIPO CAIXA GALVANIZADO ALTURA DE 1,00M","m³",324.8,240.59259259259258,"DER",324800]
[null,null,null,null,null,null,null,null,null,null,"24.09.05.01","GABIAO TIPO COLCHAO ESPES.17CM-TELA GALV","m²",104.78,77.6148148148148,"DER",104780]
[null,null,null,null,null,null,null,null,null,null,"24.09.06.01","GABIAO TIPO COLCHAO ESPESSURA 23CM - TELA GALVANIZADA","m²",120.62,89.34814814814814,"DER",120620]
[null,null,null,null,null,null,null,null,null,null,"24.09.07.01","GABIAO TIPO COLCHAO ESPES.30CM-TELA GALV","m²",137.11,101.56296296296297,"DER",137110]
[null,null,null,null,null,null,null,null,null,null,"24.09.08.01","GABIAO TIPO COLCHAO ESPES.17CM-TELA PVC","m²",120.18,89.02222222222223,"DER",120180]
[null,null,null,null,null,null,null,null,null,null,"24.09.09.01","GABIAO TIPO COLCHAO ESPESSURA 23CM - TELA PVC","m²",134.85,99.88888888888887,"DER",134850]
[null,null,null,null,null,null,null,null,null,null,"24.09.10.01","GABIAO TIPO COLCHAO ESPESSURA 30CM - TELA PVC","m²",152.78,113.17037037037036,"DER",152780]
[null,null,null,null,null,null,null,null,null,null,"24.09.11","GABIAO TIPO SACO-TELA GALV.","m³",345.79,256.14074074074074,"DER",345790]
[null,null,null,null,null,null,null,null,null,null,"24.09.12","GABIAO TIPO SACO - TELA GALVANIZADA REVESTIDA DE PVC","m³",361.85,268.037037037037,"DER",361850]
[null,null,null,null,null,null,null,null,null,null,"24.09.13","CAMADA FILTRANTE PEDRA BRITADA","m³",120.15,89,"DER",120150]
[null,null,null,null,null,null,null,null,null,null,"24.10.02","CALCAMENTO CONCRETO FCK 15 MPA","m³",610.14,451.9555555555555,"DER",610140]
[null,null,null,null,null,null,null,null,null,null,"24.10.03","CALCAMENTO CONCRETO FCK 10 MPA","m³",568.25,420.9259259259259,"DER",568250]
[null,null,null,null,null,null,null,null,null,null,"24.11.01","ALVENARIA TIJOLO","m³",797.65,590.8518518518518,"DER",797650]
[null,null,null,null,null,null,null,null,null,null,"24.11.02","ALVENARIA DE PEDRA SECA","m³",304.1,225.25925925925927,"DER",304100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.11.04","ALVENARIA DE PEDRA ARGAMASSADA","m³",539.1,399.3333333333333,"DER",539100]
[null,null,null,null,null,null,null,null,null,null,"24.11.05","ALVENARIA DE BLOCO DE CONCRETO","m³",460.87,341.38518518518515,"DER",460870]
[null,null,null,null,null,null,null,null,null,null,"24.11.07","ARGAM.DE CIMENTO E AREIA TRACO 1:3 E=2CM","m²",34.41,25.488888888888884,"DER",34410]
[null,null,null,null,null,null,null,null,null,null,"24.12.01.01","ENCHIMENTO DE VALA COM PEDRA BRITADA 1E2","m³",98.43,72.91111111111111,"DER",98430]
[null,null,null,null,null,null,null,null,null,null,"24.12.01.02","ENCHIMENTO DE VALA COM PEDRA BRITADA 3E4","m³",105.19,77.91851851851851,"DER",105190]
[null,null,null,null,null,null,null,null,null,null,"24.12.01.03","ENCHIMENTO DE VALA COM BICA CORRIDA","m³",106.34,78.77037037037037,"DER",106340]
[null,null,null,null,null,null,null,null,null,null,"24.12.02","ENCHIMENTO DE VALA COM AREIA","m³",131.19,97.17777777777776,"DER",131190]
[null,null,null,null,null,null,null,null,null,null,"24.12.03","ENCHIMENTO DE VALA COM PEDRA MARROADA","m³",91.7,67.92592592592592,"DER",91700]
[null,null,null,null,null,null,null,null,null,null,"24.12.05","ENCHIMENTO BASE TUBO COM PEDRA BRITADA","m³",130.32,96.53333333333332,"DER",130320]
[null,null,null,null,null,null,null,null,null,null,"24.12.08","COMPACTACAO MANUAL C/REATERRO SOLO LOCAL","m³",24.16,17.896296296296295,"DER",24160]
[null,null,null,null,null,null,null,null,null,null,"24.12.09","COMPACTACAO MANUAL PARA BASES DE CAIXAS E VALAS","m²",12.08,8.948148148148148,"DER",12080]
[null,null,null,null,null,null,null,null,null,null,"24.13.01","VALETA SECAO TRANSV.ATE 0,50m² 1 CAT.","m³",55.57,41.16296296296296,"DER",55570]
[null,null,null,null,null,null,null,null,null,null,"24.13.02","VALETA SECAO TRANSV.ATE 0,50m² 2 CAT.","m³",82.21,60.896296296296285,"DER",82210]
[null,null,null,null,null,null,null,null,null,null,"24.13.03","VALETA SECAO TRANSV.ATE 0,50m² 3 CAT.","m³",170.2,126.07407407407406,"DER",170200]
[null,null,null,null,null,null,null,null,null,null,"24.13.04","VALETA SECAO TRANSV.MAIOR 0,50m² 1 CAT.","m³",16.44,12.177777777777777,"DER",16440]
[null,null,null,null,null,null,null,null,null,null,"24.13.05","VALETA SECAO TRANSV.MAIOR 0,50m² 2 CAT.","m³",21.93,16.244444444444444,"DER",21930]
[null,null,null,null,null,null,null,null,null,null,"24.13.06","VALETA SECAO TRANSV.MAIOR 0,50m² 3 CAT - COM EXPLOSIVOS","m³",114.58,84.87407407407407,"DER",114580]
[null,null,null,null,null,null,null,null,null,null,"24.13.07","VALETA SECAO TRANSV.MAIOR 0.50m² - SEM EXPLOSIVO","m³",90.94,67.36296296296295,"DER",90940]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.01","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 07 KN/M","m²",4.67,3.459259259259259,"DER",4670]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.02","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 08 KN/M","m²",5.02,3.718518518518518,"DER",5020]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.03","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 09 KN/M","m²",5.79,4.288888888888889,"DER",5790]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.04","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 10 KN/M","m²",6.34,4.696296296296296,"DER",6340]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.05","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 14 KN/M","m²",7.68,5.688888888888888,"DER",7680]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.06","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 16 KN/M","m²",9,6.666666666666666,"DER",9000]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.07","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 21 KN/M","m²",11.66,8.637037037037036,"DER",11660]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.08","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 26 KN/M","m²",14.31,10.6,"DER",14310]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.09","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 31 KN/M","m²",16.95,12.555555555555554,"DER",16950]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.10","MANTA GEOTEXTIL TECIDA RESIST. LONGIT. 24 KN/M","m²",6.53,4.837037037037037,"DER",6530]
[null,null,null,null,null,null,null,null,null,null,"24.14.01.11","MANTA GEOTEXTIL TECIDA RESISTENCIA LOGINTUDINAL 48 KN/M","m²",10.19,7.548148148148147,"DER",10190]
[null,null,null,null,null,null,null,null,null,null,"24.14.02","MANTA GEOTEXTIL TECIDA","kg",35.21,26.08148148148148,"DER",35210]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.15.01","TUBO DRENO CONCRETO 15CM","m",50.1,37.11111111111111,"DER",50100]
[null,null,null,null,null,null,null,null,null,null,"24.15.02","TUBO DRENO CONCRETO 20CM","m",59.35,43.96296296296296,"DER",59350]
[null,null,null,null,null,null,null,null,null,null,"24.15.03","TUBO DRENO BARRO 15CM","m",45.4,33.629629629629626,"DER",45400]
[null,null,null,null,null,null,null,null,null,null,"24.15.04","TUBO DRENO BARRO 20CM","m",60.41,44.74814814814814,"DER",60410]
[null,null,null,null,null,null,null,null,null,null,"24.15.05","TUBO DE PVC PERFURADO OU NAO D=0,05M","m",20.06,14.859259259259257,"DER",20060]
[null,null,null,null,null,null,null,null,null,null,"24.15.06","TUBO DE PVC PERFURADO OU NAO D=0,075M","m",25.56,18.93333333333333,"DER",25560]
[null,null,null,null,null,null,null,null,null,null,"24.15.07","TUBO DE PVC PERFURADO OU NAO D=0,10M","m",36.29,26.88148148148148,"DER",36290]
[null,null,null,null,null,null,null,null,null,null,"24.15.08","TUBO DE PVC PERFURADO OU NAO D=0,15M","m",73.33,54.318518518518516,"DER",73330]
[null,null,null,null,null,null,null,null,null,null,"24.15.09","DRENO HORIZONTAL PROFunDO","m",201.4,149.1851851851852,"DER",201400]
[null,null,null,null,null,null,null,null,null,null,"24.15.09.01","DRENO LONGITUDINAL PROFunDO PARA CORTE EM ROCHA DPR-PP-DE-","m",133.5,98.88888888888889,"DER",133500]
[null,null,null,null,null,null,null,null,null,null,null,"H07/123",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.15.09.02","DRENO TRANSVERSAL RASO PARA CORTE EM ROCHA TIPO DRR, PP-DE-H07/123.","m",28.95,21.444444444444443,"DER",28950]
[null,null,null,null,null,null,null,null,null,null,"24.15.09.03","DRENO LONGITUDINAL RASO DLR-2, PP-DE-H07/125.","m",59.83,44.318518518518516,"DER",59830]
[null,null,null,null,null,null,null,null,null,null,"24.15.09.04","DRENOS LONGITUDINAIS PROFunDOS PARA SOLOS ARENOSOS","m",124.23,92.02222222222223,"DER",124230]
[null,null,null,null,null,null,null,null,null,null,"24.15.09.05","DRENOS LONGITUDINAIS PROFunDOS EM SOLOS SILTOSOS E/OU ARGILOSOS","m",138,102.22222222222221,"DER",138000]
[null,null,null,null,null,null,null,null,null,null,"24.15.11","TUBO DRENO DE POLIET.DE ALTA DENS.0,10M","m",32.9,24.370370370370367,"DER",32900]
[null,null,null,null,null,null,null,null,null,null,"24.15.12","TUBO DRENO DE POLIET.DE ALTA DENS.0,15M","m",52.22,38.68148148148148,"DER",52220]
[null,null,null,null,null,null,null,null,null,null,"24.15.13","TUBO DRENO DE POLIET.DE ALTA DENS.0,20M","m",89.95,66.62962962962963,"DER",89950]
[null,null,null,null,null,null,null,null,null,null,"24.15.14","DUTO CORRUG. PEAD 0,05M","m",23.62,17.496296296296297,"DER",23620]
[null,null,null,null,null,null,null,null,null,null,"24.15.15","DUTO CORRUG.PEAD 0,075M","m",35.09,25.992592592592594,"DER",35090]
[null,null,null,null,null,null,null,null,null,null,"24.15.16","DUTO CORRUG.PEAD 0,10M","m",44.53,32.98518518518518,"DER",44530]
[null,null,null,null,null,null,null,null,null,null,"24.15.17","DUTO CORRUG.PEAD 0,15M","m",93.35,69.14814814814814,"DER",93350]
[null,null,null,null,null,null,null,null,null,null,"24.16.01","TUBO DE CONCRETO D=0,40M CLASSE PA-1","m",136.48,101.09629629629629,"DER",136480]
[null,null,null,null,null,null,null,null,null,null,"24.16.02","TUBO DE CONCRETO D=0,40M CLASSE PA-2","m",138.25,102.4074074074074,"DER",138250]
[null,null,null,null,null,null,null,null,null,null,"24.16.03","TUBO DE CONCRETO D=0,50M CLASSE PA-1","m",183.71,136.0814814814815,"DER",183710]
[null,null,null,null,null,null,null,null,null,null,"24.16.04","TUBO DE CONCRETO D=0,50M CLASSE PA-2","m",183.95,136.25925925925924,"DER",183950]
[null,null,null,null,null,null,null,null,null,null,"24.16.05","TUBO DE CONCRETO D=0,50M CLASSE PA-3","m",193.33,143.2074074074074,"DER",193330]
[null,null,null,null,null,null,null,null,null,null,"24.16.06","TUBO DE CONCRETO D=0,50M CLASSE PA-4","m",201.77,149.45925925925926,"DER",201770]
[null,null,null,null,null,null,null,null,null,null,"24.16.07","TUBO DE CONCRETO D=0,60M CLASSE PA-1","m",203.84,150.9925925925926,"DER",203840]
[null,null,null,null,null,null,null,null,null,null,"24.16.08","TUBO DE CONCRETO D=0,60M CLASSE PA-2","m",224.28,166.13333333333333,"DER",224280]
[null,null,null,null,null,null,null,null,null,null,"24.16.09","TUBO DE CONCRETO D=0,60M CLASSE PA-3","m",252.46,187.0074074074074,"DER",252460]
[null,null,null,null,null,null,null,null,null,null,"24.16.10","TUBO DE CONCRETO D=0,60M CLASSE PA-4","m",284.12,210.45925925925926,"DER",284120]
[null,null,null,null,null,null,null,null,null,null,"24.16.11","TUBO DE CONCRETO D=0,80M CLASSE PA-1","m",323.15,239.37037037037032,"DER",323150]
[null,null,null,null,null,null,null,null,null,null,"24.16.12","TUBO DE CONCRETO D=0,80M CLASSE PA-2","m",328.77,243.5333333333333,"DER",328770]
[null,null,null,null,null,null,null,null,null,null,"24.16.13","TUBO DE CONCRETO D=0,80M CLASSE PA-3","m",407.45,301.8148148148148,"DER",407450]
[null,null,null,null,null,null,null,null,null,null,"24.16.14","TUBO DE CONCRETO D=0,80M CLASSE PA-4","m",467.75,346.48148148148147,"DER",467750]
[null,null,null,null,null,null,null,null,null,null,"24.16.15","TUBO DE CONCRETO D=1,00M CLASSE PA-1","m",440.69,326.437037037037,"DER",440690]
[null,null,null,null,null,null,null,null,null,null,"24.16.16","TUBO DE CONCRETO D=1,00M CLASSE PA-2","m",453.48,335.9111111111111,"DER",453480]
[null,null,null,null,null,null,null,null,null,null,"24.16.17","TUBO DE CONCRETO D=1,00M CLASSE PA-3","m",560.15,414.92592592592587,"DER",560150]
[null,null,null,null,null,null,null,null,null,null,"24.16.18","TUBO DE CONCRETO D=1,00M CLASSE PA-4","m",579.06,428.9333333333333,"DER",579060]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.16.19","TUBO DE CONCRETO D=1,20M CLASSE PA-1","m",657.41,486.9703703703703,"DER",657410]
[null,null,null,null,null,null,null,null,null,null,"24.16.20","TUBO DE CONCRETO D=1,20M CLASSE PA-2","m",715.88,530.2814814814815,"DER",715880]
[null,null,null,null,null,null,null,null,null,null,"24.16.21","TUBO DE CONCRETO D=1,20M CLASSE PA-3","m",811.58,601.1703703703704,"DER",811580]
[null,null,null,null,null,null,null,null,null,null,"24.16.22","TUBO DE CONCRETO D=1,20M CLASSE PA-4","m",831.75,616.1111111111111,"DER",831750]
[null,null,null,null,null,null,null,null,null,null,"24.16.23","TUBO DE CONCRETO D=1,50M CLASSE PA-1","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.026,370"]
[null,null,null,null,null,null,null,null,null,null,"24.16.24","TUBO DE CONCRETO D=1,50M CLASSE PA-2","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.045,410"]
[null,null,null,null,null,null,null,null,null,null,"24.16.25","TUBO DE CONCRETO D=1,50M CLASSE PA-3","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.215,800"]
[null,null,null,null,null,null,null,null,null,null,"24.16.26","TUBO DE CONCRETO D=1,50M CLASSE PA-4","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.253,630"]
[null,null,null,null,null,null,null,null,null,null,"24.16.27","TUBO DE CONCRETO SIMPLES D=0,40M","m",82.63,61.2074074074074,"DER",82630]
[null,null,null,null,null,null,null,null,null,null,"24.16.28","TUBO DE CONCRETO SIMPLES D=0,60M","m",123.83,91.72592592592592,"DER",123830]
[null,null,null,null,null,null,null,null,null,null,"24.18.01","CANALETA CONCRETO 40CM","m",43.1,31.925925925925924,"DER",43100]
[null,null,null,null,null,null,null,null,null,null,"24.18.02","CANALETA CONCRETO 60CM","m",69.7,51.629629629629626,"DER",69700]
[null,null,null,null,null,null,null,null,null,null,"24.18.03","CANALETA CONCRETO 80CM","m",133.62,98.97777777777777,"DER",133620]
[null,null,null,null,null,null,null,null,null,null,"24.19.03","GUIA PRE-FABRICADA CONCRETO FCK 15MPA","m",45.71,33.85925925925926,"DER",45710]
[null,null,null,null,null,null,null,null,null,null,"24.19.03.01","GUIA PRE-FABRICADA CONCRETO FCK 20 MPA","m",46.86,34.71111111111111,"DER",46860]
[null,null,null,null,null,null,null,null,null,null,"24.19.04.01","SARJETA DE CONCRETO FCK 20 MPA","m³",603.32,446.9037037037037,"DER",603320]
[null,null,null,null,null,null,null,null,null,null,"24.19.05.01","GUIA DE CONCRETO FCK 20 MPA","m³",751.75,556.8518518518518,"DER",751750]
[null,null,null,null,null,null,null,null,null,null,"24.19.06","TELAR E TAMPAO DE FERRO FUNDIDO","un",455.44,337.3629629629629,"DER",455440]
[null,null,null,null,null,null,null,null,null,null,"24.19.07.01","GRELHA DE CONCRETO DE 10X44X120CM - FCK 20 MPA","un",168.8,125.03703703703704,"DER",168800]
[null,null,null,null,null,null,null,null,null,null,"24.19.08","GRELHA FERRO FUNDIDO BOCA LOB GRS-135","un",410,303.7037037037037,"DER",410000]
[null,null,null,null,null,null,null,null,null,null,"24.20.01","TUBO ACO CORR.GALV.MET.NAO DESTRUTIVO","kg",30.56,22.637037037037036,"DER",30560]
[null,null,null,null,null,null,null,null,null,null,"24.20.02","TUBO ACO CORR.EPOXI MET.NAO DESTRUTIVO","kg",31.44,23.288888888888888,"DER",31440]
[null,null,null,null,null,null,null,null,null,null,"24.20.03","TUBO ACO CORR.GALV.MET.DESTRUTIVO","kg",17.21,12.748148148148148,"DER",17210]
[null,null,null,null,null,null,null,null,null,null,"24.20.04","TUBO ACO CORRUGADO EPOXI MET. DESTRUTIVO","kg",18.61,13.785185185185183,"DER",18610]
[null,null,null,null,null,null,null,null,null,null,"24.21.01","BROCA DE CONCRETO ARMADO D=20,00CM","m",48.28,35.76296296296296,"DER",48280]
[null,null,null,null,null,null,null,null,null,null,"24.21.02","BROCA DE CONCRETO D=25,00CM","m",74.6,55.25925925925925,"DER",74600]
[null,null,null,null,null,null,null,null,null,null,"24.21.03","BROCA DE CONCRETO D=15,00CM","m",27.61,20.45185185185185,"DER",27610]
[null,null,null,null,null,null,null,null,null,null,"24.22.01","GEOFORMA TEXTIL TENSORIZADA TIPO COLCHAO - ESPESSURA DE 15 CM","m²",168.58,124.87407407407407,"DER",168580]
[null,null,null,null,null,null,null,null,null,null,"24.22.02","GEOFORMA TEXTIL COM DISPOSITIVO AUTO-DRENANTE \"unIFLUXO\"","m³",571.63,423.4296296296296,"DER",571630]
[null,null,null,null,null,null,null,null,null,null,null,"GEOCOMPOSTO DRENANTE (GEOMANTA+GEOTEXTIL 1 LADO PERM.) TIPO 1L -",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.01","12 MM","m²",19.87,14.718518518518518,"DER",19870]
[null,null,null,null,null,null,null,null,null,null,null,"GEOCOMPOSTO DRENANTE (GEOMANTA+GEOTEXTIL 1 LADO PERM.) TIPO 1S -",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.02","18 MM","m²",22.77,16.866666666666664,"DER",22770]
[null,null,null,null,null,null,null,null,null,null,null,"GEOCOMPOSTO DRENANTE (GEOMANTA+GEOTEXTIL 2 LADOS PERM.TIPO 2L -",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.03","10 MM","m²",25.69,19.02962962962963,"DER",25690]
[null,null,null,null,null,null,null,null,null,null,null,"GEOCOMPOSTO DRENANTE (GEOMANTA+GEOTEXTIL 2 LADOS PERM.)TIPO 2S -",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.04","16 MM","m²",28.58,21.170370370370367,"DER",28580]
[null,null,null,null,null,null,null,null,null,null,null,"GEOCOMP. DRENANTE (GEOMANTA+GEOTEXTIL 1 LADO PER./1 LADOIMP.) TIPO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.05","2L FP-10MM","m²",32.94,24.399999999999995,"DER",32940]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.06","GEOCOMP. TRINCHEIRA DRENANTE (GEOMANTA+GEOTEXTIL 2 LADOS PERM.)","m",36.6,27.11111111111111,"DER",36600]
[null,null,null,null,null,null,null,null,null,null,null,"H=90CM / 10MM",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.07","GEOCOMP. TRINCHEIRA DRENANTE (GEOMANTA+GEOTEXTIL 2 LADOSPERM.)","m",20.99,15.548148148148146,"DER",20990]
[null,null,null,null,null,null,null,null,null,null,null,"H=60CM / 10MM",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.08","GEOCOMP. TRINCHEIRA DRENANTE (GEOMANTA+GEOTEXTIL 2 LADOS PERM.)","m",24.07,17.82962962962963,"DER",24070]
[null,null,null,null,null,null,null,null,null,null,null,"H=30CM / 10MM",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"24.23.09","GEOCOMPOSTO DRENANTE VERTICAL (GEOMANTA + GEOTEXTIL 2","m",27.12,20.08888888888889,"DER",27120]
[null,null,null,null,null,null,null,null,null,null,null,"LADOSPERM.)",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.01.01","ATERRO DE ACESSO","m³",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"25.01.02","ATERRO SOLO COM 3% DE CIMENTO EM USINA","m³",51.59,38.214814814814815,"DER",51590]
[null,null,null,null,null,null,null,null,null,null,"25.01.03","ATERRO SOLO COM 3% DE CIMENTO C/PULVE.","m³",47.85,35.44444444444444,"DER",47850]
[null,null,null,null,null,null,null,null,null,null,"25.01.03.05","ATERRO SOLO COM 6% DE CIMENTO C/PULVE.","m³",89.83,66.54074074074073,"DER",89830]
[null,null,null,null,null,null,null,null,null,null,"25.02.01","ESCAVACAO MANUAL PARA OBRAS S/EXPLOSIVO","m³",50.17,37.162962962962965,"DER",50170]
[null,null,null,null,null,null,null,null,null,null,"25.02.02","ESCAVACAO MECANICA P/ OBRAS S/EXPLOSIVO","m³",10.92,8.088888888888889,"DER",10920]
[null,null,null,null,null,null,null,null,null,null,"25.02.03","ESCAVACAO MECANICA P/ OBRAS C/EXPLOSIVO","m³",43.09,31.918518518518518,"DER",43090]
[null,null,null,null,null,null,null,null,null,null,"25.02.04","CORTA-RIO ESCAVACAO SEM EXPLOSIVO","m³",10.92,8.088888888888889,"DER",10920]
[null,null,null,null,null,null,null,null,null,null,"25.02.05","CORTA-RIO ESCAVACAO COM EXPLOSIVO","m³",43.09,31.918518518518518,"DER",43090]
[null,null,null,null,null,null,null,null,null,null,"25.02.06","ESCAV.FunD.BUEIRO OU DRENO S/EXPL.ATE 2M","m³",62.83,46.54074074074074,"DER",62830]
[null,null,null,null,null,null,null,null,null,null,"25.02.07","ACRESC.P/ESCAV.1,5M PROFunDIDADE,ALEM 2M","m³",13.05,9.666666666666666,"DER",13050]
[null,null,null,null,null,null,null,null,null,null,"25.02.08","ESCAV.FunD.BUEIRO OU DRENO C/EXPL.ATE 2M","m³",199.61,147.85925925925926,"DER",199610]
[null,null,null,null,null,null,null,null,null,null,"25.02.09","ACRESC.ESC.ENS.EXPL.C/1,5M PROF.ALEM 2M","m³",18.94,14.02962962962963,"DER",18940]
[null,null,null,null,null,null,null,null,null,null,"25.02.10","ESCAV.FunD.DENTRO ENSEC. SEM EXPL.ATE 3M","m³",53.8,39.85185185185185,"DER",53800]
[null,null,null,null,null,null,null,null,null,null,"25.02.11","ACR.P/ESCAV.ENSEC.P/CADA1,0M PROF.ALEm³M","m³",10.78,7.985185185185184,"DER",10780]
[null,null,null,null,null,null,null,null,null,null,"25.02.12","ESCAV.FunD.DENTRO ENSEC.C/EXPL.ATE  3M","m³",166.18,123.09629629629629,"DER",166180]
[null,null,null,null,null,null,null,null,null,null,"25.02.13","ACRESC.P/ESC.ENSEC.C/EXPL.C/1,5M ALEM 3M","m³",18.94,14.02962962962963,"DER",18940]
[null,null,null,null,null,null,null,null,null,null,"25.03.01","PAREDE ENSECADEIRA COM PRANCHA-ESP.0,05M","m²",199.49,147.77037037037036,"DER",199490]
[null,null,null,null,null,null,null,null,null,null,"25.03.02","PAREDE ENSECADEIRA C/PRANCHA-ESP.0,075M","m²",280.41,207.7111111111111,"DER",280410]
[null,null,null,null,null,null,null,null,null,null,"25.03.03","PAREDE ENSECADEIRA COM PERFIL METALICO","m²",388.21,287.56296296296296,"DER",388210]
[null,null,null,null,null,null,null,null,null,null,"25.03.04","ARGILA ENCH.ENSECADEIRA,INCL.APILOAMENTO","m³",51.11,37.859259259259254,"DER",51110]
[null,null,null,null,null,null,null,null,null,null,"25.03.04.01","ENSECADEIRA COM SACOS DE AREIA","m³",362.86,268.7851851851852,"DER",362860]
[null,null,null,null,null,null,null,null,null,null,"25.03.04.03","SOLO CIMENTO ENSACADO, COM TEOR DE CIMENTO A 4%","m³",180.52,133.71851851851852,"DER",180520]
[null,null,null,null,null,null,null,null,null,null,"25.03.04.04","SOLO CIMENTO ENSACADO, COM TEOR DE CIMENTO A 6%","m³",200.44,148.47407407407405,"DER",200440]
[null,null,null,null,null,null,null,null,null,null,"25.03.05","ESGOTAMENTO CONTINUO AGUA","m³",2.02,1.4962962962962962,"DER",2020]
[null,null,null,null,null,null,null,null,null,null,"25.03.06","ESCORAMENTO DE VALAS/CAVAS P/FunD.CONT.","m²",96,71.1111111111111,"DER",96000]
[null,null,null,null,null,null,null,null,null,null,"25.03.07","ESCORAMENTO DE VALAS/CAVAS P/FunD.DESC.","m²",64.68,47.91111111111111,"DER",64680]
[null,null,null,null,null,null,null,null,null,null,"25.03.08","ESCORAMENTO PARA FORMAS","m²",35.8,26.518518518518515,"DER",35800]
[null,null,null,null,null,null,null,null,null,null,"25.04.01","ESTACA CONCRETO PRE-MOLDADO - 20/25T","m",88.2,65.33333333333333,"DER",88200]
[null,null,null,null,null,null,null,null,null,null,"25.04.02","ESTACA CONCRETO PRE-MOLDADO - 30/35T","m",93.66,69.37777777777777,"DER",93660]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.04.03","ESTACA CONCRETO PRE-MOLDADO - 40/45T","m",112.1,83.03703703703702,"DER",112100]
[null,null,null,null,null,null,null,null,null,null,"25.04.04","ESTACA CONCRETO PRE-MOLDADO - 50/60T","m",131.4,97.33333333333333,"DER",131400]
[null,null,null,null,null,null,null,null,null,null,"25.04.05","ESTACA CONCRETO PRE-MOLDADO - 70/80T","m",185.58,137.46666666666667,"DER",185580]
[null,null,null,null,null,null,null,null,null,null,"25.04.06","ESTACA METALICA, FORNEC. E CRAVACAO","kg",9.17,6.792592592592592,"DER",9170]
[null,null,null,null,null,null,null,null,null,null,"25.04.07","ESTACA DE MADEIRA D=20CM - 8 TON","m",75.5,55.925925925925924,"DER",75500]
[null,null,null,null,null,null,null,null,null,null,"25.04.08","ESTACA DE MADEIRA D=25CM - 15TON","m",82.99,61.47407407407407,"DER",82990]
[null,null,null,null,null,null,null,null,null,null,"25.04.09","ESTACA RAIZ EM SOLO D=15CM","m",263.06,194.85925925925926,"DER",263060]
[null,null,null,null,null,null,null,null,null,null,"25.04.10","ESTACA RAIZ EM SOLO D=16CM","m",281.8,208.74074074074073,"DER",281800]
[null,null,null,null,null,null,null,null,null,null,"25.04.11","ESTACA RAIZ EM SOLO D=20CM","m",333.91,247.34074074074076,"DER",333910]
[null,null,null,null,null,null,null,null,null,null,"25.04.12","ESTACA RAIZ EM SOLO D=25CM","m",402.59,298.21481481481476,"DER",402590]
[null,null,null,null,null,null,null,null,null,null,"25.04.13","ESTACA RAIZ EM SOLO D=31CM","m",507.33,375.79999999999995,"DER",507330]
[null,null,null,null,null,null,null,null,null,null,"25.04.14","ESTACA RAIZ EM SOLO D=40CM","m",692.39,512.8814814814814,"DER",692390]
[null,null,null,null,null,null,null,null,null,null,"25.04.15","ESTACA RAIZ EM ROCHA ALTERADA D=15CM","m",624.49,462.58518518518514,"DER",624490]
[null,null,null,null,null,null,null,null,null,null,"25.04.16","ESTACA RAIZ EM ROCHA ALTERADA D=16CM","m",645.46,478.1185185185185,"DER",645460]
[null,null,null,null,null,null,null,null,null,null,"25.04.17","ESTACA RAIZ EM ROCHA ALTERADA D=20CM","m",774.78,573.911111111111,"DER",774780]
[null,null,null,null,null,null,null,null,null,null,"25.04.18","ESTACA RAIZ EM ROCHA ALTERADA D=25CM","m",888.58,658.2074074074073,"DER",888580]
[null,null,null,null,null,null,null,null,null,null,"25.04.19","ESTACA RAIZ EM ROCHA ALTERADA D=31CM","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.132,680"]
[null,null,null,null,null,null,null,null,null,null,"25.04.20","ESTACA RAIZ EM ROCHA ALTERADA D=40CM","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.438,250"]
[null,null,null,null,null,null,null,null,null,null,"25.04.21","TAXA DE INSTALACAO EQUIPAM.ESTACA RAIZ","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","18.547,580"]
[null,null,null,null,null,null,null,null,null,null,"25.04.23.01","ESTACA TIPO STRAUSS D=32CM","m",79.8,59.11111111111111,"DER",79800]
[null,null,null,null,null,null,null,null,null,null,"25.04.28","TAXA MOBIL. DE EQUIPAMENTO BATE-ESTACA","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.491,870"]
[null,null,null,null,null,null,null,null,null,null,"25.05.01","ANDAIME DE MADEIRA","m³",12.63,9.355555555555556,"DER",12630]
[null,null,null,null,null,null,null,null,null,null,"25.05.02","ANDAIME TUBULAR","m³",18.12,13.422222222222222,"DER",18120]
[null,null,null,null,null,null,null,null,null,null,"25.06.01","FORMA PLANA PARA CONCRETO ARMADO COMUM","m²",80.07,59.3111111111111,"DER",80070]
[null,null,null,null,null,null,null,null,null,null,"25.06.02","FORMA PL.P/CONCRETO PROTENDIDO OU APAR.","m²",90.3,66.88888888888889,"DER",90300]
[null,null,null,null,null,null,null,null,null,null,"25.07.01","BARRA DE ACO CA-25","kg",8.78,6.503703703703703,"DER",8780]
[null,null,null,null,null,null,null,null,null,null,"25.07.02","BARRA DE ACO CA-50","kg",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"25.07.03","BARRA DE ACO CA-60","kg",9.2,6.814814814814814,"DER",9200]
[null,null,null,null,null,null,null,null,null,null,"25.07.04","ACO PARA CONCRETO PROTENDIDO","kg",19.14,14.177777777777777,"DER",19140]
[null,null,null,null,null,null,null,null,null,null,"25.07.05","TELA METALICA","kg",7.38,5.466666666666666,"DER",7380]
[null,null,null,null,null,null,null,null,null,null,"25.07.06","ACO P/CONCRETO PROTENDIDO TIPO DYWIDAG","kg",29.82,22.08888888888889,"DER",29820]
[null,null,null,null,null,null,null,null,null,null,"25.08.02","AP.ANC.P/CABOS PROTEN.ATIVA 12 FIOS-8MM","un",689.95,511.0740740740741,"DER",689950]
[null,null,null,null,null,null,null,null,null,null,"25.08.03","AP.ANC.P/CABOS PROTEN.ATIVA 4FIOS-12,7MM","un",553.32,409.8666666666667,"DER",553320]
[null,null,null,null,null,null,null,null,null,null,"25.08.04","AP.ANC.P/CABOS PROTEN.ATIVA 6FIOS-12,7MM","un",766.88,568.0592592592592,"DER",766880]
[null,null,null,null,null,null,null,null,null,null,"25.08.05","AP.ANC.P/CABOS PROTEN.ATIV.12FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.580,840"]
[null,null,null,null,null,null,null,null,null,null,"25.08.06","AP.ANC.P/CABOS PROTEN.ATIV.19FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.609,960"]
[null,null,null,null,null,null,null,null,null,null,"25.08.07","AP.ANC.P/CABOS PROTEN.ATIV.22FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.339,470"]
[null,null,null,null,null,null,null,null,null,null,"25.08.09","AP.ANC.P/CABOS PROTEN.PAS. 4 FIOS-12,7MM","un",108.01,80.0074074074074,"DER",108010]
[null,null,null,null,null,null,null,null,null,null,"25.08.10","AP.ANC.P/CABOS PROTEN.PAS. 6 FIOS-12,7MM","un",148.07,109.68148148148147,"DER",148070]
[null,null,null,null,null,null,null,null,null,null,"25.08.11","AP.ANC.P/CABOS PROTEN.PAS. 12FIOS-12,7MM","un",515.05,381.5185185185185,"DER",515050]
[null,null,null,null,null,null,null,null,null,null,"25.08.12","AP.ANC.P/CABOS PROTEN.PAS. 19FIOS-12,7MM","un",972.92,720.6814814814815,"DER",972920]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.08.13.01","APARELHO DE ANCORAGEM ATIVO DE 4 FIOS DE Ã 5/8\" (15,2MM)","un",741.27,549.0888888888888,"DER",741270]
[null,null,null,null,null,null,null,null,null,null,"25.08.13.02","APARELHO DE ANCORAGEM ATIVO DE 12 FIOS DE Ã 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.358,030"]
[null,null,null,null,null,null,null,null,null,null,"25.08.13.03","APARELHO DE ANCORAGEM ATIVO DE 15 FIOS DE Ã 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.202,050"]
[null,null,null,null,null,null,null,null,null,null,"25.08.13.04","APARELHO DE ANCORAGEM ATIVO DE 19 FIOS DE Ã 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.829,970"]
[null,null,null,null,null,null,null,null,null,null,"25.08.15.01","TIRANTE  40TF 5 FIOS D=1/2\" FORN. E INST","m",185.59,137.47407407407405,"DER",185590]
[null,null,null,null,null,null,null,null,null,null,"25.08.15.02","TIRANTE  60TF 8 FIOS D=1/2\" FORN. E INST","m",211.36,156.56296296296296,"DER",211360]
[null,null,null,null,null,null,null,null,null,null,"25.08.15.03","TIRANTE  80TF 10 FIOS D=1/2\" FORN.E INST","m",237.58,175.98518518518517,"DER",237580]
[null,null,null,null,null,null,null,null,null,null,"25.08.15.04","TIRAN.100TF 12 FIOS D=1/2\" FORN.E INST.","m",258.66,191.6,"DER",258660]
[null,null,null,null,null,null,null,null,null,null,"25.08.16.01","TERMO FIXO P/TIRANTES 40TF 5 FIOS D=1/2\"","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.155,050"]
[null,null,null,null,null,null,null,null,null,null,"25.08.16.02","TERMO FIXO P/TIRANTES 60TF 8 FIOS D=1/2\"","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.602,980"]
[null,null,null,null,null,null,null,null,null,null,"25.08.16.03","TERMO FIXO P/TIRANTES 80TF 10FIOS D=1/2\"","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.816,910"]
[null,null,null,null,null,null,null,null,null,null,"25.08.16.04","TERMO FIXO P/TIRANTES 100TF 12F D=1/2\"","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.971,940"]
[null,null,null,null,null,null,null,null,null,null,"25.09.01","CONCRETO FCK 10 MPA","m³",386.3,286.14814814814815,"DER",386300]
[null,null,null,null,null,null,null,null,null,null,"25.09.02","CONCRETO FCK 15 MPA","m³",426.19,315.6962962962963,"DER",426190]
[null,null,null,null,null,null,null,null,null,null,"25.09.03","CONCRETO FCK 18 MPA","m³",435.69,322.7333333333333,"DER",435690]
[null,null,null,null,null,null,null,null,null,null,"25.09.04","CONCRETO FCK 20 MPA","m³",455.28,337.2444444444444,"DER",455280]
[null,null,null,null,null,null,null,null,null,null,"25.09.05","CONCRETO FCK 25 MPA","m³",467.63,346.39259259259256,"DER",467630]
[null,null,null,null,null,null,null,null,null,null,"25.09.06","CONCRETO FCK 30 MPA","m³",483.41,358.0814814814815,"DER",483410]
[null,null,null,null,null,null,null,null,null,null,"25.09.07","CONCRETO FCK 35 MPA","m³",493.31,365.4148148148148,"DER",493310]
[null,null,null,null,null,null,null,null,null,null,"25.09.08","CONCRETO CICLOPICO","m³",390.4,289.18518518518516,"DER",390400]
[null,null,null,null,null,null,null,null,null,null,"25.09.10","CONCRETO PROJETADO","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.241,410"]
[null,null,null,null,null,null,null,null,null,null,"25.09.11","BOMBEAMENTO CONCRETO QUALQUER RESIST.","m³",42.12,31.199999999999996,"DER",42120]
[null,null,null,null,null,null,null,null,null,null,"25.09.12","INJECAO DE NATA DE CIMENTO","kg",2.64,1.9555555555555555,"DER",2640]
[null,null,null,null,null,null,null,null,null,null,"25.09.15","CONCRETO FCK 40 MPA","m³",522.21,386.82222222222225,"DER",522210]
[null,null,null,null,null,null,null,null,null,null,"25.09.16","CONCRETO FCK 45 MPA","m³",590.18,437.1703703703703,"DER",590180]
[null,null,null,null,null,null,null,null,null,null,"25.09.17","CONCRETO FCK 50 MPA","m³",609.63,451.5777777777777,"DER",609630]
[null,null,null,null,null,null,null,null,null,null,"25.10.01","PERF.P/DRENO E TIR. SOLO D=57,10MM(AX)","m",140.77,104.27407407407408,"DER",140770]
[null,null,null,null,null,null,null,null,null,null,"25.10.02","PERF.P/DRENO E TIR. SOLO D=73,00MM(BX)","m",141.93,105.13333333333333,"DER",141930]
[null,null,null,null,null,null,null,null,null,null,"25.10.03","PERF.P/DRENO E TIR. SOLO D=88,90MM(NX)","m",147.96,109.6,"DER",147960]
[null,null,null,null,null,null,null,null,null,null,"25.10.04","PERF.P/DRENO E TIR. SOLO D=114,30MM(HX)","m",151.49,112.21481481481482,"DER",151490]
[null,null,null,null,null,null,null,null,null,null,"25.10.05","PERF.P/DRENO E TIR.RCH.ALT.D=57,10MM(AX)","m",354.38,262.5037037037037,"DER",354380]
[null,null,null,null,null,null,null,null,null,null,"25.10.06","PERF.P/DRENO E TIR.RCH.ALT.D=73,00MM(BX)","m",422.02,312.6074074074074,"DER",422020]
[null,null,null,null,null,null,null,null,null,null,"25.10.07","PERF.P/DRENO E TIR.RCH.ALT.D=88,90MM(NX)","m",478.01,354.08148148148143,"DER",478010]
[null,null,null,null,null,null,null,null,null,null,"25.10.08","PERF.P/DRENO E TIR.RCH.ALT.D=114,3MM(HX)","m",528.3,391.33333333333326,"DER",528300]
[null,null,null,null,null,null,null,null,null,null,"25.10.09","PERF.P/DRENO E TIR.RCH SA D=57,10MM (AX)","m",538.18,398.6518518518518,"DER",538180]
[null,null,null,null,null,null,null,null,null,null,"25.10.10","PERF.P/DRENO E TIR.RCH SA D=73,00MM(BX)","m",639.14,473.437037037037,"DER",639140]
[null,null,null,null,null,null,null,null,null,null,"25.10.11","PERF.P/DRENO E TIR.RCH. SA D=88,90MM(NX)","m",721.28,534.2814814814815,"DER",721280]
[null,null,null,null,null,null,null,null,null,null,"25.10.12","PERF.P/DRENO E TIR RCH SA D=114,30MM(HX)","m",789,584.4444444444445,"DER",789000]
[null,null,null,null,null,null,null,null,null,null,"25.10.14","PERFURACAO MANUAL EM SOLO D=62,5MM OU D=2 1/2\"","m",9.55,7.074074074074074,"DER",9550]
[null,null,null,null,null,null,null,null,null,null,"25.10.15","PERFURAÇÃO MANUAL EM SOLO D=114,3MM OU D=4\"","m",14.07,10.422222222222222,"DER",14070]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.11.01","ENROCAMENTO PEDRA ARRUMADA","m³",210.83,156.17037037037036,"DER",210830]
[null,null,null,null,null,null,null,null,null,null,"25.11.02","ENROCAMENTO PEDRA ARRUMADA E REJunTADA","m³",324.57,240.4222222222222,"DER",324570]
[null,null,null,null,null,null,null,null,null,null,"25.11.03","ENROCAMENTO PEDRA JOGADA","m³",136.02,100.75555555555556,"DER",136020]
[null,null,null,null,null,null,null,null,null,null,"25.11.04","GABIAO TIPO CAIXA LARGURA 50CM - TELA GALVANIZADA","m³",382.7,283.48148148148147,"DER",382700]
[null,null,null,null,null,null,null,null,null,null,"25.11.05.01","GABIAO TIPO COLCHAO ESPESSURA 17CM - TELA GALVANIZADA","m²",104.78,77.6148148148148,"DER",104780]
[null,null,null,null,null,null,null,null,null,null,"25.11.06.01","GABIAO TIPO COLCHAO ESPESSURA 23CM - TELA GALVANIZADA","m²",120.62,89.34814814814814,"DER",120620]
[null,null,null,null,null,null,null,null,null,null,"25.11.07.01","GABIAO TIPO COLCHAO ESPESSURA 30CM - TELA GALVANIZADA","m²",137.11,101.56296296296297,"DER",137110]
[null,null,null,null,null,null,null,null,null,null,"25.11.08.01","GABIAO TIPO COLCHAO ESPESSURA 17CM - TELA PVC","m²",120.18,89.02222222222223,"DER",120180]
[null,null,null,null,null,null,null,null,null,null,"25.11.09.01","GABIAO TIPO COLCHAO ESPESSURA 23CM - TELA PVC","m²",134.85,99.88888888888887,"DER",134850]
[null,null,null,null,null,null,null,null,null,null,"25.11.10.01","GABIAO TIPO COLCHAO ESPESSURA 30CM - TELA PVC","m²",152.78,113.17037037037036,"DER",152780]
[null,null,null,null,null,null,null,null,null,null,"25.11.11","GABIAO TIPO SACO - TELA GALVANIZADA","m³",345.79,256.14074074074074,"DER",345790]
[null,null,null,null,null,null,null,null,null,null,"25.12.02","CALCAMENTO CONCRETO FCK 15 MPA","m³",610.14,451.9555555555555,"DER",610140]
[null,null,null,null,null,null,null,null,null,null,"25.12.03","CALCAMENTO CONCRETO FCK 10 MPA","m³",568.25,420.9259259259259,"DER",568250]
[null,null,null,null,null,null,null,null,null,null,"25.13.01","ALVENARIA TIJOLO","m³",797.65,590.8518518518518,"DER",797650]
[null,null,null,null,null,null,null,null,null,null,"25.13.02","ALVENARIA DE PEDRA SECA","m³",304.1,225.25925925925927,"DER",304100]
[null,null,null,null,null,null,null,null,null,null,"25.13.04","ALVENARIA DE PEDRA ARGAMASSADA","m³",539.1,399.3333333333333,"DER",539100]
[null,null,null,null,null,null,null,null,null,null,"25.13.05","ALVENARIA DE BLOCO DE CONCRETO","m³",460.87,341.38518518518515,"DER",460870]
[null,null,null,null,null,null,null,null,null,null,"25.13.07","ARGAM.DE CIMENTO E AREIA TRACO 1:3 E=2CM","m²",34.41,25.488888888888884,"DER",34410]
[null,null,null,null,null,null,null,null,null,null,"25.14.02","MANTA GEOTEXTIL TECIDA","kg",35.21,26.08148148148148,"DER",35210]
[null,null,null,null,null,null,null,null,null,null,"25.15.01","FORNECIMENTO DE TUBO DRENO CONCRETO 15CM","m",28.09,20.807407407407407,"DER",28090]
[null,null,null,null,null,null,null,null,null,null,"25.15.02","FORNECIMENTO DE TUBO DRENO CONCRETO 20CM","m",35.6,26.37037037037037,"DER",35600]
[null,null,null,null,null,null,null,null,null,null,"25.15.03","FORNECIMENTO DE TUBO DRENO BARRO 15CM","m",28.09,20.807407407407407,"DER",28090]
[null,null,null,null,null,null,null,null,null,null,"25.15.04","FORNECIMENTO DE TUBO DRENO BARRO 20CM","m",35.6,26.37037037037037,"DER",35600]
[null,null,null,null,null,null,null,null,null,null,"25.15.05","ASSENTAMENTO DE TUBO DRENO CONCRETO 15CM","m",27.01,20.007407407407406,"DER",27010]
[null,null,null,null,null,null,null,null,null,null,"25.15.06","ASSENTAMENTO DE TUBO DRENO CONCRETO 20CM","m",32.18,23.837037037037035,"DER",32180]
[null,null,null,null,null,null,null,null,null,null,"25.15.07","ASSENTAMENTO DE TUBO DRENO BARRO 15 CM","m",25.3,18.74074074074074,"DER",25300]
[null,null,null,null,null,null,null,null,null,null,"25.15.08","ASSENTAMENTO DE TUBO DRENO BARRO 20CM","m",30.36,22.488888888888887,"DER",30360]
[null,null,null,null,null,null,null,null,null,null,"25.15.09","TUBO DE PVC PERFURADO OU NAO D=0,050M","m",20.06,14.859259259259257,"DER",20060]
[null,null,null,null,null,null,null,null,null,null,"25.15.09.01","TUBO DE PVC PERFURADO OU NAO D=0,025M (D=1\")","m",16.11,11.933333333333332,"DER",16110]
[null,null,null,null,null,null,null,null,null,null,"25.15.10","TUBO DE PVC PERFURADO OU NAO D=0,075M","m",25.56,18.93333333333333,"DER",25560]
[null,null,null,null,null,null,null,null,null,null,"25.15.11","TUBO DE PVC PERFURADO OU NAO D=0,10M","m",36.29,26.88148148148148,"DER",36290]
[null,null,null,null,null,null,null,null,null,null,"25.15.12","TUBO DE PVC PERFURADO OU NAO D=0,15M","m",73.33,54.318518518518516,"DER",73330]
[null,null,null,null,null,null,null,null,null,null,"25.19.01","RETALUDAMENTO DE 1 E 2 CATEGORIA","m³",49.47,36.64444444444444,"DER",49470]
[null,null,null,null,null,null,null,null,null,null,"25.20.01","SOLO REFORCADO TIPO GREIDE COM ALTURA DE 0 A 6 METROS.","m²",716.86,531.0074074074074,"DER",716860]
[null,null,null,null,null,null,null,null,null,null,"25.20.02","SOLO REFORCADO TIPO GREIDE COM ALTURA DE 6 A 9 METROS","m²",785.08,581.5407407407407,"DER",785080]
[null,null,null,null,null,null,null,null,null,null,"25.20.03","SOLO REFORCADO TIPO GREIDE COM ALTURA DE 9 A 12 METROS","m²",937.16,694.1925925925925,"DER",937160]
[null,null,null,null,null,null,null,null,null,null,"25.20.04","SOLO REFORCADO TIPO GREIDE COM ALTURA DE 12 A 15 METROS","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.136,500"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.05","SOLO REFORCADO TIPO ENCONTRO PORTANTE COM ALTURA DE 0 A 6 METROS.","m²",998.35,739.5185185185185,"DER",998350]
[null,null,null,null,null,null,null,null,null,null,"25.20.06","SOLO REFORCADO TIPO ENCONTRO PORTANTE COM ALTURA DE 6 A 9 METROS","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.206,440"]
[null,null,null,null,null,null,null,null,null,null,"25.20.07","SOLO REFORCADO TIPO ENCONTRO PORTANTE COM ALTURA DE 9 A 12","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.416,110"]
[null,null,null,null,null,null,null,null,null,null,null,"METROS",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.08","SOLO REFORCADO TIPO ENCONTRO PORTANTE COM ALTURA DE 12 A 15","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.774,650"]
[null,null,null,null,null,null,null,null,null,null,null,"METROS",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.09","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 0 A 6M E ATERRO DE 0","m²",746.59,553.0296296296297,"DER",746590]
[null,null,null,null,null,null,null,null,null,null,null,"A 3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.10","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 0 A 6M E ATERRO DE 3","m²",779.8,577.6296296296296,"DER",779800]
[null,null,null,null,null,null,null,null,null,null,null,"A 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.11","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 0 A 6M E ATERRO","m²",940.67,696.7925925925925,"DER",940670]
[null,null,null,null,null,null,null,null,null,null,null,"MAIOR QUE 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.12","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 6 A 9M E ATERRO DE 0","m²",818.29,606.1407407407406,"DER",818290]
[null,null,null,null,null,null,null,null,null,null,null,"A 3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.13","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 6 A 9M E ATERRO DE 3","m²",940.67,696.7925925925925,"DER",940670]
[null,null,null,null,null,null,null,null,null,null,null,"A 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.14","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 6 A 9M E ATERRO","m²",987.9,731.7777777777777,"DER",987900]
[null,null,null,null,null,null,null,null,null,null,null,"MAIOR QUE 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.15","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 9 A 12M E ATERRO DE","m²",987.9,731.7777777777777,"DER",987900]
[null,null,null,null,null,null,null,null,null,null,null,"0 A 3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.16","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 9 A 12M E ATERRO DE","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.139,990"]
[null,null,null,null,null,null,null,null,null,null,null,"3 A 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.17","SOLO REFORCADO TIPO PE DE TALUDE COM ALTURA DE 9 A 12M E ATERRO","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.139,990"]
[null,null,null,null,null,null,null,null,null,null,null,"MAIOR QUE 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.20.18","SOLO REFORCADO TIPO DE PE DE TALUDE DE 12 A 15M E ATERRO DE 0 A 3M","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.197,710"]
[null,null,null,null,null,null,null,null,null,null,"25.20.19","SOLO REFORCADO TIPO PE DE TALUDE DE 12 A 15M E ATERRO DE 3 A 6M","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.286,240"]
[null,null,null,null,null,null,null,null,null,null,"25.20.20","SOLO REFORCADO TIPO PE DE TALUDE DE 12 A 15M E ATERRO MAIOR QUE 6M","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.323,570"]
[null,null,null,null,null,null,null,null,null,null,"25.21.01","SOLO REF. C/ MALHA HEXAG. DUPLA TORCAO-PANO unICO GREIDE C/ 0 A 6M -","m²",585.72,433.8666666666667,"DER",585720]
[null,null,null,null,null,null,null,null,null,null,null,"EM RACHAO.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.02","SOLO REF. C/ MALHA HEXAG. DUPLA TORCAO-PANO unICO GREIDE C/ 6 A 9M -","m²",626.26,463.89629629629627,"DER",626260]
[null,null,null,null,null,null,null,null,null,null,null,"EM RACHAO.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.03","SOLO REF. C/ MALHA HEXAG. DUPLA TORCAO-PANO unICO GREIDE C/ 9 A 12M","m²",756.51,560.3777777777777,"DER",756510]
[null,null,null,null,null,null,null,null,null,null,null,"- EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.04","SOLO REF. C/ MALHA HEXAG. DUPLA TORCAO-PANO unICO GREIDE C/ 12A15M","m²",902.8,668.7407407407406,"DER",902800]
[null,null,null,null,null,null,null,null,null,null,null,"- EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.05","SOLO REF. C/ MALHA HEXAG. DUPLA TORCAO-PANO unICO GREIDE C/ 15A18M","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.146,670"]
[null,null,null,null,null,null,null,null,null,null,null,"- EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.06","SOLO REF. MALHA HEXAG. DUPLA TORCAO-PANO unICO ENCONTRO PORTAN.0","m²",801.9,594,"DER",801900]
[null,null,null,null,null,null,null,null,null,null,null,"A 6M-EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.07","SOLO REF. MALHA HEXAG. DUPLA TORCAO-PANO unICO ENCONTRO PORTAN.6","m²",991.83,734.6888888888889,"DER",991830]
[null,null,null,null,null,null,null,null,null,null,null,"A 9M-EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.08","SOLO REF.MALHA HEXAG.DUPLA TORCAO-PANO unICO ENCONTRO PORTAN.9","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.144,230"]
[null,null,null,null,null,null,null,null,null,null,null,"A 12M-EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.09","SOLO REF.MALHA HEXAG.DUPLA TORCAO-PANO unICO ENCONTRO PORTAN.12","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.457,390"]
[null,null,null,null,null,null,null,null,null,null,null,"A 15M-EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.10","SOLO REF.MALHA HEXAG.DUPLA TORCAO-PANO unICO ENCONTRO PORTAN.15","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.761,000"]
[null,null,null,null,null,null,null,null,null,null,null,"A 18M-EM RACHAO",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.11","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 0A6M E","m²",582.29,431.32592592592584,"DER",582290]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 0A3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.12","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 0A6M E","m²",622.58,461.1703703703704,"DER",622580]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 3A6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.13","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 0A6M E","m²",660.06,488.9333333333333,"DER",660060]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO > 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.14","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 6A9M E","m²",657.73,487.2074074074074,"DER",657730]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 0A3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.15","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 6A9M E","m²",750.69,556.0666666666667,"DER",750690]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 3A6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.16","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 6A9M E","m²",828.97,614.0518518518518,"DER",828970]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO > 6M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.17","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 9A12M E","m²",808.85,599.1481481481482,"DER",808850]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 0A3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.18","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 9A12M E","m²",925.96,685.8962962962963,"DER",925960]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 3A6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.19","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE DE TALUDE 9A12M E","m²",989.69,733.1037037037037,"DER",989690]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO > 6M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.20","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE TALUDE C/12A15M E","m²",961.88,712.5037037037036,"DER",961880]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 0A3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.21","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE TALUDE C/12A15M E","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.054,530"]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 3A6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.22","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE TALUDE C/12A15M E","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.092,530"]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO > 6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.23","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE TALUDE C/15A18M E","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.068,280"]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 0A3M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.24","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE TALUDE C/15A18M E","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.266,290"]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO 3A6M",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.25","SOLO REF.C/MALHA HEX.DUPLA TORCAO-PANO unICO PE TALUDE C/15A18M E","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.559,140"]
[null,null,null,null,null,null,null,null,null,null,null,"ATERRO > 6M.",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.26","SOLO REF. C/ MALHA HEX. DUPLA TORCAO-PANO unICO VERDE GREIDE C/","m²",465.56,344.85925925925926,"DER",465560]
[null,null,null,null,null,null,null,null,null,null,null,"0A6M - INCL. 70",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.27","SOLO REF. C/ MALHA HEX. DUPLA TORCAO-PANO unICO VERDE GREIDE C/ 6A9M - INCL. 70","m²",574.78,425.7629629629629,"DER",574780]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.28","SOLO REF. C/ MALHA HEX. DUPLA TORCAO-PANO unICO VERDE GREIDE C/9A12M - INCL. 70","m²",672.89,498.437037037037,"DER",672890]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.29","SOLO REF. C/ MALHA HEX. DUPLA TORCAO-PANO unICO VERDE GREIDE C/12A15M - INCL.70","m²",765.29,566.8814814814814,"DER",765290]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.30","SOLO REF. C/ MALHA HEX. DUPLA TORCAO-PANO unICO VERDE GREIDE C/15A18M - INCL.70","m²",857.79,635.4,"DER",857790]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.31","SOL.REF.C/MALH.HEX.DUPL.TORCAO-PANO unICO VERDE PE DE TALUDE C/0A6M-0A3M-INC.70","m²",513.88,380.6518518518518,"DER",513880]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.32","SOL.REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE C/0A6M-3A6M-INC.70","m²",574.78,425.7629629629629,"DER",574780]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.33","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 0A6 E ATERRO >6M","m²",672.89,498.437037037037,"DER",672890]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.34","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 6A9 E ATERRO 0A3M","m²",626.68,464.20740740740735,"DER",626680]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.35","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 6A9 E ATERRO 3A6M","m²",672.89,498.437037037037,"DER",672890]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.36","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 6A9E ATERRO > 6M","m²",765.29,566.8814814814814,"DER",765290]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.37","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 9A12 E ATER.0A3M","m²",719.1,532.6666666666666,"DER",719100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.38","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 9A12 E ATER.3A6M","m²",811.47,601.0888888888888,"DER",811470]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.39","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 9A12E ATER. >6M","m²",888.92,658.4592592592592,"DER",888920]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.40","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 12A15 E ATER.0A3M","m²",811.47,601.0888888888888,"DER",811470]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.41","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 12A15 E ATER.3A6M","m²",908.6,673.037037037037,"DER",908600]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.42","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE12A15 E ATER. >6M","m²",986.65,730.8518518518517,"DER",986650]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.43","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 15A18 E ATER.0A3M","m²",903.87,669.5333333333333,"DER",903870]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.44","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 15A18 E ATER.3A6M","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.112,500"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"25.21.45","SOLO REF.C/MAL.HEX.DUPLA TORCAO-PANO unICO VERDE PE DE TALUDE 15A18 E ATER. >6M","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.181,360"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.01.01","ESCAVACAO MANUAL P/ OBRAS S/EXPLOSIVO","m³",50.17,37.162962962962965,"DER",50170]
[null,null,null,null,null,null,null,null,null,null,"26.01.02","ESCAVACAO MECANICA P/ OBRAS S/EXPLOSIVO","m³",10.92,8.088888888888889,"DER",10920]
[null,null,null,null,null,null,null,null,null,null,"26.01.03","ESCAVACAO MECANICA P/ OBRAS C/ EXPLOSIVO","m³",43.09,31.918518518518518,"DER",43090]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.02.01","ESTACA CONCRETO PRE-MOLDADO - 20/25 T","m",88.2,65.33333333333333,"DER",88200]
[null,null,null,null,null,null,null,null,null,null,"26.02.02","ESTACA CONCRETO PRE-MOLDADO - 30/35 T","m",93.66,69.37777777777777,"DER",93660]
[null,null,null,null,null,null,null,null,null,null,"26.02.03","ESTACA CONCRETO PRE-MOLDADO - 40/45 T","m",112.1,83.03703703703702,"DER",112100]
[null,null,null,null,null,null,null,null,null,null,"26.02.04","ESTACA CONCRETO PRE-MOLDADO - 50/60 T","m",131.4,97.33333333333333,"DER",131400]
[null,null,null,null,null,null,null,null,null,null,"26.02.05","ESTACA CONCRETO PRE-MOLDADO - 70/80 T","m",185.58,137.46666666666667,"DER",185580]
[null,null,null,null,null,null,null,null,null,null,"26.02.06","TAXA MOBIL. DE EQUIP. BATE-ESTACA","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.491,870"]
[null,null,null,null,null,null,null,null,null,null,"26.02.07","ESTACA METALICA, FORNEC. E CRAVACAO","kg",9.17,6.792592592592592,"DER",9170]
[null,null,null,null,null,null,null,null,null,null,"26.02.13","ESTACAO EM SOLO D=1,00M","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.305,790"]
[null,null,null,null,null,null,null,null,null,null,"26.02.14","ESTACAO EM SOLO D=1,20M","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.808,320"]
[null,null,null,null,null,null,null,null,null,null,"26.02.15","ESTACAO EM SOLO D=1,40M","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.361,980"]
[null,null,null,null,null,null,null,null,null,null,"26.02.16","ESTACAO EM SOLO D=1,50M","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.666,040"]
[null,null,null,null,null,null,null,null,null,null,"26.02.17","ESTACAO EM SOLO D=1,60M","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.989,780"]
[null,null,null,null,null,null,null,null,null,null,"26.02.18","ESTACAO EM SOLO D=1,80M","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.766,110"]
[null,null,null,null,null,null,null,null,null,null,"26.02.19","TAXA MOBILIZACAO DE EQUIP. P/ ESTACAO","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","90.891,870"]
[null,null,null,null,null,null,null,null,null,null,"26.02.20","CAMISA METALICA","kg",9.24,6.844444444444444,"DER",9240]
[null,null,null,null,null,null,null,null,null,null,"26.02.20.01","CAMISA METALICA SEM REAPROVEITAMENTO E COM PRE-FURO","kg",10.68,7.9111111111111105,"DER",10680]
[null,null,null,null,null,null,null,null,null,null,"26.02.21","ESTACA DE MADEIRA D=20CM - 8TON","m",75.5,55.925925925925924,"DER",75500]
[null,null,null,null,null,null,null,null,null,null,"26.03.25","ESC.TUB.CEU ABERTO 1/2 CAT. - SOLO","m³",778.69,576.8074074074074,"DER",778690]
[null,null,null,null,null,null,null,null,null,null,"26.03.26","ESC.TUB.AR COMPRIMIDO 1/2 CAT - SOLO","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.966,210"]
[null,null,null,null,null,null,null,null,null,null,"26.03.27","ESC.TUB.CEU ABERTO 3 CAT.- ROCHA","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.161,620"]
[null,null,null,null,null,null,null,null,null,null,"26.03.28","ESC.TUB.AR COMPRIMIDO 3 CAT. - ROCHA","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","4.552,760"]
[null,null,null,null,null,null,null,null,null,null,"26.04.01","CIMBRAMENTO PONTES E VIADUTOS C/ ESTACA","m³",58.82,43.57037037037037,"DER",58820]
[null,null,null,null,null,null,null,null,null,null,"26.04.02","CIMBRAMENTO PONTES E VIADUTOS S/ ESTACA","m³",39.94,29.585185185185182,"DER",39940]
[null,null,null,null,null,null,null,null,null,null,"26.04.03","CIMBRAMENTO DE PASSAGEM SEC. GALERIA RET","m³",34.78,25.762962962962963,"DER",34780]
[null,null,null,null,null,null,null,null,null,null,"26.04.04","CIMBRAMENTO METALICO P/ PONTES E VIADUTO","m³",56.65,41.96296296296296,"DER",56650]
[null,null,null,null,null,null,null,null,null,null,"26.04.05","ANDAIME DE MADEIRA","m³",12.63,9.355555555555556,"DER",12630]
[null,null,null,null,null,null,null,null,null,null,"26.04.06","ANDAIME TUBULAR","m³",18.12,13.422222222222222,"DER",18120]
[null,null,null,null,null,null,null,null,null,null,"26.05.01","FORMA PLANA PARA CONC. ARMADO COMUM","m²",80.07,59.3111111111111,"DER",80070]
[null,null,null,null,null,null,null,null,null,null,"26.05.02","FORMA PLANA P/CONC.PROTEND.OU APARENTE","m²",90.3,66.88888888888889,"DER",90300]
[null,null,null,null,null,null,null,null,null,null,"26.05.03","FORMAS SEM REAPROVEITAMENTO","m²",89.59,66.36296296296297,"DER",89590]
[null,null,null,null,null,null,null,null,null,null,"26.05.04","FORMAS METALICAS ESPECIAL P/ VIGAS","m²",60.61,44.89629629629629,"DER",60610]
[null,null,null,null,null,null,null,null,null,null,"26.05.05","FORMA CURVA PARA CONCRETO COMUM","m²",103.09,76.36296296296295,"DER",103090]
[null,null,null,null,null,null,null,null,null,null,"26.05.06","FORMA CURVA PARA CONCRETO APARENTE","m²",107.66,79.74814814814815,"DER",107660]
[null,null,null,null,null,null,null,null,null,null,"26.06.01","BARRA DE ACO CA-25","kg",8.78,6.503703703703703,"DER",8780]
[null,null,null,null,null,null,null,null,null,null,"26.06.02","BARRA DE ACO CA-50","kg",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"26.06.03","BARRA DE ACO CA-60","kg",9.2,6.814814814814814,"DER",9200]
[null,null,null,null,null,null,null,null,null,null,"26.06.04","ACO PARA CONCRETO PROTENDIDO","kg",19.14,14.177777777777777,"DER",19140]
[null,null,null,null,null,null,null,null,null,null,"26.06.05","TELA METALICA","kg",7.38,5.466666666666666,"DER",7380]
[null,null,null,null,null,null,null,null,null,null,"26.06.06","ACO ST 85/105","kg",29.82,22.08888888888889,"DER",29820]
[null,null,null,null,null,null,null,null,null,null,"26.07.02","AP.ANC.P/CABOS PROTEN.ATIV. 12FIOS-8MM","un",689.95,511.0740740740741,"DER",689950]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.07.03","AP.ANC.P/CABOS PROTEN.ATIV. 4FIOS-12,7MM","un",553.32,409.8666666666667,"DER",553320]
[null,null,null,null,null,null,null,null,null,null,"26.07.04","AP.ANC.P/CABOS PROTEN.ATIV. 6FIOS-12,7MM","un",766.88,568.0592592592592,"DER",766880]
[null,null,null,null,null,null,null,null,null,null,"26.07.05","AP.ANC.P/CABOS PROTEN.ATIV.12FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.580,840"]
[null,null,null,null,null,null,null,null,null,null,"26.07.06","AP.ANC.P/CABOS PROTEN.ATIV.19FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.609,960"]
[null,null,null,null,null,null,null,null,null,null,"26.07.07","AP.ANC.P/CABOS PROTEN.ATIV.22FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.339,470"]
[null,null,null,null,null,null,null,null,null,null,"26.07.09","AP.ANC.P/CABOS PROTEN.PASS. 4FIOS-12,7MM","un",108.01,80.0074074074074,"DER",108010]
[null,null,null,null,null,null,null,null,null,null,"26.07.10","AP.ANC.P/CABOS PROTEN.PASS. 6FIOS-12,7MM","un",148.07,109.68148148148147,"DER",148070]
[null,null,null,null,null,null,null,null,null,null,"26.07.12","AP.ANC.P/CABOS PROTEN.PAS. 19FIOS-12,7MM","un",972.92,720.6814814814815,"DER",972920]
[null,null,null,null,null,null,null,null,null,null,"26.07.13.01","APARELHO DE ANCORAGEM ATIVO DE 4 FIOS DE Ã 5/8\" (15,2MM)","un",741.27,549.0888888888888,"DER",741270]
[null,null,null,null,null,null,null,null,null,null,"26.07.13.02","APARELHO DE ANCORAGEM ATIVO DE 12 F-5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.358,030"]
[null,null,null,null,null,null,null,null,null,null,"26.07.13.03","APARELHO DE ANCORAGEM ATIVO 15 FIOS DE Ã 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.202,050"]
[null,null,null,null,null,null,null,null,null,null,"26.07.13.04","APARELHO DE ANCORAGEM ATIVO DE 19 FIOS DE Ã 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.829,970"]
[null,null,null,null,null,null,null,null,null,null,"26.08.01","APARELHO DE APOIO NEOPRENE FRETADO","dm³",73.79,54.65925925925926,"DER",73790]
[null,null,null,null,null,null,null,null,null,null,"26.08.03","ARTICULACAO DE CONCRETO TIPO\"FREYSSINET\"","dm²",7.44,5.511111111111111,"DER",7440]
[null,null,null,null,null,null,null,null,null,null,"26.09.01","CONCRETO FCK 10MPA","m³",386.3,286.14814814814815,"DER",386300]
[null,null,null,null,null,null,null,null,null,null,"26.09.02","CONCRETO FCK 15MPA","m³",426.19,315.6962962962963,"DER",426190]
[null,null,null,null,null,null,null,null,null,null,"26.09.03","CONCRETO FCK 18MPA","m³",435.69,322.7333333333333,"DER",435690]
[null,null,null,null,null,null,null,null,null,null,"26.09.04","CONCRETO FCK 20 MPA","m³",455.28,337.2444444444444,"DER",455280]
[null,null,null,null,null,null,null,null,null,null,"26.09.05","CONCRETO FCK 25 MPA","m³",467.62,346.38518518518515,"DER",467620]
[null,null,null,null,null,null,null,null,null,null,"26.09.06","CONCRETO FCK 30MPA","m³",483.41,358.0814814814815,"DER",483410]
[null,null,null,null,null,null,null,null,null,null,"26.09.07","CONCRETO CICLOPICO","m³",390.4,289.18518518518516,"DER",390400]
[null,null,null,null,null,null,null,null,null,null,"26.09.09","BOMBEAMENTO P/ CONC. QUALQUER RESIST.","m³",42.12,31.199999999999996,"DER",42120]
[null,null,null,null,null,null,null,null,null,null,"26.09.12","CONCRETO FCK 35 MPA","m³",493.31,365.4148148148148,"DER",493310]
[null,null,null,null,null,null,null,null,null,null,"26.09.13","CONCRETO FCK 40 MPA","m³",522.21,386.82222222222225,"DER",522210]
[null,null,null,null,null,null,null,null,null,null,"26.09.14","CONCRETO FCK 45 MPA","m³",590.18,437.1703703703703,"DER",590180]
[null,null,null,null,null,null,null,null,null,null,"26.09.15","CONCRETO FCK 50 MPA","m³",609.63,451.5777777777777,"DER",609630]
[null,null,null,null,null,null,null,null,null,null,"26.10.01","JunTA/RETRACAO C/LABIO POLIM.AB.15 ATE 40 MM","m",709.74,525.7333333333333,"DER",709740]
[null,null,null,null,null,null,null,null,null,null,"26.10.02","JunTA/RETRACAO C/LABIO POLIM.AB.20 ATE 55 MM","m",940.69,696.8074074074074,"DER",940690]
[null,null,null,null,null,null,null,null,null,null,"26.10.03","JunTA/RETRACAO C/LABIO POLIM.AB. 30 ATE 80 MM","m",953.36,706.1925925925925,"DER",953360]
[null,null,null,null,null,null,null,null,null,null,"26.10.04","JunTA DE DILATACAO METALICA","m",113.84,84.32592592592593,"DER",113840]
[null,null,null,null,null,null,null,null,null,null,"26.10.05","JunTAS DE DILATACAO METALICA C/NEOPRENE","m",117.72,87.19999999999999,"DER",117720]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.10.06","FORNECIMENTO E APLICACAO DE JunTA DE DILATACAO JJ-99120 OU T-110 OU SIMILAR.","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.362,500"]
[null,null,null,null,null,null,null,null,null,null,"26.11.03.01","PLACA PRE MOLDADA DE CONCRETO PARA GUARDA CORPO PP-DE-C04/021.","un",201.23,149.05925925925925,"DER",201230]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.11.03.02","PLACA PRE MOLDADA DE CONCRETO PARA FIXACAO POSTE ILUMINACAO - PP- DE-C04/021.","un",371.53,275.20740740740735,"DER",371530]
[null,null,null,null,null,null,null,null,null,null,"26.11.03.03","LANÇAMENTO DE PLACA PRE MOLDADA DE CONCRETO, ATE 1000 KG.","un",70.65,52.333333333333336,"DER",70650]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.11.03.04","TELAMENTO METALICO PARA PASSARELA, CONFORME PP-DE-M09/001.","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.207,190"]
[null,null,null,null,null,null,null,null,null,null,"26.11.03.05","GUARDA CORPO METALICO DE PASSARELA H=0,90M, CONFORME PP-DE- C04/029.","m",781.88,579.1703703703703,"DER",781880]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.11.03.06","CORRIMAO METALICO D=2\" PARA PASSARELA, CONFORME PP-DE-K00/004.","m",162.21,120.15555555555555,"DER",162210]
[null,null,null,null,null,null,null,null,null,null,"26.11.04.01","BARREIRA DE SEGURANCA COM PASSEIO CONF. PP-DE-C01/293","m",904.11,669.7111111111111,"DER",904110]
[null,null,null,null,null,null,null,null,null,null,"26.11.04.02","BARREIRA DE SEGURANCA CONF. PP-DE-C01/293","m",440.47,326.27407407407406,"DER",440470]
[null,null,null,null,null,null,null,null,null,null,"26.11.06","BAR. DOU.FACE NEW JERSEY O.A.E.DES.5464","m",471.3,349.1111111111111,"DER",471300]
[null,null,null,null,null,null,null,null,null,null,"26.11.08.01","BARREIRA DE SEGURANçA PARA O.A.E CONF. PP-DE-C01/293","m",362.94,268.84444444444443,"DER",362940]
[null,null,null,null,null,null,null,null,null,null,"26.12.01","TUBO DE PVC PERFURADO OU NAO D=0,050M","m",20.06,14.859259259259257,"DER",20060]
[null,null,null,null,null,null,null,null,null,null,"26.12.02","TUBO DE PVC PERFURADO OU NAO D=0,075M","m",25.56,18.93333333333333,"DER",25560]
[null,null,null,null,null,null,null,null,null,null,"26.12.03","TUBO DE PVC PERFURADO OU NAO D=0,100M","m",36.29,26.88148148148148,"DER",36290]
[null,null,null,null,null,null,null,null,null,null,"26.12.04","TUBO DE PVC PERFURADO OU NAO D=0,150M","m",73.33,54.318518518518516,"DER",73330]
[null,null,null,null,null,null,null,null,null,null,"26.13.01","LANC.VIGA P<=50T-GUINDASTE AUTO P","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","7.990,520"]
[null,null,null,null,null,null,null,null,null,null,"26.13.02","LANC.VIGA 50<P<=80 T C/GUIND.AUTO P","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","8.852,890"]
[null,null,null,null,null,null,null,null,null,null,"26.14.01","ESGOTAMENTO CONTINUO AGUA","m³",2.02,1.4962962962962962,"DER",2020]
[null,null,null,null,null,null,null,null,null,null,"26.14.02","ESCORAMENTO VALAS/CAVAS P/FunD.CONTINUO","m²",96,71.1111111111111,"DER",96000]
[null,null,null,null,null,null,null,null,null,null,"26.14.03","PAREDE ENSECADEIRA C/PRANCHA-ESP.0,050M","m²",199.49,147.77037037037036,"DER",199490]
[null,null,null,null,null,null,null,null,null,null,"26.14.04","PAREDE ENSECADEIRA C/PRANCHA-ESP.0,075M","m²",280.41,207.7111111111111,"DER",280410]
[null,null,null,null,null,null,null,null,null,null,"26.15.01","ENROCAMENTO PEDRA ARRUMADA","m³",210.83,156.17037037037036,"DER",210830]
[null,null,null,null,null,null,null,null,null,null,"26.15.02","ENROCAMENTO PEDRA ARRUMADA E REJunTADA","m³",324.57,240.4222222222222,"DER",324570]
[null,null,null,null,null,null,null,null,null,null,"26.15.03","ENROCAMENTO PEDRA JOGADA","m³",136.02,100.75555555555556,"DER",136020]
[null,null,null,null,null,null,null,null,null,null,"26.16.01","PROTECAO DE TALUDE COM BLOCO PRE-MOLDADO SEXTAVADO 30X30X5CM INTERTRAVADO.","m²",115.31,85.4148148148148,"DER",115310]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.16.02","PROTECAO TALUDE SOB OAE EM PLACAS PRE MOLDADAS TRAPEZOIDAL, 98X80X40CM.","m²",326.63,241.94814814814814,"DER",326630]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"26.16.03","PROTECAO TALUDE SOB OAE COM PECAS PRE-MOLDADAS RETANGULAR 20X10X6CM.","m²",100.88,74.72592592592592,"DER",100880]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.01.01","REMOCAO MANUAL DE CONCRETO SEGREGADO","dm³",22.76,16.85925925925926,"DER",22760]
[null,null,null,null,null,null,null,null,null,null,"27.01.02","DEMOLICAO DE CONCRETO SIMPLES","m³",158.86,117.67407407407407,"DER",158860]
[null,null,null,null,null,null,null,null,null,null,"27.01.03","DEMOLICAO DE CONCRETO ARMADO","m³",298.95,221.44444444444443,"DER",298950]
[null,null,null,null,null,null,null,null,null,null,"27.01.04","REMOCAO,CARGA E TRANSP.ENTULHO EM GERAL","t*km",1.24,0.9185185185185184,"DER",1240]
[null,null,null,null,null,null,null,null,null,null,"27.01.29","LIXAMENTO MECÂNICO DE SUPERFÍCIO DE CONCRETO","m²",15.43,11.429629629629629,"DER",15430]
[null,null,null,null,null,null,null,null,null,null,"27.01.40","TRATAMENTO DE ARMADURA COM PRIMER RICO EM ZINCO","m²",18.82,13.94074074074074,"DER",18820]
[null,null,null,null,null,null,null,null,null,null,"27.02.01","APIC.MANUAL CONC.C/ELIMINACAO SUP.LISAS","m²",40.96,30.34074074074074,"DER",40960]
[null,null,null,null,null,null,null,null,null,null,"27.02.02","LIMPEZA COM JATO D´AGUA S/SUP.DE CONC.","m²",3.99,2.9555555555555557,"DER",3990]
[null,null,null,null,null,null,null,null,null,null,"27.02.03","LIXAMENTO MANUAL DA SUPERFICIE DE CONCR.","m²",6.83,5.059259259259259,"DER",6830]
[null,null,null,null,null,null,null,null,null,null,"27.02.05","JATEAMENTO EM ESTR.CONCRETO COM AGUA","m²",4.78,3.5407407407407407,"DER",4780]
[null,null,null,null,null,null,null,null,null,null,"27.02.08","LIMPEZA MANUAL COM ESCOVA DE ACO P/ ACO","m",5.31,3.9333333333333327,"DER",5310]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.02.09","LIMPEZA MANUAL C/ESCOVA ACO P/CONCRETO","m²",7.21,5.34074074074074,"DER",7210]
[null,null,null,null,null,null,null,null,null,null,"27.03.01","ANDAIME DE MADEIRA","m³",12.63,9.355555555555556,"DER",12630]
[null,null,null,null,null,null,null,null,null,null,"27.03.02","ANDAIME TUBULAR","m³",18.12,13.422222222222222,"DER",18120]
[null,null,null,null,null,null,null,null,null,null,"27.03.03.01","EXECUCAO DE ANDAIME SUSPENSO AREA MAXIMA DE 560 m².","m²",48.83,36.170370370370364,"DER",48830]
[null,null,null,null,null,null,null,null,null,null,"27.03.03.02","DESMOB. DESLOCAMENTO, MONTAGEM E FURO NO CONCRETO PARA ANDAIME SUSPENSO.","m²",44.59,33.02962962962963,"DER",44590]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.04.01","FURO NO CONCRETO D=1\" PROFunD.DE 5CM","un",8.01,5.933333333333333,"DER",8010]
[null,null,null,null,null,null,null,null,null,null,"27.04.02","FURO NO CONCRETO D=1\" PROFunD.DE 15CM","un",20.04,14.844444444444443,"DER",20040]
[null,null,null,null,null,null,null,null,null,null,"27.04.03","FURO NO CONCRETO D=1\" PROFunD. DE 30CM","un",40.06,29.674074074074074,"DER",40060]
[null,null,null,null,null,null,null,null,null,null,"27.04.04","FURO NO CONCRETO D=3/4\" PROFunD.DE 5CM","un",6.59,4.881481481481481,"DER",6590]
[null,null,null,null,null,null,null,null,null,null,"27.04.05","FURO NO CONCRETO D=3/4\" PROFunD.DE 15CM","un",16.47,12.199999999999998,"DER",16470]
[null,null,null,null,null,null,null,null,null,null,"27.04.06","FURO NO CONCRETO D=3/4\" PROFunD.DE 30CM","un",32.93,24.392592592592592,"DER",32930]
[null,null,null,null,null,null,null,null,null,null,"27.04.07","FURO NO CONCRETO D=1/2\" PROFunD.DE 5CM","un",5.34,3.9555555555555553,"DER",5340]
[null,null,null,null,null,null,null,null,null,null,"27.04.08","FURO NO CONCRETO D=1/2\" PROFunD.DE 15CM","un",13.35,9.888888888888888,"DER",13350]
[null,null,null,null,null,null,null,null,null,null,"27.04.09","FURO NO CONCRETO D=1/2\" PROFunD.DE 30CM","un",26.71,19.785185185185185,"DER",26710]
[null,null,null,null,null,null,null,null,null,null,"27.04.10","FURO NO CONCRETO D=3/8\" PROFunD.DE 5CM","un",3.92,2.9037037037037035,"DER",3920]
[null,null,null,null,null,null,null,null,null,null,"27.04.11","FURO NO CONCRETO D=3/8\" PROFunD.DE 15CM","un",9.8,7.2592592592592595,"DER",9800]
[null,null,null,null,null,null,null,null,null,null,"27.04.12","FURO NO CONCRETO D=3/8\" PROFunD.DE 30CM","un",19.58,14.503703703703701,"DER",19580]
[null,null,null,null,null,null,null,null,null,null,"27.05.01","FORMA PLANA P/CONC.ARMADO COMUM","m²",80.07,59.3111111111111,"DER",80070]
[null,null,null,null,null,null,null,null,null,null,"27.05.02","FORMA PLANA P/CONC.PROTEND.OU APARENTE","m²",90.3,66.88888888888889,"DER",90300]
[null,null,null,null,null,null,null,null,null,null,"27.05.03","FORMAS METALICAS PARA CONCRETO","m²",60.61,44.89629629629629,"DER",60610]
[null,null,null,null,null,null,null,null,null,null,"27.06.01","BARRA DE ACO CA-25","kg",8.78,6.503703703703703,"DER",8780]
[null,null,null,null,null,null,null,null,null,null,"27.06.02","BARRA DE ACO CA-50 PARA RECUPERACAO ESTRUTURAL","kg",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"27.06.03","BARRA DE ACO CA-60","kg",9.2,6.814814814814814,"DER",9200]
[null,null,null,null,null,null,null,null,null,null,"27.06.04","ACO PARA CONCRETO PROTENDIDO","kg",19.14,14.177777777777777,"DER",19140]
[null,null,null,null,null,null,null,null,null,null,"27.06.05","TELA METALICA","kg",7.38,5.466666666666666,"DER",7380]
[null,null,null,null,null,null,null,null,null,null,"27.06.06","SUBSTITUICAO DE ACO DA ARMADURA","kg",18.02,13.348148148148146,"DER",18020]
[null,null,null,null,null,null,null,null,null,null,"27.06.07","RETIRADA DA ARMADURA CORROIDA","kg",7.13,5.281481481481481,"DER",7130]
[null,null,null,null,null,null,null,null,null,null,"27.06.08","ACO P/ CONCRETO PROTENDIDO ST 85/105","kg",29.82,22.08888888888889,"DER",29820]
[null,null,null,null,null,null,null,null,null,null,"27.06.09","EMENDA DE BARRA DE ACO COM LUVA PRENSADA D=12MM","un",31.97,23.68148148148148,"DER",31970]
[null,null,null,null,null,null,null,null,null,null,"27.06.10","EMENDA DE BARRA DE ACO COM LUVA PRENSADA D=16MM","un",37.31,27.637037037037036,"DER",37310]
[null,null,null,null,null,null,null,null,null,null,"27.06.11","EMENDA DE BARRA DE ACO COM LUVA PRENSADA D=20MM","un",48.3,35.77777777777777,"DER",48300]
[null,null,null,null,null,null,null,null,null,null,"27.06.12","EMENDA DE BARRA DE ACO COM LUVA PRENSADA D=25MM","un",73.54,54.474074074074075,"DER",73540]
[null,null,null,null,null,null,null,null,null,null,"27.06.13","EMENDA DE BARRA DE ACO COM ROSCA D=12MM","un",33.76,25.007407407407403,"DER",33760]
[null,null,null,null,null,null,null,null,null,null,"27.06.14","EMENDA DE BARRA DE ACO COM ROSCA D=16MM","un",46.39,34.36296296296296,"DER",46390]
[null,null,null,null,null,null,null,null,null,null,"27.06.15","EMENDA DE BARRA DE ACO COM ROSCA D=20MM","un",64.1,47.481481481481474,"DER",64100]
[null,null,null,null,null,null,null,null,null,null,"27.06.16","EMENDA DE BARRA DE ACO COM ROSCA D=25MM","un",97.23,72.02222222222223,"DER",97230]
[null,null,null,null,null,null,null,null,null,null,"27.06.17","CHUMBAMENTO BARRAS C/RESINA EPOX.INJ.","kg",42.86,31.748148148148147,"DER",42860]
[null,null,null,null,null,null,null,null,null,null,"27.07.02","AP.ANC.P/CABOS PROTEN. ATIVA 12FIOS-8MM","un",689.95,511.0740740740741,"DER",689950]
[null,null,null,null,null,null,null,null,null,null,"27.07.03","AP.ANC.P/CABOS PROTEN.ATIV.04FIOS-12,7MM","un",553.32,409.8666666666667,"DER",553320]
[null,null,null,null,null,null,null,null,null,null,"27.07.04","AP.ANC.P/CABOS PROTEN.ATIV. 6FIOS-12,7MM","un",766.88,568.0592592592592,"DER",766880]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.07.05","AP.ANC.P/CABOS PROTEN.ATIV.12FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.580,840"]
[null,null,null,null,null,null,null,null,null,null,"27.07.06","AP.ANC.P/CABOS PROTEN.ATIV.19FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.609,960"]
[null,null,null,null,null,null,null,null,null,null,"27.07.07","AP.ANC.P/CABOS PROTEN.ATIV.22FIOS-12,7MM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.339,470"]
[null,null,null,null,null,null,null,null,null,null,"27.07.09","AP.ANC.P/CABOS PROTEN.PASS. 4FIOS-12,7MM","un",108.01,80.0074074074074,"DER",108010]
[null,null,null,null,null,null,null,null,null,null,"27.07.10","AP.ANC.P/CABOS PROTEN.PASS. 6FIOS-12,7MM","un",148.07,109.68148148148147,"DER",148070]
[null,null,null,null,null,null,null,null,null,null,"27.07.12","AP.ANC.P/CABOS PROTEN.PAS. 19FIOS-12,7MM","un",972.92,720.6814814814815,"DER",972920]
[null,null,null,null,null,null,null,null,null,null,"27.07.13.01","APARELHO DE ANCORAGEM ATIVO DE 4 FIOS DE Ã 5/8\" (15,2MM)","un",741.27,549.0888888888888,"DER",741270]
[null,null,null,null,null,null,null,null,null,null,"27.07.13.02","APARELHO DE ANCORAGEM ATIVO DE 12 FIOS DE 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.358,030"]
[null,null,null,null,null,null,null,null,null,null,"27.07.13.03","APARELHO DE ANCORAGEM ATIVO DE 15 FIOS DE Ã 5/8\" (15,2MM)","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.202,050"]
[null,null,null,null,null,null,null,null,null,null,"27.07.13.04","APARELHO DE ANCORAGEM ATIVO DE 19 FIOS DE Ã 5/8\"","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.829,970"]
[null,null,null,null,null,null,null,null,null,null,"27.08.01","SUBSTIT.APARELHO APOIO NEOPRENE FRETADO","dm³",127.93,94.76296296296296,"DER",127930]
[null,null,null,null,null,null,null,null,null,null,"27.09.01","CONCRETO FCK 10MPA","m³",386.3,286.14814814814815,"DER",386300]
[null,null,null,null,null,null,null,null,null,null,"27.09.02","CONCRETO FCK 15MPA","m³",426.19,315.6962962962963,"DER",426190]
[null,null,null,null,null,null,null,null,null,null,"27.09.03","CONCRETO FCK 18MPA","m³",435.69,322.7333333333333,"DER",435690]
[null,null,null,null,null,null,null,null,null,null,"27.09.04","CONCRETO FCK 20MPA","m³",455.28,337.2444444444444,"DER",455280]
[null,null,null,null,null,null,null,null,null,null,"27.09.05","CONCRETO FCK 25MPA","m³",467.63,346.39259259259256,"DER",467630]
[null,null,null,null,null,null,null,null,null,null,"27.09.07","CONCRETO FCK 30MPA","m³",483.41,358.0814814814815,"DER",483410]
[null,null,null,null,null,null,null,null,null,null,"27.09.08","CONCRETO CICLOPICO","m³",390.4,289.18518518518516,"DER",390400]
[null,null,null,null,null,null,null,null,null,null,"27.09.09","CONCRETO PROJETADO,MEDIDO NA SECAO","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.241,410"]
[null,null,null,null,null,null,null,null,null,null,"27.09.10","BOMBEAMENTO P/CONC. QUALQUER RESIST.","m³",42.12,31.199999999999996,"DER",42120]
[null,null,null,null,null,null,null,null,null,null,"27.09.11","CONCRETO GROUT ALTA RESISTENCIA","dm³",11.65,8.62962962962963,"DER",11650]
[null,null,null,null,null,null,null,null,null,null,"27.09.12","ENCHIMENTO COM CONCRETO CELULAR","m³",672.43,498.0962962962962,"DER",672430]
[null,null,null,null,null,null,null,null,null,null,"27.09.15","CONCRETO FCK 35MPA","m³",493.31,365.4148148148148,"DER",493310]
[null,null,null,null,null,null,null,null,null,null,"27.09.16","CONCRETO FCK 40MPA","m³",522.21,386.82222222222225,"DER",522210]
[null,null,null,null,null,null,null,null,null,null,"27.09.17","CONCRETO FCK 45 MPA","m³",590.18,437.1703703703703,"DER",590180]
[null,null,null,null,null,null,null,null,null,null,"27.09.18","CONCRETO FCK 50 MPA","m³",609.64,451.58518518518514,"DER",609640]
[null,null,null,null,null,null,null,null,null,null,"27.10.01","JunTA/RETRACAO C/LABIO POLI.AB.15ATE40MM","m",748.66,554.562962962963,"DER",748660]
[null,null,null,null,null,null,null,null,null,null,"27.10.02","JunTA/RETRACAO C/LABIO POLI.AB.20ATE55MM","m",979.62,725.6444444444444,"DER",979620]
[null,null,null,null,null,null,null,null,null,null,"27.10.03","JunTA/RETRACAO C/LABIO POLI.AB.30ATE80MM","m",992.28,735.0222222222221,"DER",992280]
[null,null,null,null,null,null,null,null,null,null,"27.10.04","SUBSTITUICAO DE JunTA METALICA","m",200.63,148.6148148148148,"DER",200630]
[null,null,null,null,null,null,null,null,null,null,"27.10.05","MICROCONCRETO RAPFLEX 10","m",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.116,710"]
[null,null,null,null,null,null,null,null,null,null,"27.11.01","ARGAMASSA CIMENTO E AREIA 1:1","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.545,130"]
[null,null,null,null,null,null,null,null,null,null,"27.11.02","ADESIVO EPOXI P/TRI.(INCL.FUROS E MANG.)","kg",199.6,147.85185185185185,"DER",199600]
[null,null,null,null,null,null,null,null,null,null,"27.11.03","INJECAO DE CALDA DE CIMENTO","kg",2.64,1.9555555555555555,"DER",2640]
[null,null,null,null,null,null,null,null,null,null,"27.11.05","INJECAO DE CALDA DE CIMENTO EM BAINHAS","kg",2.64,1.9555555555555555,"DER",2640]
[null,null,null,null,null,null,null,null,null,null,"27.11.09","ARGAMASSA DE CIMENTO E AREIA TRACO 1:6","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.585,810"]
[null,null,null,null,null,null,null,null,null,null,"27.11.10","ARGAMASSA CIMEN.E AREIA TRAC.1:3 ESP 2CM","m²",34.41,25.488888888888884,"DER",34410]
[null,null,null,null,null,null,null,null,null,null,"27.12.01","TUBO DE PVC PERFURADO OU NAO D=0,050M","m",20.06,14.859259259259257,"DER",20060]
[null,null,null,null,null,null,null,null,null,null,"27.12.02","TUBO DE PVC PERFURADO OU NAO D=0,075M","m",25.56,18.93333333333333,"DER",25560]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.12.03","TUBO DE PVC PERFURADO OU NAO D=0,10M","m",36.29,26.88148148148148,"DER",36290]
[null,null,null,null,null,null,null,null,null,null,"27.12.04","TUBO DE PVC PERFURADO OU NAO D=0,15M","m",73.33,54.318518518518516,"DER",73330]
[null,null,null,null,null,null,null,null,null,null,"27.13.02","ADITIVO SUPER PLASTIFICANTE","kg",7.52,5.5703703703703695,"DER",7520]
[null,null,null,null,null,null,null,null,null,null,"27.13.03","ADITIVO SUPER FLUIDIFICANTE","kg",4.94,3.6592592592592594,"DER",4940]
[null,null,null,null,null,null,null,null,null,null,"27.13.04","ADITIVO ACELERADOR DE PEGA","kg",3.79,2.8074074074074074,"DER",3790]
[null,null,null,null,null,null,null,null,null,null,"27.13.05","ADITIVO RETARDADOR DE PEGA","kg",6.02,4.459259259259259,"DER",6020]
[null,null,null,null,null,null,null,null,null,null,"27.14.01.01","PINTURA HIDROFUGANTE C/SILICONE BASE AGUA - UMA DEMAO","m²",11.39,8.437037037037037,"DER",11390]
[null,null,null,null,null,null,null,null,null,null,"27.14.02","PINT.C/VERNIZ POLIURETANO INCOLOR-3DEMAO","m²",47.63,35.28148148148148,"DER",47630]
[null,null,null,null,null,null,null,null,null,null,"27.14.03","PINTURA A BASE DE EPOXI - 2DEMAOS","m²",44.85,33.22222222222222,"DER",44850]
[null,null,null,null,null,null,null,null,null,null,"27.14.04","PINTURA ACRILICA - 2DEMAOS","m²",29.18,21.614814814814814,"DER",29180]
[null,null,null,null,null,null,null,null,null,null,"27.14.05","PINTURA A BASE DE ESMALTE SINTETICO 3 DEMAOS, SENDO UMA DEMAO FunDO OXIDO FERRO","m²",39.06,28.933333333333334,"DER",39060]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.16.01","APLICACAO MANUAL E PREPARO DE PASTA PARA ESTUCAMENTO EM OAE, SEM PINTURA.","m²",13.93,10.318518518518518,"DER",13930]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"27.18.01","ATERRO SOLO COM 3% DE CIMENTO C/PULVE.","m³",47.85,35.44444444444444,"DER",47850]
[null,null,null,null,null,null,null,null,null,null,"28.01.04.01","FORN. E TRANSPORTE DE PLACA DE ACO GT+GT","m²",710.78,526.5037037037036,"DER",710780]
[null,null,null,null,null,null,null,null,null,null,"28.01.05.01","FORN. E TRANSPORTE DE PLACA DE ACO GT+AI","m²",897.06,664.4888888888888,"DER",897060]
[null,null,null,null,null,null,null,null,null,null,"28.01.07.01","FORN. E TRANSPORTE DE PLACA MOD.ALUMINIO GT+GT","m²",972.46,720.3407407407407,"DER",972460]
[null,null,null,null,null,null,null,null,null,null,"28.01.08.01","FORN. E TRANSPORTE DE PLACA DE ALUMINIO GT+AI","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.143,180"]
[null,null,null,null,null,null,null,null,null,null,"28.01.09","FORN.E INSTAL.PLACA ALUM. AI+GD","m²",968.64,717.5111111111111,"DER",968640]
[null,null,null,null,null,null,null,null,null,null,"28.01.20.01","PLACA EM CHAPA DE POLIESTER COM FIBRA DE VIDRO GT+GT SIMPLES","m²",501.26,371.30370370370366,"DER",501260]
[null,null,null,null,null,null,null,null,null,null,"28.01.20.02","PLACA EM CHAPA DE POLIESTER COM FIBRA DE VIDRO GT+AI SIMPLES","m²",585.9,433.99999999999994,"DER",585900]
[null,null,null,null,null,null,null,null,null,null,"28.01.24.01","COLOCACAO DE PLACA EM SUP. MADEIRA/METALICO-SOLO","m²",44.06,32.63703703703704,"DER",44060]
[null,null,null,null,null,null,null,null,null,null,"28.01.25.01","COLOCACAO DE PLACA AEREA EM PORTICOS OU SEMI-PORTICO","m²",63.03,46.68888888888889,"DER",63030]
[null,null,null,null,null,null,null,null,null,null,"28.01.26.01","RETIRADA DE PLACA DE SOLO EM SUPORTE DE MADEIRA OU METALICO","m²",37.77,27.977777777777778,"DER",37770]
[null,null,null,null,null,null,null,null,null,null,"28.01.27.01","RETIRADA DE PLACA AEREA","m²",50.42,37.34814814814815,"DER",50420]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.01.28","FORN.TRANSP.INSTAL.PLC CHAPA DE LAMINADO FENOL MELAM. C/ACAB. GTP+GTP,MOD.AçO","m²",536.29,397.2518518518518,"DER",536290]
[null,null,null,null,null,null,null,null,null,null,"28.01.29","FORNECIMENTO, TRANSPORTE E INSTALACAO DE PLACA DE AÇO AI+GD","m²",863.76,639.8222222222222,"DER",863760]
[null,null,null,null,null,null,null,null,null,null,"28.02.01.01","FORN.,TRANSP.E FIXACAO DE PORTICO TUB.MET.VAO DE 15,20M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","38.060,160"]
[null,null,null,null,null,null,null,null,null,null,"28.02.02.01","FORN., TRANSP. E FIXACAO DE PORTICO TUB. MET. VAO DE 18,80M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","48.895,950"]
[null,null,null,null,null,null,null,null,null,null,"28.02.03.01","FORN., TRANSP. E FIXACAO DE PORTICO TUB. MET. COM VAO DE 22,40M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","52.618,190"]
[null,null,null,null,null,null,null,null,null,null,"28.02.04.01","FORN., TRANSP. E FIX. DE SEMI-PORT TUB. EM BALANCO VAO DE 5,10M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","17.001,170"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.02.05.01","FORN., TRANSP. E FIX. DE SEMI-PORT TUB. EM BALANCO VAO DE 8,60M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","23.323,920"]
[null,null,null,null,null,null,null,null,null,null,"28.02.06.01","FORN., TRANSP. E FIX. DE SEMI-PORT TUB. EM BALANCO DUPLO 5,10M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","24.166,960"]
[null,null,null,null,null,null,null,null,null,null,"28.02.07.01","FORN., TRANSP. E FIX. DE SEMI-PORT TUB. EM BALANCO DUPLO 8,60M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","37.690,920"]
[null,null,null,null,null,null,null,null,null,null,"28.03.02","SINALIZ.HOR.C/RESINA VINILICA OU ACRILI.","m²",21.01,15.562962962962963,"DER",21010]
[null,null,null,null,null,null,null,null,null,null,"28.03.03","SINALIZ.HOR. C/TERMOPLAST. HOT-SPRAY","m²",44.48,32.94814814814814,"DER",44480]
[null,null,null,null,null,null,null,null,null,null,"28.03.04","SINALIZ.HOR. C/TERMOPLAST.SPRAY-C/VISIB.","m²",51.84,38.4,"DER",51840]
[null,null,null,null,null,null,null,null,null,null,"28.03.05","SINALIZ.HOR.C/TERMOPLAST EXTRUDADO","m²",47.74,35.36296296296296,"DER",47740]
[null,null,null,null,null,null,null,null,null,null,"28.03.05.03","SIN.HORIZ.PLAST.A FRIO,POR EXTRUSAO, ALTO RELEVO, ESPACAMENTO 500MM.","m²",149.3,110.5925925925926,"DER",149300]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.03.05.04","SINAL.HORIZ.PLAST.FRIO BASE DE RES. METACRIL. REATIVAS, DISP.ESTRUT.APLIC. MEC.","m²",106.67,79.01481481481481,"DER",106670]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.03.06","SINALIZ.HOR.TINTA P/ POUCO TRAFEGO","m²",15.19,11.251851851851852,"DER",15190]
[null,null,null,null,null,null,null,null,null,null,"28.03.07","SINALIZ.HOR.ACRILICA BASE AGUA","m²",18.72,13.866666666666665,"DER",18720]
[null,null,null,null,null,null,null,null,null,null,"28.03.08","SINALIZ.HOR. ACRILICA BASE AGUA C/VISIB.","m²",22.86,16.933333333333334,"DER",22860]
[null,null,null,null,null,null,null,null,null,null,"28.03.09.02","TACHA REFLETIVA BIDIRECIONAL TIPO III OU IV ABNT (VIDRO OU PRISMÁTICO)","un",30.35,22.48148148148148,"DER",30350]
[null,null,null,null,null,null,null,null,null,null,"28.03.10","MINI TACHAO MONODIRECIONAL REFL. VIDRO","un",43.08,31.911111111111108,"DER",43080]
[null,null,null,null,null,null,null,null,null,null,"28.03.10.01","MINI TACHAO BIDIRECIONAL REFL. VIDRO","un",44.85,33.22222222222222,"DER",44850]
[null,null,null,null,null,null,null,null,null,null,"28.03.11","TACHAO MONODIRECIONAL REFLETIVO DE VIDRO","un",45.79,33.91851851851852,"DER",45790]
[null,null,null,null,null,null,null,null,null,null,"28.03.12","TACHAO BIDIRECIONAL REFLETIVO DE VIDRO","un",52.8,39.11111111111111,"DER",52800]
[null,null,null,null,null,null,null,null,null,null,"28.03.13","TACHA MONODIRECIONAL REFLETIVO PLASTICO","un",14.23,10.540740740740741,"DER",14230]
[null,null,null,null,null,null,null,null,null,null,"28.03.14","TACHA BIDIRECIONAL REFLETIVO PLASTICO","un",15.92,11.792592592592591,"DER",15920]
[null,null,null,null,null,null,null,null,null,null,"28.03.15.01","TACHA REFLETIVA MONODIRECIONAL TIPO III OU IV ABNT (VIDRO OU PRISMÁTICO)","un",24.88,18.429629629629627,"DER",24880]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.04.18","FORN. E INSTAL. DE BALIZADOR LAT. DE SOLO BIREFLETIVO AI","un",154.04,114.10370370370369,"DER",154040]
[null,null,null,null,null,null,null,null,null,null,"28.05.01","DEFENSA-MALEAVEL SIMPLES","m",289.2,214.2222222222222,"DER",289200]
[null,null,null,null,null,null,null,null,null,null,"28.05.02","DEFENSA-MALEAVEL DUPLO","m",362.39,268.437037037037,"DER",362390]
[null,null,null,null,null,null,null,null,null,null,"28.05.03","DEFENSA-MALEAVEL SIMPLES-IMPLANTACAO","m",48.99,36.28888888888889,"DER",48990]
[null,null,null,null,null,null,null,null,null,null,"28.05.04","DEFENSA-MALEAVEL DUPLO-IMPLANTACAO","m",65.31,48.37777777777777,"DER",65310]
[null,null,null,null,null,null,null,null,null,null,"28.05.05","DEFENSA SEMI_MALEAVEL SIMPLES_FORNECIMEN","m",198,146.66666666666666,"DER",198000]
[null,null,null,null,null,null,null,null,null,null,"28.05.06","DEFENSA SEMI-MALEAVEL SIMPLES-INSTALACAO","m",32.27,23.903703703703705,"DER",32270]
[null,null,null,null,null,null,null,null,null,null,"28.05.08","FORNEC.TRANSP.MONT.INSTAL. TERMINAL ATERNUADOR DE IMPACTO NÃO DIRECIONAVEL","conjunto",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","12.825,000"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.05.09","FORN.INST.MODULO DE TRANSICAO DE DEF.METALICA P/BAR.CONCRETO C/DEF.MET.TRIPLA","conjunto",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","8.100,000"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.06.02","G.C.INTRANSPONIVEL TIPO II - DES.5307","m",501.69,371.6222222222222,"DER",501690]
[null,null,null,null,null,null,null,null,null,null,"28.06.03","G.C.DE CONC.PRE-PASSARELA-DES.5370","m",311.93,231.05925925925925,"DER",311930]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.06.03.01","GUARDA CORPO DE CONCRETO P/ PASSARELA - DES. PP-C04/812 (DERSA)","m",402.82,298.38518518518515,"DER",402820]
[null,null,null,null,null,null,null,null,null,null,"28.06.04.01","BARREIRA DE SEGURANCA COM PASSEIO CONF. PP-DE-CO1/293","m",904.11,669.7111111111111,"DER",904110]
[null,null,null,null,null,null,null,null,null,null,"28.06.04.02","BARREIRA DE SEGURANCA CONF. PP-DE-C01/293","m",440.47,326.27407407407406,"DER",440470]
[null,null,null,null,null,null,null,null,null,null,"28.06.06","BAR.DOUBLE FACE NEW J. O.A.E. DES.5464","m",471.3,349.1111111111111,"DER",471300]
[null,null,null,null,null,null,null,null,null,null,"28.06.08.01","BARREIRA DE SEGURANCA PARA O.A.E CONF. PP-DE-C01/293","m",362.94,268.84444444444443,"DER",362940]
[null,null,null,null,null,null,null,null,null,null,"28.06.10","SUPORTE MADEIRA TRATADA 0,10X0,10M","m",74.29,55.02962962962963,"DER",74290]
[null,null,null,null,null,null,null,null,null,null,"28.06.10.01","RETIRADA DE SUPORTE DE MADEIRA TRATADA","m",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"28.06.11","SUPORTE DE PERFIL METALICO GALVANIZADO.","kg",18.7,13.851851851851851,"DER",18700]
[null,null,null,null,null,null,null,null,null,null,"28.06.12","SUPORTE TUBULAR GALVANIZADO 2 1/2\"","m",81.51,60.37777777777778,"DER",81510]
[null,null,null,null,null,null,null,null,null,null,"28.06.13.01","BARREIRA RIGIDA MOLD. IN LOCO (DUPLA FACE)-EXTRUDADA-DES.PP-CO5/003- 5564A","m",237.07,175.60740740740738,"DER",237070]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.06.17","BARREIRA RIGIDA DE CONCRETO ARMADO SIMPLES BAIXA NBR 14.885","m",229.46,169.97037037037038,"DER",229460]
[null,null,null,null,null,null,null,null,null,null,"28.06.18","BARREIRA RIGIDA DE CONCRETO ARMADO SIMPLES ALTA NBR 14.885","m",301.74,223.5111111111111,"DER",301740]
[null,null,null,null,null,null,null,null,null,null,"28.06.19","BARREIRA RIGIDA DE CONCRETO ARMADO DUPLA BAIXA NBR 14.885","m",268.72,199.05185185185186,"DER",268720]
[null,null,null,null,null,null,null,null,null,null,"28.06.20","BARREIRA RIGIDA DE CONCRETO ARMADO DUPLA ALTA NBR 14.885","m",405.86,300.63703703703703,"DER",405860]
[null,null,null,null,null,null,null,null,null,null,"28.06.21","BARREIRA RIGIDA DE CONCRETO ARMADO DUPLA ASSIMETRICA NBR 14.885","m",390.41,289.1925925925926,"DER",390410]
[null,null,null,null,null,null,null,null,null,null,"28.06.23","TERMINAIS DEFLEXAO - BARREIRA SIMPLES BAIXA - OP-06-26","un",496.24,367.5851851851852,"DER",496240]
[null,null,null,null,null,null,null,null,null,null,"28.06.24","TERMINAIS DEFLEXAO - BARREIRA SIMPLES ALTA - OP-06-26","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.062,250"]
[null,null,null,null,null,null,null,null,null,null,"28.06.25","TERMINAIS RETO - BARREIRA SIMPLES BAIXA - OP-06-26","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.486,390"]
[null,null,null,null,null,null,null,null,null,null,"28.06.26","TERMINAIS RETO - BARREIRA SIMPLES ALTA - OP-06-26","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.001,530"]
[null,null,null,null,null,null,null,null,null,null,"28.06.27","TERMINAIS RETO - BARREIRA DUPLA BAIXA - OP-06-26","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.812,950"]
[null,null,null,null,null,null,null,null,null,null,"28.06.28","TERMINAIS RETO - BARREIRA DUPLA ALTA - OP-06-26","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.412,790"]
[null,null,null,null,null,null,null,null,null,null,"28.06.30","SUPORTE DE PLACAS DE SOLO ECOLOGICO E COLAPSIVEL 75X75MM.","m",80.24,59.43703703703703,"DER",80240]
[null,null,null,null,null,null,null,null,null,null,"28.07.01","BROCA DE CONCRETO ARMADO D=20,00CM","m",48.28,35.76296296296296,"DER",48280]
[null,null,null,null,null,null,null,null,null,null,"28.07.02","BROCA DE CONCRETO ARMADO, D=25,00CM","m",74.6,55.25925925925925,"DER",74600]
[null,null,null,null,null,null,null,null,null,null,"28.07.03","BROCA DE CONCRETO ARMADO D=15,00CM","m",27.61,20.45185185185185,"DER",27610]
[null,null,null,null,null,null,null,null,null,null,"28.07.06","BROCA DE CONTRETO ARMADO D=30CM","m",90.68,67.17037037037038,"DER",90680]
[null,null,null,null,null,null,null,null,null,null,"28.08.01.01","CONFECCAO, MONTAGEM E INSTALACAO DE PLACA INSTITUCIONAL","m²",166.87,123.60740740740741,"DER",166870]
[null,null,null,null,null,null,null,null,null,null,"28.08.02.01","MANUTENCAO DE PLACA INSTITUCIONAL","m² x mes",36.26,26.859259259259257,"DER",36260]
[null,null,null,null,null,null,null,null,null,null,"28.09.01","REMOCAO DE PINTURA ACRILIC. DEMARC. DE VIA POR PROCESSO MANUAL","m²",50.87,37.68148148148148,"DER",50870]
[null,null,null,null,null,null,null,null,null,null,"28.09.02","REMOCAO DE PINTURA TERMOPL. DEMARC. DE VIA - GRANALHA DE ACO","m²",75.79,56.14074074074074,"DER",75790]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.10.01","FORN./INSTAL. BALIZ.(CATADIOPTRICO) P/DEF. MET. C/PELICULA GT+GT, CONF.OP-06-05","un",25.89,19.177777777777777,"DER",25890]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.10.02","FORN./INSTAL. BALIZ. (CATADIOPTRICO) P/BAR. RIGIDA C/PEL. GT+GT, CONF. OP-06-05","un",26.51,19.637037037037036,"DER",26510]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"28.12.01","PINTURA ANTI PICHACAO A BASE DE AGUA PARA PLACA DE SINALIZACAO","m²",47.34,35.06666666666667,"DER",47340]
[null,null,null,null,null,null,null,null,null,null,"28.12.02","PINTURA ANTI-PICHACAO A BASE DE AGUA PARA CONCRETO APARENTE","m²",72.88,53.98518518518518,"DER",72880]
[null,null,null,null,null,null,null,null,null,null,"30.01.01","GRAMA EM PLACA SEM ADUBO","m²",6.56,4.859259259259258,"DER",6560]
[null,null,null,null,null,null,null,null,null,null,"30.01.02","GRAMA PLACA COM ADUBO","m²",7.34,5.437037037037037,"DER",7340]
[null,null,null,null,null,null,null,null,null,null,"30.01.03","GRAMA MUDA SEM ADUBO","m²",5.85,4.333333333333333,"DER",5850]
[null,null,null,null,null,null,null,null,null,null,"30.01.04","GRAMA MUDA COM ADUBO","m²",6.46,4.785185185185185,"DER",6460]
[null,null,null,null,null,null,null,null,null,null,"30.01.05","PLANTIO LEGUM.SEMENTES SEM ADUBO","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,750"]
[null,null,null,null,null,null,null,null,null,null,"30.01.06","PLANTIO LEGUM.SEMENTES COM ADUBO","m²",1.45,1.074074074074074,"DER",1450]
[null,null,null,null,null,null,null,null,null,null,"30.01.07","PLANTIO DE GRAMA PROC.HIDROSSEMEADURA","m²",5.3,3.9259259259259256,"DER",5300]
[null,null,null,null,null,null,null,null,null,null,"30.01.08","IRRIGACAO DE REVESTIMENTO VEGETAL","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,190"]
[null,null,null,null,null,null,null,null,null,null,"30.01.09","GRAMA ARMADA TELA VEGETAL","m²",21.22,15.718518518518517,"DER",21220]
[null,null,null,null,null,null,null,null,null,null,"30.01.10","ROCADA MANUAL","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.203,110"]
[null,null,null,null,null,null,null,null,null,null,"30.01.11","ROCADA MECANIZADA","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.145,080"]
[null,null,null,null,null,null,null,null,null,null,"30.01.12","CAPINA MANUAL,INCL.AMONT.CARGA/DESC.","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.716,980"]
[null,null,null,null,null,null,null,null,null,null,"30.01.21","PLANTIO DE ARBUSTOS","un",14.54,10.770370370370369,"DER",14540]
[null,null,null,null,null,null,null,null,null,null,"30.01.22","PLANTIO DE ARVORES","un",40.65,30.111111111111107,"DER",40650]
[null,null,null,null,null,null,null,null,null,null,"30.01.30","PLANTIO DE GRAMINEAS SEMENTE TELA BIODEG","m²",11.93,8.837037037037037,"DER",11930]
[null,null,null,null,null,null,null,null,null,null,"30.01.40.01","PLANTIO COM ESSENCIAS FLORESTAIS NATIVAS H<=0,60M","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","9.213,350"]
[null,null,null,null,null,null,null,null,null,null,"30.01.40.02","MANUTENCAO DO PLANTIO COM ESSENCIAS FLORESTAIS NATIVAS","ha x mes",504.19,373.47407407407405,"DER",504190]
[null,null,null,null,null,null,null,null,null,null,"30.01.40.03","PLANTIO ESSENCIAS FLORESTAIS NATIVAS h>=1,50M","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","29.107,320"]
[null,null,null,null,null,null,null,null,null,null,"30.02.02.01","ALAMBRADO COM TELA 15X5 E ESTICADOR","m²",55.03,40.76296296296296,"DER",55030]
[null,null,null,null,null,null,null,null,null,null,"30.02.04","CERCA DE ARAME DE ACO OVALADO - 4 FIOS","m",10.69,7.918518518518518,"DER",10690]
[null,null,null,null,null,null,null,null,null,null,"30.02.05","ALAMBRADO EM TELA REVESTIDA EM PVC PARA CONDUCAO DE FAunA","m²",74.65,55.2962962962963,"DER",74650]
[null,null,null,null,null,null,null,null,null,null,"30.03.01","PROJETO DE PLANTIO COM ESSENCIAS FLORESTAIS NATIVAS","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.775,010"]
[null,null,null,null,null,null,null,null,null,null,"34.03.01","LIMPEZA DE AREAS INT.PISOS ACARPETADOS","m² x mes",4.22,3.1259259259259253,"DER",4220]
[null,null,null,null,null,null,null,null,null,null,"34.03.02","LIMPEZA DE AREAS INTERNAS E PISOS FRIOS","m² x mes",4.22,3.1259259259259253,"DER",4220]
[null,null,null,null,null,null,null,null,null,null,"34.03.03","LIMPEZA DE AREAS INTERNAS LABORATORIOS","m² x mes",7.66,5.674074074074074,"DER",7660]
[null,null,null,null,null,null,null,null,null,null,"34.03.04","LIMPEZA DE AREAS INT.ALMOXARIF.E GALPOES","m² x mes",1.87,1.385185185185185,"DER",1870]
[null,null,null,null,null,null,null,null,null,null,"34.03.05","LIMPEZA DE AREAS INTERNAS OFICINAS","m² x mes",2.1,1.5555555555555556,"DER",2100]
[null,null,null,null,null,null,null,null,null,null,"34.03.06","LIMPEZA AREAS EXT.PISOS PAV.E TERRA","m² x mes",2.1,1.5555555555555556,"DER",2100]
[null,null,null,null,null,null,null,null,null,null,"34.03.07","LIMP.EXT.PAT.E AREAS VERDES - ALTA FREQ.","m² x mes",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,380"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"34.03.08","LIMP.EXT.PAT.E AREAS VERDES - MEDIA FREQ","m² x mes",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,190"]
[null,null,null,null,null,null,null,null,null,null,"34.03.09","LIMP.EXT.PAT.E AREAS VERDES - BAIXA FREQ","m² x mes",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,100"]
[null,null,null,null,null,null,null,null,null,null,"34.03.10","VIDROS EXTERNOS C/EXP.RISCO TRIMESTR.","m² x mes",1.58,1.1703703703703703,"DER",1580]
[null,null,null,null,null,null,null,null,null,null,"34.03.11","VIDROS EXTERNOS S/EXP.RISCO - TRIMESTR.","m² x mes",1.23,0.911111111111111,"DER",1230]
[null,null,null,null,null,null,null,null,null,null,"34.03.12","VIDROS EXTERNOS C/EXP.RISCO - SEMESTRAL","m² x mes",1.32,0.9777777777777777,"DER",1320]
[null,null,null,null,null,null,null,null,null,null,"34.03.13","VIDROS EXTERNOS S/EXP.RISCO - SEMESTRAL","m² x mes",1.13,0.8370370370370369,"DER",1130]
[null,null,null,null,null,null,null,null,null,null,"34.04.02","VIG.44H SEM. DIURNO","postoxdia",188.41,139.56296296296296,"DER",188410]
[null,null,null,null,null,null,null,null,null,null,"34.04.04","VIG.12H DIURNO DE SEGunDA A DOMINGO","postoxdia",248.93,184.3925925925926,"DER",248930]
[null,null,null,null,null,null,null,null,null,null,"34.04.06","VIG.12H NOTURNO DE SEGunDA A DOMINGO","postoxdia",283.72,210.16296296296298,"DER",283720]
[null,null,null,null,null,null,null,null,null,null,"34.05.02","PORT.44H SEM.DIURNO DE SEG./SEXTA-FEIRA","postoxdia",127.32,94.3111111111111,"DER",127320]
[null,null,null,null,null,null,null,null,null,null,"34.05.04","PORT.12H DIARIAS DIURNO DE SEG./SEXTA-FEIRA","postoxdia",163.02,120.75555555555556,"DER",163020]
[null,null,null,null,null,null,null,null,null,null,"34.05.06","PORT.8H DIURNO DE SEGunDA A DOMINGO","postoxdia",121.36,89.89629629629628,"DER",121360]
[null,null,null,null,null,null,null,null,null,null,"34.05.08","PORT.24 DIUTURNO DE SEGunDA A DOMINGO","postoxdia",359.59,266.3629629629629,"DER",359590]
[null,null,null,null,null,null,null,null,null,null,"34.07.01.01","MEDICO SUPERVISOR","hora",155.56,115.22962962962963,"DER",155560]
[null,null,null,null,null,null,null,null,null,null,"34.07.01.02","PARAMEDICO","hora",33.49,24.807407407407407,"DER",33490]
[null,null,null,null,null,null,null,null,null,null,"34.07.01.03","ATENDENTE DE PRIMEIROS SOCORROS","hora",19.45,14.407407407407407,"DER",19450]
[null,null,null,null,null,null,null,null,null,null,"34.07.01.04","AUX.ATENDENTE DE PRIMEIROS SOCORROS","hora",21.66,16.044444444444444,"DER",21660]
[null,null,null,null,null,null,null,null,null,null,"34.07.01.05","MOTORISTA AMBULANCIA","hora",19.17,14.200000000000001,"DER",19170]
[null,null,null,null,null,null,null,null,null,null,"34.07.01.06","OPERADOR DE GUINCHO","hora",19.24,14.25185185185185,"DER",19240]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.01","ESTUDO HIDROLOGICO E APROV. DO DAEE","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","13.208,670"]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.02.01","CARACT.AMBIENTAL EMPREEND.ROD.ELAB.REL.TECN.INTERV.AREA","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","11.860,470"]
[null,null,null,null,null,null,null,null,null,null,null,"PRES.CETESB S19 E S07",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,"CARACT.AMBIENTAL EMPREEND.ROD.AREA PRESERV.CETESB S19 E S07",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.02.02",">10<=20KM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","16.579,750"]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.02.03","CARACT.AMBIENTAL EMPREEND.ROD.AREA PRESERV.CETESB S19 E S07 >20<=30","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","21.300,220"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.02.04","CARACT.AMBIENTAL EMPREEND.ROD.AREA PRESERV.CETESB S19 E S07 >30<=40KM","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","26.019,500"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.03","ELABORACAO DE EVI E APROVACAO DE IMPLANTACAO DO EMPREENDIMENTO NO DAEE.","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","7.019,030"]
[null,null,null,null,null,null,null,null,null,null,"34.08.27.04","DIREITO DE USO DO RECURSO HIDRICO EM TRAVESSIAS / DAEE","un",288.78,213.91111111111107,"DER",288780]
[null,null,null,null,null,null,null,null,null,null,"34.09.01","EQUIPE DE MERGULHO COM FILMAGEM","equipe.dia",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.736,050"]
[null,null,null,null,null,null,null,null,null,null,"34.09.02","EQUIPE DE MERGULHO SEM FILMAGEM","equipe.dia",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.459,230"]
[null,null,null,null,null,null,null,null,null,null,"35.03.01","ADVOGADO JunIOR","hora",69.85,51.74074074074073,"DER",69850]
[null,null,null,null,null,null,null,null,null,null,"35.03.02","ADVOGADO PLENO","hora",108.57,80.42222222222222,"DER",108570]
[null,null,null,null,null,null,null,null,null,null,"35.03.03","ADVOGADO SENIOR","hora",179.43,132.9111111111111,"DER",179430]
[null,null,null,null,null,null,null,null,null,null,"35.03.04","ANALISTA DE SISTEMA JunIOR","hora",70.18,51.98518518518519,"DER",70180]
[null,null,null,null,null,null,null,null,null,null,"35.03.05","ANALISTA DE SISTEMA PLENO","hora",106.55,78.92592592592592,"DER",106550]
[null,null,null,null,null,null,null,null,null,null,"35.03.06","ANALISTA DE SISTEMA SENIOR","hora",146.12,108.23703703703703,"DER",146120]
[null,null,null,null,null,null,null,null,null,null,"35.03.07","ARQUITETO JunIOR","hora",105.81,78.37777777777778,"DER",105810]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"35.03.08","ARQUITETO PLENO","hora",115.37,85.45925925925926,"DER",115370]
[null,null,null,null,null,null,null,null,null,null,"35.03.09","ARQUITETO SENIOR","hora",204.68,151.61481481481482,"DER",204680]
[null,null,null,null,null,null,null,null,null,null,"35.03.10","AUXILIAR DE ESCRITORIO","hora",22.25,16.48148148148148,"DER",22250]
[null,null,null,null,null,null,null,null,null,null,"35.03.11","AUXILIAR DE LABORATORIO","hora",23.34,17.288888888888888,"DER",23340]
[null,null,null,null,null,null,null,null,null,null,"35.03.12","AUXILIAR DE TOPOGRAFIA","hora",22.52,16.68148148148148,"DER",22520]
[null,null,null,null,null,null,null,null,null,null,"35.03.13","AUXILIAR TECNICO","hora",33.84,25.066666666666666,"DER",33840]
[null,null,null,null,null,null,null,null,null,null,"35.03.14","CHEFE DE ESCRITORIO","hora",74.21,54.97037037037036,"DER",74210]
[null,null,null,null,null,null,null,null,null,null,"35.03.15","CONSULTOR","hora",500.32,370.6074074074074,"DER",500320]
[null,null,null,null,null,null,null,null,null,null,"35.03.16","CONSULTOR B","hora",295.88,219.17037037037036,"DER",295880]
[null,null,null,null,null,null,null,null,null,null,"35.03.17","CONSULTOR C","hora",224.99,166.65925925925924,"DER",224990]
[null,null,null,null,null,null,null,null,null,null,"35.03.18","CONSULTOR INTERNACIONAL","hora",500.32,370.6074074074074,"DER",500320]
[null,null,null,null,null,null,null,null,null,null,"35.03.19","CONSULTOR JURIDICO","hora",500.32,370.6074074074074,"DER",500320]
[null,null,null,null,null,null,null,null,null,null,"35.03.20","COORDENADOR","hora",347.06,257.0814814814815,"DER",347060]
[null,null,null,null,null,null,null,null,null,null,"35.03.21","CADISTA","hora",47.45,35.148148148148145,"DER",47450]
[null,null,null,null,null,null,null,null,null,null,"35.03.23","CADISTA / CALCULISTA I","hora",39.48,29.24444444444444,"DER",39480]
[null,null,null,null,null,null,null,null,null,null,"35.03.24","CADISTA / CALCULISTA II","hora",46.12,34.16296296296296,"DER",46120]
[null,null,null,null,null,null,null,null,null,null,"35.03.25","CADISTA / CALCULISTA III","hora",58.13,43.05925925925926,"DER",58130]
[null,null,null,null,null,null,null,null,null,null,"35.03.26","DIGITADOR","hora",18.1,13.407407407407408,"DER",18100]
[null,null,null,null,null,null,null,null,null,null,"35.03.27","ECONOMISTA JunIOR","hora",70.89,52.511111111111106,"DER",70890]
[null,null,null,null,null,null,null,null,null,null,"35.03.28","ECONOMISTA PLENO","hora",112.88,83.6148148148148,"DER",112880]
[null,null,null,null,null,null,null,null,null,null,"35.03.29","ECONOMISTA SENIOR","hora",139.51,103.34074074074073,"DER",139510]
[null,null,null,null,null,null,null,null,null,null,"35.03.30","ENGENHEIRO JunIOR","hora",115.17,85.3111111111111,"DER",115170]
[null,null,null,null,null,null,null,null,null,null,"35.03.31","ENGENHEIRO PLENO","hora",143.42,106.23703703703703,"DER",143420]
[null,null,null,null,null,null,null,null,null,null,"35.03.32","ENGENHEIRO SENIOR","hora",198.21,146.82222222222222,"DER",198210]
[null,null,null,null,null,null,null,null,null,null,"35.03.33","ESPECIALISTA EM TREINAMENTO PLENO","hora",141.49,104.80740740740741,"DER",141490]
[null,null,null,null,null,null,null,null,null,null,"35.03.34","ESPECIALISTA EM TREINAMENTO SENIOR","hora",142.38,105.46666666666665,"DER",142380]
[null,null,null,null,null,null,null,null,null,null,"35.03.35","FISCAL DE OBRAS","hora",46.34,34.32592592592593,"DER",46340]
[null,null,null,null,null,null,null,null,null,null,"35.03.36","GEOLOGO JunIOR","hora",99.75,73.88888888888889,"DER",99750]
[null,null,null,null,null,null,null,null,null,null,"35.03.37","GEOLOGO PLENO","hora",143.96,106.63703703703703,"DER",143960]
[null,null,null,null,null,null,null,null,null,null,"35.03.38","GEOLOGO SENIOR","hora",180.07,133.38518518518518,"DER",180070]
[null,null,null,null,null,null,null,null,null,null,"35.03.39","LABORATORISTA","hora",54.05,40.03703703703703,"DER",54050]
[null,null,null,null,null,null,null,null,null,null,"35.03.40","MENSAGEIRO","hora",19.74,14.62222222222222,"DER",19740]
[null,null,null,null,null,null,null,null,null,null,"35.03.41","MOTORISTA","hora",27.73,20.54074074074074,"DER",27730]
[null,null,null,null,null,null,null,null,null,null,"35.03.42","NIVELADOR","hora",31.01,22.97037037037037,"DER",31010]
[null,null,null,null,null,null,null,null,null,null,"35.03.43","PROGRAMADOR DE COMPUTADOR JunIOR","hora",51.36,38.044444444444444,"DER",51360]
[null,null,null,null,null,null,null,null,null,null,"35.03.44","PROGRAMADOR DE COMPUTADOR PLENO","hora",61.38,45.46666666666667,"DER",61380]
[null,null,null,null,null,null,null,null,null,null,"35.03.45","PROGRAMADOR DE COMPUTADOR SENIOR","hora",98.19,72.73333333333332,"DER",98190]
[null,null,null,null,null,null,null,null,null,null,"35.03.46","PROJETISTA A / ASSISTENTE TECNICO I","hora",84.39,62.511111111111106,"DER",84390]
[null,null,null,null,null,null,null,null,null,null,"35.03.47","PROJETISTA B / ASSISTENTE TECNICO II","hora",117.19,86.8074074074074,"DER",117190]
[null,null,null,null,null,null,null,null,null,null,"35.03.48","PROJETISTA C / ASSISTENTE TECNICO III","hora",192.3,142.44444444444446,"DER",192300]
[null,null,null,null,null,null,null,null,null,null,"35.03.50","SECRETARIA","hora",51.24,37.955555555555556,"DER",51240]
[null,null,null,null,null,null,null,null,null,null,"35.03.51","TOPOGRAFO","hora",82.64,61.21481481481481,"DER",82640]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"35.04.01","ADVOGADO JunIOR TEMPORARIO","hora",42.04,31.14074074074074,"DER",42040]
[null,null,null,null,null,null,null,null,null,null,"35.04.02","ADVOGADO PLENO TEMPORARIO","hora",65.35,48.4074074074074,"DER",65350]
[null,null,null,null,null,null,null,null,null,null,"35.04.03","ADVOGADO SENIOR TEMPORARIO","hora",108,80,"DER",108000]
[null,null,null,null,null,null,null,null,null,null,"35.04.04","ANALISTA DE SISTEMA JunIOR TEMPORARIO","hora",42.24,31.288888888888888,"DER",42240]
[null,null,null,null,null,null,null,null,null,null,"35.04.05","ANALISTA DE SISTEMA PLENO TEMPORARIO","hora",64.13,47.5037037037037,"DER",64130]
[null,null,null,null,null,null,null,null,null,null,"35.04.06","ANALISTA DE SISTEMA SENIOR TEMPORARIO","hora",87.95,65.14814814814815,"DER",87950]
[null,null,null,null,null,null,null,null,null,null,"35.04.07","ARQUITETO JunIOR TEMPORARIO","hora",63.69,47.17777777777777,"DER",63690]
[null,null,null,null,null,null,null,null,null,null,"35.04.08","ARQUITETO PLENO TEMPORARIO","hora",69.44,51.43703703703703,"DER",69440]
[null,null,null,null,null,null,null,null,null,null,"35.04.09","ARQUITETO SENIOR TEMPORARIO","hora",123.19,91.25185185185184,"DER",123190]
[null,null,null,null,null,null,null,null,null,null,"35.04.10","AUXILIAR DE ESCRITORIO TEMPORARIO","hora",13.38,9.911111111111111,"DER",13380]
[null,null,null,null,null,null,null,null,null,null,"35.04.11","AUXILIAR DE LABORATORIO TEMPORARIO","hora",14.05,10.407407407407407,"DER",14050]
[null,null,null,null,null,null,null,null,null,null,"35.04.12","AUXILIAR DE TOPOGRAFIA TEMPORARIO","hora",13.56,10.044444444444444,"DER",13560]
[null,null,null,null,null,null,null,null,null,null,"35.04.13","AUXILIAR TECNICO TEMPORARIO","hora",20.37,15.088888888888889,"DER",20370]
[null,null,null,null,null,null,null,null,null,null,"35.04.14","CHEFE DE ESCRITORIO TEMPORARIO","hora",44.67,33.08888888888889,"DER",44670]
[null,null,null,null,null,null,null,null,null,null,"35.04.15","CONSULTOR TEMPORARIO","hora",301.14,223.06666666666663,"DER",301140]
[null,null,null,null,null,null,null,null,null,null,"35.04.16","CONSULTOR B TEMPORARIO","hora",178.09,131.9185185185185,"DER",178090]
[null,null,null,null,null,null,null,null,null,null,"35.04.17","CONSULTO C TEMPORARIO","hora",135.42,100.31111111111109,"DER",135420]
[null,null,null,null,null,null,null,null,null,null,"35.04.18","CONSULTOR INTERNACIONAL TEMPORARIO","hora",301.14,223.06666666666663,"DER",301140]
[null,null,null,null,null,null,null,null,null,null,"35.04.19","CONSULTOR JURIDICO TEMPORARIO","hora",301.14,223.06666666666663,"DER",301140]
[null,null,null,null,null,null,null,null,null,null,"35.04.20","COORDENADOR TEMPORARIO","hora",208.89,154.73333333333332,"DER",208890]
[null,null,null,null,null,null,null,null,null,null,"35.04.21","CADISTA TEMPORARIO","hora",28.56,21.15555555555555,"DER",28560]
[null,null,null,null,null,null,null,null,null,null,"35.04.23","CADISTA / CALCULISTA I TEMPORARIO","hora",23.76,17.6,"DER",23760]
[null,null,null,null,null,null,null,null,null,null,"35.04.24","CADISTA / CALCULISTA II TEMPORARIO","hora",27.76,20.562962962962963,"DER",27760]
[null,null,null,null,null,null,null,null,null,null,"35.04.25","CADISTA / CALCULISTA III TEMPORARIO","hora",34.99,25.918518518518518,"DER",34990]
[null,null,null,null,null,null,null,null,null,null,"35.04.26","DIGITADOR TEMPORARIO","hora",10.89,8.066666666666666,"DER",10890]
[null,null,null,null,null,null,null,null,null,null,"35.04.27","ECONOMISTA JunIOR TEMPORARIO","hora",42.67,31.607407407407408,"DER",42670]
[null,null,null,null,null,null,null,null,null,null,"35.04.28","ECONOMISTA PLENO TEMPORARIO","hora",67.94,50.32592592592592,"DER",67940]
[null,null,null,null,null,null,null,null,null,null,"35.04.29","ECONOMISTA SENIOR TEMPORARIO","hora",83.97,62.199999999999996,"DER",83970]
[null,null,null,null,null,null,null,null,null,null,"35.04.30","ENGENHEIRO JunIOR TEMPORARIO","hora",69.32,51.34814814814814,"DER",69320]
[null,null,null,null,null,null,null,null,null,null,"35.04.31","ENGENHEIRO PLENO TEMPORARIO","hora",86.32,63.94074074074073,"DER",86320]
[null,null,null,null,null,null,null,null,null,null,"35.04.32","ENGENHEIRO SENIOR TEMPORARIO","hora",119.3,88.37037037037037,"DER",119300]
[null,null,null,null,null,null,null,null,null,null,"35.04.33","ESPECIALISTA EM TREINAMENTO PLENO TEMPORARIO","hora",85.16,63.081481481481475,"DER",85160]
[null,null,null,null,null,null,null,null,null,null,"35.04.34","ESPECIALISTA EM TREINAMENTO SENIOR TEMPORARIO","hora",85.7,63.48148148148148,"DER",85700]
[null,null,null,null,null,null,null,null,null,null,"35.04.35","FISCAL DE OBRA TEMPORARIO","hora",27.89,20.659259259259258,"DER",27890]
[null,null,null,null,null,null,null,null,null,null,"35.04.36","GEOLOGO JunIOR TEMPORARIO","hora",60.04,44.47407407407407,"DER",60040]
[null,null,null,null,null,null,null,null,null,null,"35.04.37","GEOLOGO PLENO TEMPORARIO","hora",86.65,64.18518518518519,"DER",86650]
[null,null,null,null,null,null,null,null,null,null,"35.04.38","GEOLOGO SENIOR TEMPORARIO","hora",108.38,80.28148148148148,"DER",108380]
[null,null,null,null,null,null,null,null,null,null,"35.04.39","LABORATORISTA TEMPORARIO","hora",32.53,24.096296296296295,"DER",32530]
[null,null,null,null,null,null,null,null,null,null,"35.04.40","MENSAGEIRO TEMPORARIO","hora",11.88,8.8,"DER",11880]
[null,null,null,null,null,null,null,null,null,null,"35.04.41","MOTORISTA TEMPORARIO","hora",16.69,12.362962962962962,"DER",16690]
[null,null,null,null,null,null,null,null,null,null,"35.04.42","NIVELADOR TEMPORARIO","hora",18.66,13.822222222222221,"DER",18660]
[null,null,null,null,null,null,null,null,null,null,"35.04.43","PROGRAMADOR DE COMPUTADOR JunIOR TEMPORARIO","hora",30.91,22.896296296296295,"DER",30910]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"35.04.44","PROGRAMADOR DE COMPUTADOR PLENO TEMPORARIO","hora",36.94,27.36296296296296,"DER",36940]
[null,null,null,null,null,null,null,null,null,null,"35.04.45","PROGRAMADOR DE COMPUTADOR SENIOR TEMPORARIO","hora",59.1,43.77777777777778,"DER",59100]
[null,null,null,null,null,null,null,null,null,null,"35.04.46","PROJETISTA A / ASSISTENTE TECNICO I TEMPORARIO","hora",50.8,37.629629629629626,"DER",50800]
[null,null,null,null,null,null,null,null,null,null,"35.04.47","PROJETISTA B / ASSISTENTE TECNICO II TEMPORARIO","hora",70.54,52.25185185185185,"DER",70540]
[null,null,null,null,null,null,null,null,null,null,"35.04.48","PROJETISTA C / ASSISTENTE TECNICO III TEMPORARIO","hora",115.75,85.74074074074073,"DER",115750]
[null,null,null,null,null,null,null,null,null,null,"35.04.50","SECRETARIA TEMPORARIO","hora",30.84,22.84444444444444,"DER",30840]
[null,null,null,null,null,null,null,null,null,null,"35.04.51","TOPOGRAFO TEMPORARIO","hora",49.74,36.84444444444444,"DER",49740]
[null,null,null,null,null,null,null,null,null,null,"36.01.01.01","INST.CANTEIRO-TIPO I (1,500%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.01.02","OPER.E MANUTENCAO CANTEIRO TIPOI(0,875%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.01.03","DESMOBILIZACAO CANTEIRO TIPOI(0,125%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.02.01","INST.CANTEIRO-TIPOII (1,800%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.02.02","OPER.E MANUTENCAO CANTEIRO II (1,050%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.02.03","DESMOBILIZACAO CANTEIRO TIPO II (0,150%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.03.01","INST.CANTEIRO TIPO III (4,800%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.03.02","OPER./MANUTENCAO CANTEIRO III (0,900%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"36.01.03.03","DESMOBILIZACAO CANTEIRO III (0,300%)","global",1,0.7407407407407407,"DER",1000]
[null,null,null,null,null,null,null,null,null,null,"37.01.01","REPARO TOTAL DE CERCA","m",28.55,21.14814814814815,"DER",28550]
[null,null,null,null,null,null,null,null,null,null,"37.01.02","REPARO PARCIAL DE CERCA - MOURAO","m",21.44,15.881481481481481,"DER",21440]
[null,null,null,null,null,null,null,null,null,null,"37.01.03","REPARO PARCIAL DE CERCA-ARAME","m",3.49,2.585185185185185,"DER",3490]
[null,null,null,null,null,null,null,null,null,null,"37.01.04","LIMPEZA DE DRENAGEM DA PLATAFORMA","m",1.05,0.7777777777777778,"DER",1050]
[null,null,null,null,null,null,null,null,null,null,"37.01.05","LIMPEZA DE DRENAGEM FORA DA PLATAFORMA","m",1.26,0.9333333333333332,"DER",1260]
[null,null,null,null,null,null,null,null,null,null,"37.01.06","LIMPEZA DE BUEIROS DIAMETRO D<=0,60M","m",39.13,28.985185185185184,"DER",39130]
[null,null,null,null,null,null,null,null,null,null,"37.01.07","LIMPEZA DE BUEIROS DIAMETRO 0,6<D<=0,8M","m",50.02,37.05185185185185,"DER",50020]
[null,null,null,null,null,null,null,null,null,null,"37.01.08","LIMPEZA DE BUEIROS DIAMETRO 0,8 < D <=1,0M","m",52.28,38.72592592592592,"DER",52280]
[null,null,null,null,null,null,null,null,null,null,"37.01.09","LIMPEZA DE BUEIROS DIAMETRO 1,0<D<=1,20M","m",55.88,41.39259259259259,"DER",55880]
[null,null,null,null,null,null,null,null,null,null,"37.01.10","LIMPEZA DE BUEIROS 1,20<D<=1,50M","m",59.14,43.8074074074074,"DER",59140]
[null,null,null,null,null,null,null,null,null,null,"37.01.11","LIMPEZA DE GALERIA","m",52.62,38.977777777777774,"DER",52620]
[null,null,null,null,null,null,null,null,null,null,"37.01.12","REPARO DRENAGEM SUPERFICIAL DE CONCRETO","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.015,660"]
[null,null,null,null,null,null,null,null,null,null,"37.01.13","DEMOLICAO OBRAS DE CONCRETO SIMPLES","m³",158.86,117.67407407407407,"DER",158860]
[null,null,null,null,null,null,null,null,null,null,"37.01.14","DEMOLICAO OBRAS DE CONCRETO ARMADO","m³",298.95,221.44444444444443,"DER",298950]
[null,null,null,null,null,null,null,null,null,null,"37.01.15","DEMOLICAO E RETIRADA DE GUARDA-CORPO","m³",272.54,201.88148148148147,"DER",272540]
[null,null,null,null,null,null,null,null,null,null,"37.01.16","LIMPEZA DE PLACA","m²",7.3,5.4074074074074066,"DER",7300]
[null,null,null,null,null,null,null,null,null,null,"37.01.17","LIMPEZA TACHA REFLETIVA MONO/BIDIREC","un",1.96,1.4518518518518517,"DER",1960]
[null,null,null,null,null,null,null,null,null,null,"37.01.18","PINTURA DE CAIACAO 2 DEMAOS","m²",16.52,12.237037037037036,"DER",16520]
[null,null,null,null,null,null,null,null,null,null,"37.01.19","LIMPEZA SUPERFICIAL CONCRETO","m²",6.72,4.977777777777777,"DER",6720]
[null,null,null,null,null,null,null,null,null,null,"37.01.20","ALVENARIA DE 1 TIJOLO","m³",797.65,590.8518518518518,"DER",797650]
[null,null,null,null,null,null,null,null,null,null,"37.01.21","RECOLHIMENTO DE ANIMAIS","equipe.hor",75.08,55.61481481481481,"DER",75080]
[null,null,null,null,null,null,null,null,null,null,"37.01.22","EQUIPE PARA SERVICOS CONSERVACAO","equip/dia",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.455,690"]
[null,null,null,null,null,null,null,null,null,null,"37.01.23","TRANSPORTE DE PESSOAL","km",1.15,0.8518518518518517,"DER",1150]
[null,null,null,null,null,null,null,null,null,null,"37.01.24","PINTURA LATEX ACRILICA","m²",25.26,18.711111111111112,"DER",25260]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.02.01","REPOSICAO DE REVEST.PRIMARIO NA PISTA","m³",105.41,78.08148148148148,"DER",105410]
[null,null,null,null,null,null,null,null,null,null,"37.02.02","REPOSICAO REVEST.PRIMARIO ACOSTAMENTO","m³",105.41,78.08148148148148,"DER",105410]
[null,null,null,null,null,null,null,null,null,null,"37.02.03","RECONFORMACAO DE PLATAFORMA","km",334.71,247.9333333333333,"DER",334710]
[null,null,null,null,null,null,null,null,null,null,"37.02.04","RECONFORMACAO DE ACOSTAMENTO","km",115.05,85.22222222222221,"DER",115050]
[null,null,null,null,null,null,null,null,null,null,"37.02.05","RECOMPOSICAO MANUAL DE ATERRO","m³",65.37,48.422222222222224,"DER",65370]
[null,null,null,null,null,null,null,null,null,null,"37.02.06","RECOMPOSICAO MECANICA DE ATERRO","m³",19.47,14.42222222222222,"DER",19470]
[null,null,null,null,null,null,null,null,null,null,"37.02.07","REMOCAO MANUAL DE BARREIRA","m³",39.24,29.066666666666666,"DER",39240]
[null,null,null,null,null,null,null,null,null,null,"37.02.08","REMOCAO MECANICA DE BARREIRA","m³",27.23,20.17037037037037,"DER",27230]
[null,null,null,null,null,null,null,null,null,null,"37.02.10","RETALUDAMENTO MECANICO 1A/2A CAT.","m³",49.47,36.64444444444444,"DER",49470]
[null,null,null,null,null,null,null,null,null,null,"37.02.11","DEST.ARV.COM PERIMETRO MAIOR QUE 78CM","un",22.86,16.933333333333334,"DER",22860]
[null,null,null,null,null,null,null,null,null,null,"37.02.12","LIMP.TERRENO C/DEST.ARV.PERIMETRO<=78","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,680"]
[null,null,null,null,null,null,null,null,null,null,"37.02.13","LIMP.TERRENO S/DESTOCAMENTO DE ARVORE","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,280"]
[null,null,null,null,null,null,null,null,null,null,"37.02.14.01","ESCAVACAO E CARGA DE MATERIAL DE 1/2A CATEGORIA","m³",4.9,3.6296296296296298,"DER",4900]
[null,null,null,null,null,null,null,null,null,null,"37.02.17","ESCAV.CARGA MATERIAL 2A.CAT.C/RIPPER","m³",5.44,4.029629629629629,"DER",5440]
[null,null,null,null,null,null,null,null,null,null,"37.02.18","ESCAV.CARGA MATERIAL 2A.CAT.C/EXPLOSIVO","m³",19.85,14.703703703703704,"DER",19850]
[null,null,null,null,null,null,null,null,null,null,"37.02.19","ESCAVACAO E CARGA MATERIAL DE 3A.CAT.","m³",31.63,23.429629629629627,"DER",31630]
[null,null,null,null,null,null,null,null,null,null,"37.02.20","COMPACTACAO ATERRO MAIOR/IGUAL 95%PS","m³",3.01,2.2296296296296294,"DER",3010]
[null,null,null,null,null,null,null,null,null,null,"37.02.21","TRANSPORTE DE 1A/2A. CATEGORIA ATE 1KM","m³*km",3.74,2.77037037037037,"DER",3740]
[null,null,null,null,null,null,null,null,null,null,"37.02.22","TRANSPORTE DE 1A/2A. CATEGORIA ATE 2KM","m³*km",2.2,1.6296296296296298,"DER",2200]
[null,null,null,null,null,null,null,null,null,null,"37.02.23","TRANSPORTE DE 1A/2A. CATEGORIA ATE 5KM","m³*km",1.71,1.2666666666666666,"DER",1710]
[null,null,null,null,null,null,null,null,null,null,"37.02.24","TRANSPORTE DE 1A/2A. CATEGORIA ATE 10KM","m³*km",1.43,1.0592592592592591,"DER",1430]
[null,null,null,null,null,null,null,null,null,null,"37.02.25","TRANSPORTE DE 1A/2A. CATEGORIA ATE 15KM","m³*km",1.26,0.9333333333333332,"DER",1260]
[null,null,null,null,null,null,null,null,null,null,"37.02.26","TRANSPORTE DE 1A/2A. CATEGORIA ALEM 15KM","m³*km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,990"]
[null,null,null,null,null,null,null,null,null,null,"37.02.27","REVESTIMENTO PRIMARIO","m³",105.41,78.08148148148148,"DER",105410]
[null,null,null,null,null,null,null,null,null,null,"37.03.01","REMENDO PRE-MISTURADO A QUENTE","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.179,610"]
[null,null,null,null,null,null,null,null,null,null,"37.03.02","REMENDO PRE-MISTURADO A FRIO","m³",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.131,040"]
[null,null,null,null,null,null,null,null,null,null,"37.03.03","REPARO EMERGENCIAL DE PAV.-TAPA BURACO","m³",803.78,595.3925925925926,"DER",803780]
[null,null,null,null,null,null,null,null,null,null,"37.03.03.01","REPARO EMERGENCIAL DE PAV.-TAPA BURACO COM CBUQ E EQUIP. C/ SILO MOVEL TERMICO","m³",926.1,686,"DER",926100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.03.04","REPARO DE BASE BRITA GRADUADA","m³",356.65,264.18518518518516,"DER",356650]
[null,null,null,null,null,null,null,null,null,null,"37.03.05.02","SELAGEM DE TRINCA COM MASTIQUE ASFALTICO","litro",21.58,15.985185185185182,"DER",21580]
[null,null,null,null,null,null,null,null,null,null,"37.03.06","REPARO DE CONCRETO PORTLAND","m³",483.99,358.5111111111111,"DER",483990]
[null,null,null,null,null,null,null,null,null,null,"37.03.07","ESCAVACAO P/ REFORCO DE SUB-LEITO","m³",5.06,3.7481481481481476,"DER",5060]
[null,null,null,null,null,null,null,null,null,null,"37.03.08","COMPACTACAO PARA REFORCO DE SUB-LEITO","m³",5.09,3.77037037037037,"DER",5090]
[null,null,null,null,null,null,null,null,null,null,"37.03.09","PREPARO E MELHORAMENTO SUB-LEITO","m²",1.14,0.8444444444444443,"DER",1140]
[null,null,null,null,null,null,null,null,null,null,"37.03.10","SUB-BASE OU BASE BRITA GRAD.SIMPLES","m³",168.38,124.72592592592592,"DER",168380]
[null,null,null,null,null,null,null,null,null,null,"37.03.11","IMPRIMADURA BET.IMPERMEABILIZANTE","m²",3.42,2.533333333333333,"DER",3420]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.03.12","IMPRIMADURA BETUMINOSA LIGANTE","m²",1.32,0.9777777777777777,"DER",1320]
[null,null,null,null,null,null,null,null,null,null,"37.03.13","TRATAMENTO SUPERF.C/LAMA ASFALTICA","m²",4.52,3.3481481481481477,"DER",4520]
[null,null,null,null,null,null,null,null,null,null,"37.03.14","CAMADA DE LAMA ASFALTICA GROSSA","m²",5.8,4.296296296296296,"DER",5800]
[null,null,null,null,null,null,null,null,null,null,"37.03.15","CAMADA DE ROLAMENTO CBUQ - PANOS S/DOP","m³",646.25,478.7037037037037,"DER",646250]
[null,null,null,null,null,null,null,null,null,null,"37.03.16","CAM.BASE/REGULARIZACAO DE PMF","m³",442.63,327.87407407407403,"DER",442630]
[null,null,null,null,null,null,null,null,null,null,"37.03.17","CAPA SELANTE BETUMINOSA","m²",2.51,1.859259259259259,"DER",2510]
[null,null,null,null,null,null,null,null,null,null,"37.03.18","FRESAGEM PAVIMENTO","m³",139.28,103.17037037037036,"DER",139280]
[null,null,null,null,null,null,null,null,null,null,"37.03.19","IMPRIMADURA BET. AUXILIAR DE LIGACAO","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,730"]
[null,null,null,null,null,null,null,null,null,null,"37.03.20","REMOCAO CAMADA DE ROLAMENTO","m³",27.85,20.62962962962963,"DER",27850]
[null,null,null,null,null,null,null,null,null,null,"37.03.21","TRATAMENTO SUPERFICIAL DUPLO","m³",330.83,245.05925925925922,"DER",330830]
[null,null,null,null,null,null,null,null,null,null,"37.03.22","TRATAMENTO SUPERFICIAL TRIPLO","m³",412.88,305.837037037037,"DER",412880]
[null,null,null,null,null,null,null,null,null,null,"37.03.23","TRANSPORTE DE SOLO CIMENTO ATE 5 KM","m³*km",2.22,1.6444444444444444,"DER",2220]
[null,null,null,null,null,null,null,null,null,null,"37.03.24","SUB-BASE OU BASE SOLO CIM. 7% - PULV.","m³",91.1,67.48148148148147,"DER",91100]
[null,null,null,null,null,null,null,null,null,null,"37.03.25","SUB-BASE OU BASE SOLO CIM. 10% - PULV.","m³",120.95,89.5925925925926,"DER",120950]
[null,null,null,null,null,null,null,null,null,null,"37.03.26","RECICLAGEM PAVIMENTO IN LOCO","m³",170.2,126.07407407407406,"DER",170200]
[null,null,null,null,null,null,null,null,null,null,"37.04.01","REPARO DE GUARDA CORPO METALICO","m",112.09,83.02962962962962,"DER",112090]
[null,null,null,null,null,null,null,null,null,null,"37.04.02.01","GUIA DE CONCRETO FCK 20 MPA","m³",751.75,556.8518518518518,"DER",751750]
[null,null,null,null,null,null,null,null,null,null,"37.04.03.01","SARJETA DE CONCRETO FCK 20 MPA","m³",603.32,446.9037037037037,"DER",603320]
[null,null,null,null,null,null,null,null,null,null,"37.04.04","ESCAVACAO MANUAL DE 1A/2A CATEGORIA","m³",52.22,38.68148148148148,"DER",52220]
[null,null,null,null,null,null,null,null,null,null,"37.04.05","ESCAV.FunD.,BUEIRO OU DRENO S/EXPL.ATE2M","m³",62.83,46.54074074074074,"DER",62830]
[null,null,null,null,null,null,null,null,null,null,"37.04.06","ACRESC.P/ESCAV. 1,5M PROF.,ALEM 2M","m³",13.05,9.666666666666666,"DER",13050]
[null,null,null,null,null,null,null,null,null,null,"37.04.07","ESCAV.FunD.,BUEIRO OU DRENO C/EXPL.ATE2M","m³",199.61,147.85925925925926,"DER",199610]
[null,null,null,null,null,null,null,null,null,null,"37.04.08","ACR.ESC.ENSEC.EXPL.C/1,5M PROF.ALEM 3M","m³",18.94,14.02962962962963,"DER",18940]
[null,null,null,null,null,null,null,null,null,null,"37.04.09","COMPACTACAO MANUAL,REATERRO SOLO LOCAL","m³",24.16,17.896296296296295,"DER",24160]
[null,null,null,null,null,null,null,null,null,null,"37.04.10","FORMA PLANA P/CONCRETO COMUM","m²",80.07,59.3111111111111,"DER",80070]
[null,null,null,null,null,null,null,null,null,null,"37.04.11","FORMA PLANA PARA CONCRETO APARENTE","m²",90.3,66.88888888888889,"DER",90300]
[null,null,null,null,null,null,null,null,null,null,"37.04.12","FORMA CURVA PARA CONCRETO COMUM","m²",103.09,76.36296296296295,"DER",103090]
[null,null,null,null,null,null,null,null,null,null,"37.04.13","FORMA CURVA PARA CONCRETO APARENTE","m²",107.66,79.74814814814815,"DER",107660]
[null,null,null,null,null,null,null,null,null,null,"37.04.14","BARRA DE ACO CA-25","kg",8.78,6.503703703703703,"DER",8780]
[null,null,null,null,null,null,null,null,null,null,"37.04.15","BARRA DE ACO CA-50","kg",8.52,6.31111111111111,"DER",8520]
[null,null,null,null,null,null,null,null,null,null,"37.04.16","BARRA DE ACO CA-60","kg",9.2,6.814814814814814,"DER",9200]
[null,null,null,null,null,null,null,null,null,null,"37.04.17","CONCRETO FCK 10MPA","m³",386.3,286.14814814814815,"DER",386300]
[null,null,null,null,null,null,null,null,null,null,"37.04.19","CONCRETO FCK 15MPA","m³",426.19,315.6962962962963,"DER",426190]
[null,null,null,null,null,null,null,null,null,null,"37.04.21","CONCRETO FCK 18MPA","m³",435.69,322.7333333333333,"DER",435690]
[null,null,null,null,null,null,null,null,null,null,"37.04.22","CONCRETO FCK 20MPA","m³",455.28,337.2444444444444,"DER",455280]
[null,null,null,null,null,null,null,null,null,null,"37.04.23","CONCRETO FCK 25MPA","m³",467.63,346.39259259259256,"DER",467630]
[null,null,null,null,null,null,null,null,null,null,"37.04.24","CONCRETO FCK 30MPA","m³",483.41,358.0814814814815,"DER",483410]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.04.25","CONCRETO FCK 35MPA","m³",493.31,365.4148148148148,"DER",493310]
[null,null,null,null,null,null,null,null,null,null,"37.04.26","CONCRETO FCK 40MPA","m³",522.21,386.82222222222225,"DER",522210]
[null,null,null,null,null,null,null,null,null,null,"37.04.27","CONCRETO CICLOPICO","m³",390.4,289.18518518518516,"DER",390400]
[null,null,null,null,null,null,null,null,null,null,"37.04.28","BOMBEAMENTO P/CONC.QUALQUER RESIST.","m³",42.12,31.199999999999996,"DER",42120]
[null,null,null,null,null,null,null,null,null,null,"37.04.29","ENROCAMENTO PEDRA ARRUMADA","m³",210.83,156.17037037037036,"DER",210830]
[null,null,null,null,null,null,null,null,null,null,"37.04.30","ENROCAMENTO PEDRA ARRUMADA E REJunTADA","m³",324.57,240.4222222222222,"DER",324570]
[null,null,null,null,null,null,null,null,null,null,"37.04.31","ENROCAMENTO PEDRA JOGADA","m³",136.02,100.75555555555556,"DER",136020]
[null,null,null,null,null,null,null,null,null,null,"37.04.32","TUBO CONCRETO D=0,40M PA-1 - FORNEC.","m",94.94,70.32592592592592,"DER",94940]
[null,null,null,null,null,null,null,null,null,null,"37.04.33","TUBO CONCRETO D=0,40M PA-2 - FORNEC.","m",96.71,71.63703703703703,"DER",96710]
[null,null,null,null,null,null,null,null,null,null,"37.04.34","TUBO CONCRETO D=0,50M PA-3 - FORNEC.","m",144.47,107.01481481481481,"DER",144470]
[null,null,null,null,null,null,null,null,null,null,"37.04.35","TUBO CONCRETO D=0,60M PA-1 - FORNEC.","m",148.53,110.02222222222221,"DER",148530]
[null,null,null,null,null,null,null,null,null,null,"37.04.36","TUBO CONCRETO D=0,60M PA-2 - FORNEC.","m",168.97,125.16296296296295,"DER",168970]
[null,null,null,null,null,null,null,null,null,null,"37.04.37","TUBO CONCRETO D=0,60M PA-3 - FORNEC.","m",197.14,146.0296296296296,"DER",197140]
[null,null,null,null,null,null,null,null,null,null,"37.04.38","TUBO CONCRETO D=0,60M PA-4 - FORNEC.","m",228.81,169.48888888888888,"DER",228810]
[null,null,null,null,null,null,null,null,null,null,"37.04.39","TUBO CONCRETO D=0,80M PA-1 - FORNEC.","m",247.16,183.08148148148146,"DER",247160]
[null,null,null,null,null,null,null,null,null,null,"37.04.40","TUBO CONCRETO D=0,80M PA-2 - FORNEC.","m",252.78,187.24444444444444,"DER",252780]
[null,null,null,null,null,null,null,null,null,null,"37.04.41","TUBO CONCRETO D=0,80M PA-3 - FORNEC.","m",331.45,245.5185185185185,"DER",331450]
[null,null,null,null,null,null,null,null,null,null,"37.04.42","TUBO CONCRETO D=0,80M PA-4 - FORNEC.","m",391.76,290.1925925925926,"DER",391760]
[null,null,null,null,null,null,null,null,null,null,"37.04.43","TUBO CONCRETO D=1,00M PA-1 - FORNEC.","m",347.12,257.1259259259259,"DER",347120]
[null,null,null,null,null,null,null,null,null,null,"37.04.44","TUBO CONCRETO D=1,20M PA-1 - FORNEC.","m",502.37,372.1259259259259,"DER",502370]
[null,null,null,null,null,null,null,null,null,null,"37.04.45","TUBO CONCRETO D=1,50M PA-1 - FORNEC.","m",790.5,585.5555555555555,"DER",790500]
[null,null,null,null,null,null,null,null,null,null,"37.04.46","TUBO CONCRETO D=0,40M ASSENTAMENTO","m",41.54,30.77037037037037,"DER",41540]
[null,null,null,null,null,null,null,null,null,null,"37.04.47","TUBO CONCRETO D=0,50M ASSENTAMENTO","m",48.86,36.19259259259259,"DER",48860]
[null,null,null,null,null,null,null,null,null,null,"37.04.48","TUBO CONCRETO D=0,60M ASSENTAMENTO","m",55.31,40.97037037037037,"DER",55310]
[null,null,null,null,null,null,null,null,null,null,"37.04.49","TUBO CONCRETO D=0,80M ASSENTAMENTO","m",75.99,56.288888888888884,"DER",75990]
[null,null,null,null,null,null,null,null,null,null,"37.04.50","TUBO CONCRETO D=1,00M ASSENTAMENTO","m",93.57,69.3111111111111,"DER",93570]
[null,null,null,null,null,null,null,null,null,null,"37.04.51","TUBO CONCRETO D=1,20M ASSENTAMENTO","m",155.04,114.84444444444443,"DER",155040]
[null,null,null,null,null,null,null,null,null,null,"37.04.52","TUBO CONCRETO D=1,50M ASSENTAMENTO","m",235.87,174.71851851851852,"DER",235870]
[null,null,null,null,null,null,null,null,null,null,"37.04.53","GABIAO TIPO CAIXA LARG.50CM - TELA GALV.","m³",382.7,283.48148148148147,"DER",382700]
[null,null,null,null,null,null,null,null,null,null,"37.04.54","GABIAO TIPO COLCHAO ESPES.17CM-TELA GALV","m²",104.78,77.6148148148148,"DER",104780]
[null,null,null,null,null,null,null,null,null,null,"37.04.55","GABIAO TIPO COLCHAO ESPES.23CM-TELA GALV","m²",120.62,89.34814814814814,"DER",120620]
[null,null,null,null,null,null,null,null,null,null,"37.04.56","GABIAO TIPO COLCHAO ESPES.30CM-TELA GALV","m²",137.11,101.56296296296297,"DER",137110]
[null,null,null,null,null,null,null,null,null,null,"37.04.57","GABIAO TIPO COLCHAO ESPES.17CM-TELA PVC","m²",120.18,89.02222222222223,"DER",120180]
[null,null,null,null,null,null,null,null,null,null,"37.04.58","GABIAO TIPO COLCHAO ESPES.23CM-TELA PVC","m²",134.85,99.88888888888887,"DER",134850]
[null,null,null,null,null,null,null,null,null,null,"37.04.59","GABIAO TIPO COLCHAO ESPES.30CM-TELA PVC","m²",152.78,113.17037037037036,"DER",152780]
[null,null,null,null,null,null,null,null,null,null,"37.04.60","GABIAO TIPO SACO - TELA GALV.","m³",345.79,256.14074074074074,"DER",345790]
[null,null,null,null,null,null,null,null,null,null,"37.04.61","CAMADA FILTRANTE PEDRA BRITADA","m³",120.15,89,"DER",120150]
[null,null,null,null,null,null,null,null,null,null,"37.04.62","CANALETA CONCRETO 40CM","m",43.1,31.925925925925924,"DER",43100]
[null,null,null,null,null,null,null,null,null,null,"37.04.63","CANALETA CONCRETO 60CM","m",69.7,51.629629629629626,"DER",69700]
[null,null,null,null,null,null,null,null,null,null,"37.04.64","CANALETA CONCRETO 80CM","m",133.62,98.97777777777777,"DER",133620]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.04.65","TUBO PVC PERFURADO OU NAO D=0,050M","m",20.06,14.859259259259257,"DER",20060]
[null,null,null,null,null,null,null,null,null,null,"37.04.66","TUBO PVC PERFURADO OU NAO D=0,10M","m",36.29,26.88148148148148,"DER",36290]
[null,null,null,null,null,null,null,null,null,null,"37.04.67","TUBO PVC PERFURADO OU NAO D=0,15M","m",73.33,54.318518518518516,"DER",73330]
[null,null,null,null,null,null,null,null,null,null,"37.04.68","MANTA GEOTEXTIL NAO TECIDA","kg",23.73,17.577777777777776,"DER",23730]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.01","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 7KN/M","m²",4.67,3.459259259259259,"DER",4670]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.02","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 8KN/M","m²",5.02,3.718518518518518,"DER",5020]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.03","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 9KN/M","m²",5.79,4.288888888888889,"DER",5790]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.04","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 10 KN/M","m²",6.34,4.696296296296296,"DER",6340]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.05","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 14 KN/M","m²",7.68,5.688888888888888,"DER",7680]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.06","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 16 KN/M","m²",9,6.666666666666666,"DER",9000]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.07","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 21 KN/M","m²",11.66,8.637037037037036,"DER",11660]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.08","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 26 KN/M","m²",14.31,10.6,"DER",14310]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.09","MANTA GEOTEXTIL NAO TECIDA RESISTENCIA LONGITUDINAL 31 KN/M","m²",16.95,12.555555555555554,"DER",16950]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.10","MANTA GEOTEXTIL TECIDA RESISTENCIA LONGITUDINAL 24 KN/M","m²",6.53,4.837037037037037,"DER",6530]
[null,null,null,null,null,null,null,null,null,null,"37.04.68.11","MANTA GEOTEXTIL TECIDA RESISTENCIA LONGITUDINAL 48 KN/M","m²",10.19,7.548148148148147,"DER",10190]
[null,null,null,null,null,null,null,null,null,null,"37.04.69","MANTA GEOTEXTIL TECIDA","kg",35.21,26.08148148148148,"DER",35210]
[null,null,null,null,null,null,null,null,null,null,"37.04.70","ENCHIMENTO DE VALA COM AREIA LAVADA","m³",131.19,97.17777777777776,"DER",131190]
[null,null,null,null,null,null,null,null,null,null,"37.04.71","ENCHIMENTO DE VALA COM PEDRA BRITADA 3E4","m³",105.19,77.91851851851851,"DER",105190]
[null,null,null,null,null,null,null,null,null,null,"37.04.72","ENCHIMENTO DE VALA COM PEDRA RACHAO","m³",91.66,67.89629629629628,"DER",91660]
[null,null,null,null,null,null,null,null,null,null,"37.04.73","TUBO ACO CORRUGADO GALV.MET.NAO DESTRUT.","kg",30.56,22.637037037037036,"DER",30560]
[null,null,null,null,null,null,null,null,null,null,"37.04.74","TUBO ACO CORR.EPOXI MET.NAO DESTRUTIVO","kg",31.44,23.288888888888888,"DER",31440]
[null,null,null,null,null,null,null,null,null,null,"37.04.75","TUBO ACO CORR.GALV.MET.DESTRUTIVO","kg",17.21,12.748148148148148,"DER",17210]
[null,null,null,null,null,null,null,null,null,null,"37.04.76","TUBO ACO CORR.EPOXI MET. DESTRUTIVO","kg",18.61,13.785185185185183,"DER",18610]
[null,null,null,null,null,null,null,null,null,null,"37.05.04","SUPORTE MADEIRA TRATADA 0,10X0,10M","m",74.29,55.02962962962963,"DER",74290]
[null,null,null,null,null,null,null,null,null,null,"37.05.05","SUPORTE DE PERFIL METALICO GALVANIZADO","kg",18.71,13.85925925925926,"DER",18710]
[null,null,null,null,null,null,null,null,null,null,"37.05.06","SUPORTE DE TUBO GALVANIZADO D=2 1/2\"","m",81.51,60.37777777777778,"DER",81510]
[null,null,null,null,null,null,null,null,null,null,"37.05.07","SUBSTITUICAO DE DEFENSA SEMI-MALEAVEL","m",54.75,40.55555555555555,"DER",54750]
[null,null,null,null,null,null,null,null,null,null,"37.05.08","DEFENSA SEMI-MALEAVEL SIMPLES-FORNECIMEN","m",198,146.66666666666666,"DER",198000]
[null,null,null,null,null,null,null,null,null,null,"37.05.09","DEFENSA SEMI-MALEAVEL SIMPLES-INST","m",32.27,23.903703703703705,"DER",32270]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.05.10.01","TACHA REFLETIVA MONODIRECIONAL TIPO III OU IV ABNT (VIDRO OU PRISMATICA)","un",24.88,18.429629629629627,"DER",24880]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.05.11.01","TACHA REFLETIVA BIDIRECIONAL TIPO III OU ABNT (VIDRO OU PRISMATICA)","un",30.35,22.48148148148148,"DER",30350]
[null,null,null,null,null,null,null,null,null,null,"37.05.12","TACHAO MONODIRECIONAL REFLETIVO DE VIDRO","un",45.79,33.91851851851852,"DER",45790]
[null,null,null,null,null,null,null,null,null,null,"37.05.14","MINI TACHAO MONODIRECIONAL REFL.VIDRO","un",43.09,31.918518518518518,"DER",43090]
[null,null,null,null,null,null,null,null,null,null,"37.05.15","MINI TACHAO BIDIRECIONAL REFL.VIDRO","un",44.85,33.22222222222222,"DER",44850]
[null,null,null,null,null,null,null,null,null,null,"37.05.16","TACHA MONODIRECIONAL REFLETIVO PLASTICO","un",14.23,10.540740740740741,"DER",14230]
[null,null,null,null,null,null,null,null,null,null,"37.05.17","TACHA BIDIRECIONAL REFLETIVO PLASTICO","un",15.92,11.792592592592591,"DER",15920]
[null,null,null,null,null,null,null,null,null,null,"37.05.20","SINALIZ.HORIZ.ACRIL.BASE DE AGUA","m²",18.72,13.866666666666665,"DER",18720]
[null,null,null,null,null,null,null,null,null,null,"37.05.20.01","SINALIZ.HOR.TINTA P/ POUCO TRAFEGO","m²",15.19,11.251851851851852,"DER",15190]
[null,null,null,null,null,null,null,null,null,null,"37.05.20.02","RENOV.TINTA RES.ACRIL./VINILICA","m²",20.19,14.955555555555556,"DER",20190]
[null,null,null,null,null,null,null,null,null,null,"37.05.20.03","RENOS.MAT.TERMOPL.ASPERSAO","m²",49.32,36.53333333333333,"DER",49320]
[null,null,null,null,null,null,null,null,null,null,"37.05.20.04","RENOV.MAT.TERMOPL.EXTRUSAO","m²",57.1,42.2962962962963,"DER",57100]
[null,null,null,null,null,null,null,null,null,null,"37.05.21","SINALIZ.HORIZ.ACRIL.BASE AGUA C/VISIBE.","m²",22.86,16.933333333333334,"DER",22860]
[null,null,null,null,null,null,null,null,null,null,"37.05.26","RETIRADA DE PLACA DE SOLO EM SUPORTE DE MADEIRA OU METALICO.","m²",37.77,27.977777777777778,"DER",37770]
[null,null,null,null,null,null,null,null,null,null,"37.05.27","RETIRADA DE PLACA AEREA","m²",50.42,37.34814814814815,"DER",50420]
[null,null,null,null,null,null,null,null,null,null,"37.05.28","COLOCACAO DE PLACA EM SUPORTE DE MADEIRA OU METALICO - SOLO","m²",44.06,32.63703703703704,"DER",44060]
[null,null,null,null,null,null,null,null,null,null,"37.05.29","COLOCACAO DE PLACA AEREA EM PORTICOS OU SEMI-PORTICOS.","m²",63.03,46.68888888888889,"DER",63030]
[null,null,null,null,null,null,null,null,null,null,"37.05.30","FORNECIMENTO E TRANSPORTE DE PLACA DE ACO GT+GT.","m²",710.78,526.5037037037036,"DER",710780]
[null,null,null,null,null,null,null,null,null,null,"37.05.31","FORNECIMENTO E TRANSPORTE DE PLACA MOD. ALUMINIO GT+GT.","m²",972.46,720.3407407407407,"DER",972460]
[null,null,null,null,null,null,null,null,null,null,"37.05.32.01","FORN.E COL.PL.AL.MOD.GT+AI PORT/SEMI PORT","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.143,180"]
[null,null,null,null,null,null,null,null,null,null,"37.05.33","FORN. E IMPLANT. DE BRACO PROJ. E PLACA AEREA GT-GT","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","6.938,790"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.05.34.01","FORNECIMENTO E INSTALACAO DE SEMI-PORTICO TUBULAR COM BRACO DE 5,10M","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","18.166,030"]
[null,null,null,null,null,null,null,null,null,null,"37.05.36.01","DISP.MARCADOR ALINHAM-BARR.PLAST.BICOLOR","un",654.68,484.9481481481481,"DER",654680]
[null,null,null,null,null,null,null,null,null,null,"37.05.36.02","DISP.MARC.ALINH.-CILINDRO CANAL. TRAFEGO","un",379.96,281.4518518518518,"DER",379960]
[null,null,null,null,null,null,null,null,null,null,"37.05.36.03","DISP.DELIMITADOR-BALIZADOR CIL.C/PEL.AI","un",379.96,281.4518518518518,"DER",379960]
[null,null,null,null,null,null,null,null,null,null,"37.05.36.04","DISP.MARCADOR ALINH-BAIA P/BALIZ.SIMPLES","un",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.399,450"]
[null,null,null,null,null,null,null,null,null,null,"37.05.36.05","LAMELA ANT. DEFENSA H=0,80M","m",252.64,187.1407407407407,"DER",252640]
[null,null,null,null,null,null,null,null,null,null,"37.05.36.06","DISPOSITIVO DELIMITADOR-BALIZADOR DE SOLO","un",119.49,88.5111111111111,"DER",119490]
[null,null,null,null,null,null,null,null,null,null,"37.06.01","GRAMA EM PLACA SEM ADUBO","m²",6.56,4.859259259259258,"DER",6560]
[null,null,null,null,null,null,null,null,null,null,"37.06.02","GRAMA EM PLACA COM ADUBO","m²",7.34,5.437037037037037,"DER",7340]
[null,null,null,null,null,null,null,null,null,null,"37.06.03","ROCADA MANUAL","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.203,110"]
[null,null,null,null,null,null,null,null,null,null,"37.06.04","ROCADA MECANICA","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.145,080"]
[null,null,null,null,null,null,null,null,null,null,"37.06.05","CAPINA MANUAL","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.716,980"]
[null,null,null,null,null,null,null,null,null,null,"37.06.06","CAPINA QUIMICA","m²",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,420"]
[null,null,null,null,null,null,null,null,null,null,"37.06.07","CONSERVACAO MANUAL DE ACEIRO","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.961,830"]
[null,null,null,null,null,null,null,null,null,null,"37.06.08","DESPRAGUEJAMENTO MANUAL DE GRAMADO","ha",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.484,060"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"37.06.09","REMOCAO LIXO ENTULHO","equipe.hor",268.42,198.82962962962964,"DER",268420]
[null,null,null,null,null,null,null,null,null,null,"37.28.08.01.01","CONFECCAO, MONTAGEM E INSTALACAO DE PLACA INSTITUCIONAL","m²",166.87,123.60740740740741,"DER",166870]
[null,null,null,null,null,null,null,null,null,null,"37.28.08.02.01","MANUTENCAO DE PLACA INSTITUCIONAL","m² x mes",36.26,26.859259259259257,"DER",36260]
[null,null,null,null,null,null,null,null,null,null,"72.01.01.01","ACAB.CONCRETO DE SUPERF.B-436 - COND. A","hora",27.56,20.41481481481481,"DER",27560]
[null,null,null,null,null,null,null,null,null,null,"72.01.01.02","ACAB.CONCRETO DE SUPERF.B-436 - COND. B","hora",7.47,5.533333333333333,"DER",7470]
[null,null,null,null,null,null,null,null,null,null,"72.01.01.03","ACAB.CONCRETO DE SUPERF.B-436 - COND. C","hora",27.29,20.21481481481481,"DER",27290]
[null,null,null,null,null,null,null,null,null,null,"72.01.01.04","ACAB. CONCRETO DE SUPERF.B-436 - COND. D","hora",50.71,37.56296296296296,"DER",50710]
[null,null,null,null,null,null,null,null,null,null,"72.01.02.01","ACAB.DE CONCRETO SUPERF.BG-38 - COND. A","hora",25.95,19.22222222222222,"DER",25950]
[null,null,null,null,null,null,null,null,null,null,"72.01.02.02","ACAB.DE CONCRETO SUPERF.BG-38 - COND. B","hora",5.02,3.718518518518518,"DER",5020]
[null,null,null,null,null,null,null,null,null,null,"72.01.02.03","ACAB.DE CONCRETO SUPERF.BG-38 - COND. C","hora",7.98,5.911111111111111,"DER",7980]
[null,null,null,null,null,null,null,null,null,null,"72.01.02.04","ACAB.DE CONCRETO SUPERF.BG-38 - COND. D","hora",31.4,23.259259259259256,"DER",31400]
[null,null,null,null,null,null,null,null,null,null,"72.02.01.01","VEICULO C/CAPAC.P/4 PES.1.600CC COND. A","hora",25.99,19.25185185185185,"DER",25990]
[null,null,null,null,null,null,null,null,null,null,"72.02.01.02","VEICULO C/CAPAC.P/4 PES.1600CC COND. B","hora",6.68,4.948148148148148,"DER",6680]
[null,null,null,null,null,null,null,null,null,null,"72.02.01.03","VEICULO C/CAPAC.P/4 PES.1600CC COND. C","hora",39.54,29.288888888888888,"DER",39540]
[null,null,null,null,null,null,null,null,null,null,"72.02.01.04","VEICULO C/CAPAC.P/4 PES.1.600CC COND. D","hora",61.9,45.85185185185185,"DER",61900]
[null,null,null,null,null,null,null,null,null,null,"72.02.01.05","VEICULO C/CAPAC.P/4 PES. 1.600CC COND. E","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,600"]
[null,null,null,null,null,null,null,null,null,null,"72.02.01.06","VEICULO C/CAPAC.P/4 PES. 1.600CC COND F","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.387,380"]
[null,null,null,null,null,null,null,null,null,null,"72.02.02.01","VEICULO C/CAPAC.P/4 PES. 1.000CC COND. A","hora",24.29,17.99259259259259,"DER",24290]
[null,null,null,null,null,null,null,null,null,null,"72.02.02.02","VEICULO C/CAPAC.P/4 PES. 1.000CC COND. B","hora",3.54,2.6222222222222222,"DER",3540]
[null,null,null,null,null,null,null,null,null,null,"72.02.02.03","VEICULO C/CAPAC.P/4 PES. 1.000CC COND. C","hora",31.4,23.259259259259256,"DER",31400]
[null,null,null,null,null,null,null,null,null,null,"72.02.02.04","VEICULO C/CAPAC.P/4 PES. 1.000CC COND. D","hora",53.77,39.82962962962963,"DER",53770]
[null,null,null,null,null,null,null,null,null,null,"72.02.02.05","VEICULO C/CAPAC.P/4 PES. 1.000CC COND. E","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,480"]
[null,null,null,null,null,null,null,null,null,null,"72.02.02.06","VEICULO C/CAPAC.P/4 PES.1000CC COND. F","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","2.526,330"]
[null,null,null,null,null,null,null,null,null,null,"72.02.03.01","VEIC.UTIL.09 PESSOAS 1.600CC COND.A","hora",26.44,19.585185185185185,"DER",26440]
[null,null,null,null,null,null,null,null,null,null,"72.02.03.02","VEIC.UTIL.09 PESSOAS 1.600CC COND.B","hora",7.52,5.5703703703703695,"DER",7520]
[null,null,null,null,null,null,null,null,null,null,"72.02.03.03","VEIC.UTIL.09 PESSOAS 1.600CC COND.C","hora",46.75,34.629629629629626,"DER",46750]
[null,null,null,null,null,null,null,null,null,null,"72.02.03.04","VEIC.UTIL.09 PESSOAS 1.600CC COND.D","hora",69.12,51.2,"DER",69120]
[null,null,null,null,null,null,null,null,null,null,"72.02.03.05","VEIC.UTIL.09 PESSOAS 1.600CC COND.E","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,720"]
[null,null,null,null,null,null,null,null,null,null,"72.02.03.06","VEIC.UTIL.09 PESSOAS 1.600CC COND. F","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.619,900"]
[null,null,null,null,null,null,null,null,null,null,"72.02.04.01","VEICULO UTIL.CAMIONETE P/3 PES. COND. A","hora",29.07,21.53333333333333,"DER",29070]
[null,null,null,null,null,null,null,null,null,null,"72.02.04.02","VEICULO UTIL.CAMIONETE P/3 PES. COND. B","hora",12.11,8.97037037037037,"DER",12110]
[null,null,null,null,null,null,null,null,null,null,"72.02.04.03","VEICULO UTIL.CAMIONETE P/3 PES. COND. C","hora",59.74,44.25185185185185,"DER",59740]
[null,null,null,null,null,null,null,null,null,null,"72.02.04.04","VEICULO UTIL.CAMIONETE P/3 PES. COND. D","hora",82.11,60.822222222222216,"DER",82110]
[null,null,null,null,null,null,null,null,null,null,"72.02.04.05","VEICULO UTIL.CAMIONETE P/ 3 PES. COND. E","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,950"]
[null,null,null,null,null,null,null,null,null,null,"72.02.04.06","VEICULO UTIL.CAMIONETE P/3 PES.COND. F","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.072,790"]
[null,null,null,null,null,null,null,null,null,null,"72.02.05.01","VEICULO DE PREMARCACAO - COND. A","hora",45.22,33.49629629629629,"DER",45220]
[null,null,null,null,null,null,null,null,null,null,"72.02.05.02","VEICULO DE PREMARCACAO - COND. B","hora",8.38,6.207407407407407,"DER",8380]
[null,null,null,null,null,null,null,null,null,null,"72.02.05.03","VEICULO DE PREMARCACAO - COND. C","hora",36.76,27.229629629629628,"DER",36760]
[null,null,null,null,null,null,null,null,null,null,"72.02.05.04","VEICULO DE PREMARCACAO - COND. D","hora",77.9,57.7037037037037,"DER",77900]
[null,null,null,null,null,null,null,null,null,null,"72.02.08.01","VEICULO PEQUENO 1.6CC COM AR E DIRECAO HIDRAULICA - CONDICAO A","hora",26.81,19.859259259259257,"DER",26810]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.02.08.02","VEICULO PEQUENO 1.6CC COM AR E DIRECAO HIDRAULICA - CONDICAO B","hora",8.59,6.362962962962962,"DER",8590]
[null,null,null,null,null,null,null,null,null,null,"72.02.08.03","VEICULO PEQUENO 1.6CC COM AR E DIRECAO HIDRAULICA - CONDICAO C","hora",41.45,30.703703703703702,"DER",41450]
[null,null,null,null,null,null,null,null,null,null,"72.02.08.04","VEICULO C/ CAP.P/4.PESSOAS 1.600CC C/ AR + DIR.HID. + AIR BAG - COND.D","hora",63.81,47.266666666666666,"DER",63810]
[null,null,null,null,null,null,null,null,null,null,"72.02.08.05","VEICULO PEQUENO 1.6CC COM AR E DIRECAO HIDRAULICA - CONDICAO E","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,600"]
[null,null,null,null,null,null,null,null,null,null,"72.02.08.06","VEICULO PEQUENO 1.6CC COM AR E DIRECAO HIDRAULICA - CONDICAO F","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","3.329,060"]
[null,null,null,null,null,null,null,null,null,null,"72.02.09.01","VEICULO UTILITARIO COM MINIMO DE 10 LUGARES COM AR E DIR. HID.","hora",31.05,23,"DER",31050]
[null,null,null,null,null,null,null,null,null,null,null,"CONDICAO A",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.02.09.02","VEICULO UTILITARIO COM MINIMO DE 10 LUGARES COM AR E DIR. HID.","hora",16.01,11.85925925925926,"DER",16010]
[null,null,null,null,null,null,null,null,null,null,null,"CONDICAOB",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.02.09.03","VEICULO UTILITARIO COM MINIMO DE 10 LUGARES COM AR E DIR. HID.","hora",55.24,40.91851851851852,"DER",55240]
[null,null,null,null,null,null,null,null,null,null,null,"CONDICAO C",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.02.09.04","VEICULO UTILITARIO C/MIN.10LUGARES C/ AR + DIR.HID. COND.D","hora",77.61,57.48888888888889,"DER",77610]
[null,null,null,null,null,null,null,null,null,null,"72.02.09.05","VEICULO UTILITARIO COM MINIMO DE 10 LUGARES COM AR E DIR. HID.","km",1.06,0.7851851851851852,"DER",1060]
[null,null,null,null,null,null,null,null,null,null,null,"CONDICAOE",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.02.09.06","VEICULO UTILITARIO COM MINIMO DE 10 LUGARES COM AR E DIR. HID.","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.952,650"]
[null,null,null,null,null,null,null,null,null,null,null,"CONDICAOF",null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.02.10.01","VEICULO UTILITARIO PICK-UP COM AR E DIR. HID. CONDICAO A","hora",28.9,21.407407407407405,"DER",28900]
[null,null,null,null,null,null,null,null,null,null,"72.02.10.02","VEICULO UTILITARIO PICK-UP COM AR E DIR. HID. CONDICAOB","hora",11.79,8.733333333333333,"DER",11790]
[null,null,null,null,null,null,null,null,null,null,"72.02.10.03","VEICULO UTILITARIO PICK-UP COM AR E DIR. HID. CONDICAO C","hora",59.42,44.01481481481481,"DER",59420]
[null,null,null,null,null,null,null,null,null,null,"72.02.10.04","VEICULO UTILITARIO CAMIONETE P/3 PESSOAS C/ AR + DIR.HID.+ AIRBAG","hora",81.79,60.58518518518519,"DER",81790]
[null,null,null,null,null,null,null,null,null,null,"72.02.10.05","VEICULO UTILITARIO PICK-UP COM AR E DIR. HID. CONDICAO E","km",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,940"]
[null,null,null,null,null,null,null,null,null,null,"72.02.10.06","VEICULO UTILITARIO PICK-UP COM AR E DIR. HID. CONDICAOF","veic.mens",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","5.036,300"]
[null,null,null,null,null,null,null,null,null,null,"72.03.01.01","BATE ESTACA 40 ATE 80 T - COND. A","hora",55.38,41.02222222222222,"DER",55380]
[null,null,null,null,null,null,null,null,null,null,"72.03.01.02","BATE ESTACA 40 ATE 80 T - COND. B","hora",22.84,16.918518518518518,"DER",22840]
[null,null,null,null,null,null,null,null,null,null,"72.03.01.03","BATE ESTACA 40 ATE 80 T - COND. C","hora",77.99,57.770370370370365,"DER",77990]
[null,null,null,null,null,null,null,null,null,null,"72.03.01.04","BATE ESTACA 40 ATE 80 T - COND. D","hora",119.14,88.25185185185185,"DER",119140]
[null,null,null,null,null,null,null,null,null,null,"72.03.02.01","BATE ESTACA ATE 40T COND. A","hora",54.48,40.35555555555555,"DER",54480]
[null,null,null,null,null,null,null,null,null,null,"72.03.02.02","BATE ESTACA ATE 40T CONDI. B","hora",21.39,15.844444444444443,"DER",21390]
[null,null,null,null,null,null,null,null,null,null,"72.03.02.03","BATE ESTACA ATE 40T COND. C","hora",42.96,31.82222222222222,"DER",42960]
[null,null,null,null,null,null,null,null,null,null,"72.03.02.04","BATE ESTACA ATE 40T COND. D","hora",84.11,62.3037037037037,"DER",84110]
[null,null,null,null,null,null,null,null,null,null,"72.04.01.01","BETONEIRA 320L MOTOR ELETRICO COND.A","hora",15.38,11.392592592592592,"DER",15380]
[null,null,null,null,null,null,null,null,null,null,"72.04.01.02","BETONEIRA 320L MOTOR ELETRICO COND.B","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,670"]
[null,null,null,null,null,null,null,null,null,null,"72.04.01.03","BETONEIRA 320L MOTOR ELETRICO COND.C","hora",1.65,1.222222222222222,"DER",1650]
[null,null,null,null,null,null,null,null,null,null,"72.04.01.04","BETONEIRA 320L MOTOR ELETRICO COND.D","hora",16.69,12.362962962962962,"DER",16690]
[null,null,null,null,null,null,null,null,null,null,"72.04.02.01","BETONEIRA 320L MOTOR GASOLINA COND. A","hora",15.65,11.592592592592592,"DER",15650]
[null,null,null,null,null,null,null,null,null,null,"72.04.02.02","BETONEIRA 320L MOTOR GASOLINA COND. B","hora",1.22,0.9037037037037037,"DER",1220]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.04.02.03","BETONEIRA 320L MOTOR GASOLINA COND. C","hora",3.9,2.888888888888889,"DER",3900]
[null,null,null,null,null,null,null,null,null,null,"72.04.02.04","BETONEIRA 320L MOTOR GASOLINA COND. D","hora",18.94,14.02962962962963,"DER",18940]
[null,null,null,null,null,null,null,null,null,null,"72.04.03.01","BETONEIRA 580L ELETRICA C/CARREG. COND.A","hora",17.4,12.888888888888888,"DER",17400]
[null,null,null,null,null,null,null,null,null,null,"72.04.03.02","BETONEIRA 580L ELETRICA C/CARREG. COND.B","hora",4.71,3.4888888888888885,"DER",4710]
[null,null,null,null,null,null,null,null,null,null,"72.04.03.03","BETONEIRA 580L ELETRICA C/CARREG. COND.C","hora",7.3,5.4074074074074066,"DER",7300]
[null,null,null,null,null,null,null,null,null,null,"72.04.03.04","BETONEIRA 580L ELETRICA C/CARREG. COND.D","hora",22.34,16.548148148148147,"DER",22340]
[null,null,null,null,null,null,null,null,null,null,"72.04.04.01","BETONEIRA 580L MOTOR A DIESEL COND. A","hora",18.17,13.459259259259259,"DER",18170]
[null,null,null,null,null,null,null,null,null,null,"72.04.04.02","BETONEIRA 580L MOTOR A DIESEL COND. B","hora",6.24,4.622222222222222,"DER",6240]
[null,null,null,null,null,null,null,null,null,null,"72.04.04.03","BETONEIRA 580L MOTOR A DIESEL COND. C","hora",10.18,7.54074074074074,"DER",10180]
[null,null,null,null,null,null,null,null,null,null,"72.04.04.04","BETONEIRA 580L MOTOR A DIESEL - COND. D","hora",25.22,18.68148148148148,"DER",25220]
[null,null,null,null,null,null,null,null,null,null,"72.05.01.01","BOMBA DREN.SUBMER.ELETR.27m³/H COND. A","hora",15.5,11.481481481481481,"DER",15500]
[null,null,null,null,null,null,null,null,null,null,"72.05.01.02","BOMBA DREN.SUBMER.ELETR.27m³/H COND. B","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,760"]
[null,null,null,null,null,null,null,null,null,null,"72.05.01.03","BOMBA DREN.SUBMER.ELETR.27m³/H COND. C","hora",8.78,6.503703703703703,"DER",8780]
[null,null,null,null,null,null,null,null,null,null,"72.05.01.04","BOMBA DREN.SUBMER.ELETR.27m³/H COND. D","hora",23.82,17.644444444444442,"DER",23820]
[null,null,null,null,null,null,null,null,null,null,"72.05.02.01","BOMBA DREN.SUBMER.ELETR.60m³/H COND. A","hora",15.95,11.814814814814813,"DER",15950]
[null,null,null,null,null,null,null,null,null,null,"72.05.02.02","BOMBA DREN.SUBMER.ELETR.60m³/H COND. B","hora",1.51,1.1185185185185185,"DER",1510]
[null,null,null,null,null,null,null,null,null,null,"72.05.02.03","BOMBA DREN.SUBMER.ELETR.60m³/H COND. C","hora",8.56,6.340740740740741,"DER",8560]
[null,null,null,null,null,null,null,null,null,null,"72.05.02.04","BOMBA DREN.SUBMER.ELETR.60m³/H COND. D","hora",23.6,17.48148148148148,"DER",23600]
[null,null,null,null,null,null,null,null,null,null,"72.05.03.01","BOMBA DREN.SUBMER.ELETR.144m³/H COND. A","hora",16.85,12.481481481481481,"DER",16850]
[null,null,null,null,null,null,null,null,null,null,"72.05.03.02","BOMBA DREN.SUBMER.ELETR.144m³/H COND. B","hora",3.01,2.2296296296296294,"DER",3010]
[null,null,null,null,null,null,null,null,null,null,"72.05.03.03","BOMBA DREN.SUBMER.ELETR.144m³/H COND. C","hora",11.04,8.177777777777777,"DER",11040]
[null,null,null,null,null,null,null,null,null,null,"72.05.03.04","BOMBA DREN.SUBMER.ELETR.144m³/H COND. D","hora",26.08,19.318518518518516,"DER",26080]
[null,null,null,null,null,null,null,null,null,null,"72.05.04.01","BOMBA DREN.SUBMER.ELETR.180m³/H COND. A","hora",18.21,13.488888888888889,"DER",18210]
[null,null,null,null,null,null,null,null,null,null,"72.05.04.02","BOMBA DREN.SUBMER.ELETR.180m³/H COND. B","hora",5.27,3.903703703703703,"DER",5270]
[null,null,null,null,null,null,null,null,null,null,"72.05.04.03","BOMBA DREN.SUBMER.ELETR.180m³/H COND. C","hora",14.26,10.562962962962962,"DER",14260]
[null,null,null,null,null,null,null,null,null,null,"72.05.04.04","BOMBA DREN.SUBMER.ELETR.180m³/H COND. D","hora",29.3,21.703703703703702,"DER",29300]
[null,null,null,null,null,null,null,null,null,null,"72.05.05.01","BOMBA DREN.SUB.GAS.60.000L/H COND. A","hora",15.52,11.496296296296295,"DER",15520]
[null,null,null,null,null,null,null,null,null,null,"72.05.05.02","BOMBA DREN.SUB.GAS.60.000L/H COND. B","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,800"]
[null,null,null,null,null,null,null,null,null,null,"72.05.05.03","BOMBA DREN.SUB.GAS.60.000L/H COND. C","hora",5.17,3.8296296296296295,"DER",5170]
[null,null,null,null,null,null,null,null,null,null,"72.05.05.04","BOMBA DREN.SUB.GAS.60.000L/H COND. D","hora",20.21,14.97037037037037,"DER",20210]
[null,null,null,null,null,null,null,null,null,null,"72.06.01.01","BOMBA INJ.PROJ.NATA CIM.ARG.1m³/H COND.A","hora",35.4,26.222222222222218,"DER",35400]
[null,null,null,null,null,null,null,null,null,null,"72.06.01.02","BOMBA INJ.PROJ.NATA CIM.ARG.1m³/H COND.B","hora",23.12,17.125925925925927,"DER",23120]
[null,null,null,null,null,null,null,null,null,null,"72.06.01.03","BOMBA INJ.PROJ.NATA CIM.ARG.1m³/H COND.C","hora",86.1,63.77777777777777,"DER",86100]
[null,null,null,null,null,null,null,null,null,null,"72.06.01.04","BOMBA INJ.PROJ.NATA CIM.ARG.1m³/H COND.D","hora",109.53,81.13333333333333,"DER",109530]
[null,null,null,null,null,null,null,null,null,null,"72.06.02.01","BOMBA INJ.PROJ.NATA CIM.ARG.3m³/H COND.A","hora",28.72,21.274074074074072,"DER",28720]
[null,null,null,null,null,null,null,null,null,null,"72.06.02.02","BOMBA INJ.PROJ.NATA CIM.ARG.3m³/H COND.B","hora",10.22,7.57037037037037,"DER",10220]
[null,null,null,null,null,null,null,null,null,null,"72.06.02.03","BOMBA INJ.PROJ.NATA CIM.ARG.3m³/H COND.C","hora",59.97,44.42222222222222,"DER",59970]
[null,null,null,null,null,null,null,null,null,null,"72.06.02.04","BOMBA INJ.PROJ.NATA CIM.ARG.3m³/H COND.D","hora",83.39,61.770370370370365,"DER",83390]
[null,null,null,null,null,null,null,null,null,null,"72.06.03.01","BOM.INJ.PROJ.CONCR.35m³/H COND. A","hora",31.79,23.548148148148147,"DER",31790]
[null,null,null,null,null,null,null,null,null,null,"72.06.03.02","BOM.INJ.PROJ.CONCR.35m³/H COND. B","hora",16.16,11.97037037037037,"DER",16160]
[null,null,null,null,null,null,null,null,null,null,"72.06.03.03","BOM.INJ.PROJ.CONCR.35m³/H COND. C","hora",113.06,83.74814814814815,"DER",113060]
[null,null,null,null,null,null,null,null,null,null,"72.06.03.04","BOM.INJ.PROJ.CONCR.35m³/H COND. D","hora",136.48,101.09629629629629,"DER",136480]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.06.04.01","BOMBA PROJECAO DE CONC.MAN.10m³/H COND.A","hora",34.22,25.348148148148145,"DER",34220]
[null,null,null,null,null,null,null,null,null,null,"72.06.04.02","BOMBA PROJECAO DE CONC.MAN.10m³/H COND.B","hora",20.85,15.444444444444445,"DER",20850]
[null,null,null,null,null,null,null,null,null,null,"72.06.04.03","BOMBA PROJECAO DE CONC.MAN.10m³/H COND.C","hora",117.66,87.15555555555555,"DER",117660]
[null,null,null,null,null,null,null,null,null,null,"72.06.04.04","BOMBA PROJECAO DE CONC.MAN.10m³/H COND.D","hora",141.09,104.5111111111111,"DER",141090]
[null,null,null,null,null,null,null,null,null,null,"72.06.05.01","BOM.PROJ.CONC.C/LANCA TEL.23m³/H COND.A","hora",55.58,41.170370370370364,"DER",55580]
[null,null,null,null,null,null,null,null,null,null,"72.06.05.02","BOM.PROJ.CONC.C/LANCA TEL.23m³/H COND.B","hora",62.09,45.992592592592594,"DER",62090]
[null,null,null,null,null,null,null,null,null,null,"72.06.05.03","BOM.PROJ.CONC.C/LANCA TEL.23m³/H COND.C","hora",310.94,230.3259259259259,"DER",310940]
[null,null,null,null,null,null,null,null,null,null,"72.06.05.04","BOM.PROJ.CONC.C/LANCA TEL 23m³/H COND.D","hora",334.36,247.67407407407407,"DER",334360]
[null,null,null,null,null,null,null,null,null,null,"72.07.01.01","BOMBA HIDRAULICA PARA PROTENSAO COND.A","hora",25.48,18.874074074074073,"DER",25480]
[null,null,null,null,null,null,null,null,null,null,"72.07.01.02","BOMBA HIDRAULICA PARA PROTENSAO COND.B","hora",4.45,3.2962962962962963,"DER",4450]
[null,null,null,null,null,null,null,null,null,null,"72.07.01.03","BOMBA HIDRAULICA PARA PROTENSAO COND.C","hora",4.78,3.5407407407407407,"DER",4780]
[null,null,null,null,null,null,null,null,null,null,"72.07.01.04","BOMBA HIDRAULICA PARA PROTENSAO COND.D","hora",28.2,20.888888888888886,"DER",28200]
[null,null,null,null,null,null,null,null,null,null,"72.07.02.01","MACACO PARA PROTENSAO AU-1 COND. A","hora",1.95,1.4444444444444444,"DER",1950]
[null,null,null,null,null,null,null,null,null,null,"72.07.02.02","MACACO PARA PROTENSAO AU-1 COND. B","hora",4.22,3.1259259259259253,"DER",4220]
[null,null,null,null,null,null,null,null,null,null,"72.07.02.03","MACACO PARA PROTENSAO AU-1 COND. C","hora",4.22,3.1259259259259253,"DER",4220]
[null,null,null,null,null,null,null,null,null,null,"72.07.02.04","MACACO PARA PROTENCAO AU-1 COND. D","hora",4.22,3.1259259259259253,"DER",4220]
[null,null,null,null,null,null,null,null,null,null,"72.07.03.01","MACACO PROTENSAO AU-5 COND. A","hora",1.88,1.3925925925925924,"DER",1880]
[null,null,null,null,null,null,null,null,null,null,"72.07.03.02","MACACO PROTENSAO AU-5 COND. B","hora",4.07,3.0148148148148146,"DER",4070]
[null,null,null,null,null,null,null,null,null,null,"72.07.03.03","MACACO PROTENSAO AU-5 COND. C","hora",4.07,3.0148148148148146,"DER",4070]
[null,null,null,null,null,null,null,null,null,null,"72.07.03.04","MACACO PROTENSAO AU-5 COND. D","hora",4.07,3.0148148148148146,"DER",4070]
[null,null,null,null,null,null,null,null,null,null,"72.07.06.01","MACACO PROTENSAO S-6 COND. A","hora",2.05,1.5185185185185184,"DER",2050]
[null,null,null,null,null,null,null,null,null,null,"72.07.06.02","MACACO PROTENSAO S-6 COND. B","hora",4.43,3.281481481481481,"DER",4430]
[null,null,null,null,null,null,null,null,null,null,"72.07.06.03","MACACO PROTENSAO S-6 COND. C","hora",4.43,3.281481481481481,"DER",4430]
[null,null,null,null,null,null,null,null,null,null,"72.07.06.04","MACACO PROTENSAO S-6 COND. D","hora",4.43,3.281481481481481,"DER",4430]
[null,null,null,null,null,null,null,null,null,null,"72.07.07.01","MACACO PROTENSAO K-350 COND. A","hora",2.34,1.7333333333333332,"DER",2340]
[null,null,null,null,null,null,null,null,null,null,"72.08.01.03","CAMINHAO IRRIGADEIRA 6000L COND. C","hora",97.01,71.85925925925926,"DER",97010]
[null,null,null,null,null,null,null,null,null,null,"72.08.02.03","CAMINHAO IRRIGADEIRA 9000L COND. C","hora",103.62,76.75555555555556,"DER",103620]
[null,null,null,null,null,null,null,null,null,null,"72.09.01.04","CAMINHAO BASCULANTE 5m³ COND. D","hora",114.21,84.6,"DER",114210]
[null,null,null,null,null,null,null,null,null,null,"72.09.01.05","CAMINHAO BASCULANTE 5m³ COND. E","km",2.15,1.5925925925925923,"DER",2150]
[null,null,null,null,null,null,null,null,null,null,"72.09.02.05","CAMINHAO BASCULANTE 8m³ COND. E","km",2.63,1.948148148148148,"DER",2630]
[null,null,null,null,null,null,null,null,null,null,"72.10.01.01","CAMINHAO BASC.FORA ESTR. 18,3m³ COND. A","hora",75.02,55.57037037037036,"DER",75020]
[null,null,null,null,null,null,null,null,null,null,"72.11.01.02","CAMINHAO BETONEIRA 5m³ COND. B","hora",46.82,34.68148148148148,"DER",46820]
[null,null,null,null,null,null,null,null,null,null,"72.11.02.03","CAMINHAO BETONEIRA 7m³ COND. C","hora",147.48,109.24444444444443,"DER",147480]
[null,null,null,null,null,null,null,null,null,null,"72.11.03.03","CAMINHAO P/BOMBEAMENTO DE CONC. COND. C","hora",189.07,140.05185185185184,"DER",189070]
[null,null,null,null,null,null,null,null,null,null,"72.11.03.05","CAMINHAO P/BOMBEAMENTO DE CONC. COND. E","km",3.99,2.9555555555555557,"DER",3990]
[null,null,null,null,null,null,null,null,null,null,"72.12.01.05","CAMINHAO CARROC. MADEIRA 4,5 T COND. E","km",1.92,1.422222222222222,"DER",1920]
[null,null,null,null,null,null,null,null,null,null,"72.12.02.05","CAMINHAO CARROC. MADEIRA 8,0 TON COND. E","km",2.27,1.6814814814814814,"DER",2270]
[null,null,null,null,null,null,null,null,null,null,"72.12.03.02","CAMINHAO CARROC. MADEIRA 10,5T COND. B","hora",33.37,24.718518518518515,"DER",33370]
[null,null,null,null,null,null,null,null,null,null,"72.12.04.02","CAMINHAO PARA LUBRIFICACAO 3000L COND. B","hora",32.7,24.22222222222222,"DER",32700]
[null,null,null,null,null,null,null,null,null,null,"72.12.05.02","CAMINHAO PARA LUBRIFICACAO 7000L COND. B","hora",42.26,31.3037037037037,"DER",42260]
[null,null,null,null,null,null,null,null,null,null,"72.12.06.03","CAMINHAO ABASTECEDOR COND. C","hora",146.65,108.62962962962963,"DER",146650]
[null,null,null,null,null,null,null,null,null,null,"72.13.01.01","CAMINHAO HIDROSSEMEADOR 5600L COND. A","hora",44.05,32.629629629629626,"DER",44050]
[null,null,null,null,null,null,null,null,null,null,"72.13.01.05","CAMINHAO HIDROSSEMEADOR 5600L COND. E","km",2.38,1.7629629629629628,"DER",2380]
[null,null,null,null,null,null,null,null,null,null,"72.15.01.01","CAMINHAO GUINCHO LANC.TELES.3,75T COND.A","hora",45.42,33.644444444444446,"DER",45420]
[null,null,null,null,null,null,null,null,null,null,"72.15.02.03","CAMINHAO GUINCHO LANC.TELES.4,10T COND.C","hora",119.34,88.39999999999999,"DER",119340]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.15.03.03","CAMINHAO CARROCERIA COM GUINDAUTO 640-18, COND. C","hora",100.89,74.73333333333333,"DER",100890]
[null,null,null,null,null,null,null,null,null,null,"72.15.03.04","CAMINHAO CAR. GUINDAUTO 640-18","hora",124.17,91.97777777777777,"DER",124170]
[null,null,null,null,null,null,null,null,null,null,"72.16.01.05","CAMINHAO C/USINA LAMA ASFAL.10,5T COND.E","km",4.51,3.3407407407407406,"DER",4510]
[null,null,null,null,null,null,null,null,null,null,"72.17.01.01","CAMINHAO PANTOGRAFICO ATE 9M COND. A","hora",42.62,31.570370370370366,"DER",42620]
[null,null,null,null,null,null,null,null,null,null,"72.18.01.02","CAVALO MECANICO C/CARRETA 30000KG COND.B","hora",47.46,35.15555555555555,"DER",47460]
[null,null,null,null,null,null,null,null,null,null,"72.18.02.04","CAVALO MECANICO C/PRANCHA 30000KG COND.D","hora",219.02,162.23703703703703,"DER",219020]
[null,null,null,null,null,null,null,null,null,null,"72.19.01.04","CAMPANULA COND. D","hora",26.23,19.429629629629627,"DER",26230]
[null,null,null,null,null,null,null,null,null,null,"72.20.02.02","COMPACTADOR PLAC.VIB.MAN.1000m²/H COND.B","hora",1.93,1.4296296296296296,"DER",1930]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.21.01.04","COMPRESSOR DE AR XA-90 MWD COND. D","hora",73.95,54.77777777777778,"DER",73950]
[null,null,null,null,null,null,null,null,null,null,"72.21.03.02","COMPRESSOR DE AR XA-175MWD COND. B","hora",19,14.074074074074073,"DER",19000]
[null,null,null,null,null,null,null,null,null,null,"72.21.04.03","COMPRESSOR DE AR XA-360MWD COND. C","hora",162.4,120.29629629629629,"DER",162400]
[null,null,null,null,null,null,null,null,null,null,"72.22.01.02","DEMARCADOR DE FAIXA A FRIO 250L COND.B","hora",53.81,39.85925925925926,"DER",53810]
[null,null,null,null,null,null,null,null,null,null,"72.23.01.03","DISTRIBUIDOR AGREG.S/EST.1000T/H COND. C","hora",44.41,32.89629629629629,"DER",44410]
[null,null,null,null,null,null,null,null,null,null,"72.23.02.04","DISTRIBUIDOR AGREGADO 600T/H COND. D","hora",31.96,23.674074074074074,"DER",31960]
[null,null,null,null,null,null,null,null,null,null,"72.23.03.01","DISTR.ASF.REB.2400L COND. A","hora",26.15,19.370370370370367,"DER",26150]
[null,null,null,null,null,null,null,null,null,null,"72.24.01.03","DISTR. ADUBOS E SEMENTES 700L COND. C","hora",3.94,2.918518518518518,"DER",3940]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.26.01.01","EQUIP.VIS.OAE C/LANC.TELESC.25M COND. A","hora",90.64,67.14074074074074,"DER",90640]
[null,null,null,null,null,null,null,null,null,null,"72.26.03.01","EQUIP.VIST.OAE TP TESOURA 7,62M COND. A","hora",57.16,42.340740740740735,"DER",57160]
[null,null,null,null,null,null,null,null,null,null,"72.27.01.01","ESCAVADEIRA HIDR.S/EST.0,7m³ COND. A","hora",58.01,42.97037037037037,"DER",58010]
[null,null,null,null,null,null,null,null,null,null,"72.27.02.02","ESCAVADEIRA HIDR.S/EST.0,60m³ COND. B","hora",60.55,44.85185185185185,"DER",60550]
[null,null,null,null,null,null,null,null,null,null,"72.27.04.02","ESCAVADEIRA HID.S/EST.2,2m³ COND. B","hora",143.52,106.31111111111112,"DER",143520]
[null,null,null,null,null,null,null,null,null,null,"72.27.05.02","ESCAVADEIRA HIDR.S/PNEU 0,25m³ COND. B","hora",81.4,60.2962962962963,"DER",81400]
[null,null,null,null,null,null,null,null,null,null,"72.28.01.03","EMPILHADEIRA 2500KG COND. C","hora",33.1,24.51851851851852,"DER",33100]
[null,null,null,null,null,null,null,null,null,null,"72.28.02.01","EMPILHADEIRA 5000KG COND. A","hora",44.51,32.97037037037037,"DER",44510]
[null,null,null,null,null,null,null,null,null,null,"72.29.01.02","FRESADORA A FRIO S/PNEUS 150m²/H COND.B","hora",156.13,115.65185185185184,"DER",156130]
[null,null,null,null,null,null,null,null,null,null,"72.29.02.03","FRESADORA A FRIO S/PNEUS 670HP COND. C","hora",518.47,384.05185185185184,"DER",518470]
[null,null,null,null,null,null,null,null,null,null,"72.29.02.04","FRESADORA A FRIO S/PNEUS 670HP COND. D","hora",541.75,401.29629629629625,"DER",541750]
[null,null,null,null,null,null,null,null,null,null,"72.31.01.03","GRUPO GERADOR 40KVA COND. C","hora",27.6,20.444444444444443,"DER",27600]
[null,null,null,null,null,null,null,null,null,null,"72.31.02.03","GRUPO GERADOR 55KVA COND. C","hora",36.07,26.71851851851852,"DER",36070]
[null,null,null,null,null,null,null,null,null,null,"72.31.04.01","GRUPO GERADOR 115KVA COND. A","hora",10.89,8.066666666666666,"DER",10890]
[null,null,null,null,null,null,null,null,null,null,"72.31.05.04","GRUPO GERADOR PORTATIL 3,5KVA COND. D","hora",8.99,6.659259259259259,"DER",8990]
[null,null,null,null,null,null,null,null,null,null,"72.32.01.01","GUINCHO ELETRICO DE COLunA 30M COND. A","hora",23.79,17.62222222222222,"DER",23790]
[null,null,null,null,null,null,null,null,null,null,"72.32.02.02","GUINCHO ELETRICO TIPO ELEV. 30M COND. B","hora",7.28,5.392592592592592,"DER",7280]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.33.02.02","GUIND.HID.LANC.TELES.S/PN.27,2T COND. B","hora",116.9,86.5925925925926,"DER",116900]
[null,null,null,null,null,null,null,null,null,null,"72.34.01.02","LAVA JATO 200L/H COND. B","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,330"]
[null,null,null,null,null,null,null,null,null,null,"72.35.01.03","MARTELETE ROMP.PN.11,2KG COND. C","hora",7.28,5.392592592592592,"DER",7280]
[null,null,null,null,null,null,null,null,null,null,"72.35.02.01","MARTELETE ROMP.PN.35KG COND. A","hora",16.3,12.074074074074074,"DER",16300]
[null,null,null,null,null,null,null,null,null,null,"72.36.01.03","ROMPEDOR/DEMOL.HIDR.P/ESCAVAD. COND. C","hora",115.67,85.68148148148148,"DER",115670]
[null,null,null,null,null,null,null,null,null,null,"72.36.01.04","ROMPEDOR/DEMOL.HIDR.P/ESCAVAD. COND. D","hora",130.71,96.82222222222222,"DER",130710]
[null,null,null,null,null,null,null,null,null,null,"72.37.01.01","MOTONIVELADORA COM RIPPER 140HP COND. A","hora",76.12,56.385185185185186,"DER",76120]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.38.02.01","MOTOSCRAPER 26m³ COND. A","hora",86.25,63.888888888888886,"DER",86250]
[null,null,null,null,null,null,null,null,null,null,"72.39.02.02","MAQUINA SOLDA A DIESEL ATE 375A COND.B","hora",12.59,9.325925925925926,"DER",12590]
[null,null,null,null,null,null,null,null,null,null,"72.39.03.01","MACARICO DE CORTE COND. A","hora",15.07,11.162962962962963,"DER",15070]
[null,null,null,null,null,null,null,null,null,null,"72.40.01.02","TEODOLITO COM TRIPE COND. B","hora",1.59,1.1777777777777778,"DER",1590]
[null,null,null,null,null,null,null,null,null,null,"72.40.03.01","NIVEL COM TRIPE COND. A","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,860"]
[null,null,null,null,null,null,null,null,null,null,"72.41.01.02","PA CARREG.S/PNEUS 1,7m³ A 1,9m³ - COND.B","hora",56.2,41.629629629629626,"DER",56200]
[null,null,null,null,null,null,null,null,null,null,"72.41.02.03","PA CARREG.S/PNEUS 1,91m³ A 2,5m³ -COND.C","hora",110.22,81.64444444444443,"DER",110220]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.41.04.03","PA CARREG. S/ESTEIRA 1,85m³ COND. C","hora",168.55,124.85185185185185,"DER",168550]
[null,null,null,null,null,null,null,null,null,null,"72.41.05.04","PA CARREGADEIRA S/EST.2,3m³ COND. D","hora",241.94,179.21481481481482,"DER",241940]
[null,null,null,null,null,null,null,null,null,null,"72.42.02.04","PERFURATRIZ S/ESTEIRA COND. D","hora",391.77,290.2,"DER",391770]
[null,null,null,null,null,null,null,null,null,null,"72.42.03.04","PERFURATRIZ JUMBO 3 BRACOS COND. D","hora",561.67,416.0518518518518,"DER",561670]
[null,null,null,null,null,null,null,null,null,null,"72.42.05.01","PERFURADOR/CINZAL DE BAIXO PESO COND. A","hora",16.37,12.125925925925927,"DER",16370]
[null,null,null,null,null,null,null,null,null,null,"72.43.01.02","RETROESCAV./CARREGADEIRA 0,77m³ COND. B","hora",35.9,26.592592592592588,"DER",35900]
[null,null,null,null,null,null,null,null,null,null,"72.44.02.03","ROCADEIRA MANUAL ELETRICA COND. C","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,510"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.44.03.03","ROCADEIRA ADAPT.P/TRAT.AGRIC.COND. C","hora",2.13,1.5777777777777775,"DER",2130]
[null,null,null,null,null,null,null,null,null,null,"72.45.01.01","ROLO COMPACT.VIBRAT.CILIN./PN 7T COND. A","hora",42.7,31.62962962962963,"DER",42700]
[null,null,null,null,null,null,null,null,null,null,"72.45.03.02","ROLO COMPACT.VIBRAT.CILIN./PN10T COND.B","hora",46.04,34.1037037037037,"DER",46040]
[null,null,null,null,null,null,null,null,null,null,"72.45.04.04","ROLO COMPACT.VIBR.CILIN./PN 11,3T COND.D","hora",154.9,114.74074074074073,"DER",154900]
[null,null,null,null,null,null,null,null,null,null,"72.45.06.01","ROLO COMP.PE DE CARN./PN 15,5T COND. A","hora",67.59,50.06666666666666,"DER",67590]
[null,null,null,null,null,null,null,null,null,null,"72.46.01.02","ROLO COMPACT.VIBR.ASF.7,2T COND. B","hora",33.38,24.725925925925925,"DER",33380]
[null,null,null,null,null,null,null,null,null,null,"72.46.01.04","ROLO COMPACT.VIBR.ASF.7,2T COND. D","hora",107.44,79.58518518518518,"DER",107440]
[null,null,null,null,null,null,null,null,null,null,"72.47.01.01","ROLO COMPACT. TANDEM 2,3TON COND. A","hora",35,25.925925925925924,"DER",35000]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.47.02.04","ROLO COMPACT. TANDEM 7TON COND. D","hora",116.05,85.96296296296296,"DER",116050]
[null,null,null,null,null,null,null,null,null,null,"72.48.01.01","ROLO COMPACT.S/PNEU P/ASF. 12,5T COND. A","hora",43.72,32.38518518518518,"DER",43720]
[null,null,null,null,null,null,null,null,null,null,"72.49.01.01","TRATOR AGRIC.C/PESO DE 3,7T COND. A","hora",30.14,22.325925925925926,"DER",30140]
[null,null,null,null,null,null,null,null,null,null,"72.49.02.01","TRATOR AGRIC.C/PESO DE 5T COND. A","hora",32.54,24.1037037037037,"DER",32540]
[null,null,null,null,null,null,null,null,null,null,"72.49.03.03","MICRO TRATOR C/APAR. DE GRAMA COND. C","hora",9.21,6.822222222222222,"DER",9210]
[null,null,null,null,null,null,null,null,null,null,"72.49.04.04","TRATOR EQUIP.C/TRIT.RESIDUOS VEG.COND. D","hora",89.24,66.1037037037037,"DER",89240]
[null,null,null,null,null,null,null,null,null,null,"72.49.05.04","TRATOR AGRIC. C/PULVEMISTURADOR COND. D","hora",81.72,60.53333333333333,"DER",81720]
[null,null,null,null,null,null,null,null,null,null,"72.50.02.04","TRATOR S/EST. COM LAMINA 2,28m³ COND. D","hora",194.27,143.9037037037037,"DER",194270]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.50.03.04","TRATOR S/EST.COM LAMINA 3,18m³ COND. D","hora",372.72,276.0888888888889,"DER",372720]
[null,null,null,null,null,null,null,null,null,null,"72.50.04.03","TRATOR S/EST. C/LAMINA/RIP.1,93m³ COND.C","hora",122.44,90.69629629629628,"DER",122440]
[null,null,null,null,null,null,null,null,null,null,"72.50.05.04","TRATOR S/EST. C/LAMINA/RIP.2,28m³ COND.D","hora",205,151.85185185185185,"DER",205000]
[null,null,null,null,null,null,null,null,null,null,"72.52.01.02","USINA DE CONCRETO 200m³/H COND. B","hora",214.82,159.1259259259259,"DER",214820]
[null,null,null,null,null,null,null,null,null,null,"72.52.03.03","USINA ASFALTICA 60 A 80T/H COND. C","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","1.161,830"]
[null,null,null,null,null,null,null,null,null,null,"72.52.04.01","USINA ASF.MATER.FRES.100A150T/H COND.A","hora",349.96,259.2296296296296,"DER",349960]
[null,null,null,null,null,null,null,null,null,null,"72.52.05.03","USINA DE SOLOS 400TON/H COND. C","hora",189.38,140.28148148148148,"DER",189380]
[null,null,null,null,null,null,null,null,null,null,"72.53.01.02","VIBRADOR DE IMERSAO 12000VPM ELET.COND.B","hora",{"$error":"#VALUE!"},{"$error":"#VALUE!"},"DER","0,690"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.54.01.03","VIBRO ACAB.ASF.S/EST.400T/H COND.C","hora",171.35,126.92592592592591,"DER",171350]
[null,null,null,null,null,null,null,null,null,null,"72.54.02.04","VIBRO ACAB.ASF.S/EST. 2200TON/H COND.D","hora",403.43,298.837037037037,"DER",403430]
[null,null,null,null,null,null,null,null,null,null,"72.54.03.04","VIBRO ACAB.ASF.S/EST.500TON/H COND. D","hora",292.16,216.41481481481483,"DER",292160]
[null,null,null,null,null,null,null,null,null,null,"72.55.01.04","VIBRO ACAB.CONCRETO 200m³/H COND. D","hora",426.53,315.9481481481481,"DER",426530]
[null,null,null,null,null,null,null,null,null,null,"72.56.03.01","SERRA PARA PAVIMENTO 9HP COND. A","hora",15.77,11.68148148148148,"DER",15770]
[null,null,null,null,null,null,null,null,null,null,"72.57.01.01","SELADORA A FRIO 15HP COND. A","hora",26.63,19.725925925925925,"DER",26630]
[null,null,null,null,null,null,null,null,null,null,"72.57.01.04","SELADORA A FRIO 15HP COND. D","hora",41.71,30.896296296296295,"DER",41710]
[null,null,null,null,null,null,null,null,null,null,"72.58.02.02","unIDADE APLIC.TINTA ELAST.A FRIO COND.B","hora",14.18,10.503703703703703,"DER",14180]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,"DER"]
[null,null,null,null,null,null,null,null,null,null,"72.58.03.04","unIDADE FUSORA COND. D","hora",271.32,200.97777777777776,"DER",271320]
[null,null,null,null,null,null,null,null,null,null,"72.58.05.02","unID.APLIC.TINTA (HOFFMAN OU SIMILAR)C-B","hora",14.79,10.955555555555554,"DER",14790]
[null,null,null,null,null,null,null,null,null,null,"72.59.01.03","SILO P/ESTOC.CIMENTO 30T COND. C","hora",3.59,2.659259259259259,"DER",3590]
[null,null,null,null,null,null,null,null,null,null,"72.59.02.04","SILO P/ESTOC.MASSA ASF.35TON COND. D","hora",3.53,2.6148148148148147,"DER",3530]
[null,null,null,null,null,null,null,null,null,null,"72.63.01.03","MAQUINA DE JATO COND. C","hora",5.64,4.177777777777777,"DER",5640]
[null,null,null,null,null,null,null,null,null,null,"010207","PARECER TÉCNICO DE FunDAÇÕES, CONTENÇÕES E RECOMENDAÇÕES GERAIS PARA EMPREENDIMENTOS COM ÁREA CONSTRUÍDA ATÉ 1.000 M²","un",null,5073.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"010208","PARECER TÉCNICO DE FunDAÇÕES, CONTENÇÕES E RECOMENDAÇÕES GERAIS PARA EMPREENDIMENTOS COM ÁREA CONSTRUÍDA DE 1.001 A 2.000 M²","un",null,6975.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"010211","PARECER TÉCNICO DE FunDAÇÕES, CONTENÇÕES E RECOMENDAÇÕES GERAIS PARA EMPREENDIMENTOS COM ÁREA CONSTRUÍDA ACIMA 10.001 M²","un",null,14584.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"010602","ELABORAÇÃO DE PROJETO DE ADEQUAÇÃO DE ENTRADA DE ENERGIA ELÉTRICA JunTO A CONCESSIONÁRIA, COM MEDIÇÃO EM BAIXA TENSÃO E DEMANDA ATÉ 75 KVA","gl",null,13696.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"011704","PROJETO EXECUTIVO DE ARQUITETURA EM FORMATO A0","un",null,4149.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"011706","PROJETO EXECUTIVO DE ESTRUTURA EM FORMATO A0","un",null,2916.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"011710","PROJETO EXECUTIVO DE INSTALAÇÕES ELÉTRICAS EM FORMATO A0","un",null,1398.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012001","INSTALAÇÃO E TRANSPORTE DE EQUIPAMENTO TOPOGRÁFICO","tx",null,616.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012111","SONDAGEM DO TERRENO À PERCUSSÃO (MÍNIMO DE 30 M)","m",null,82.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"POÇO PROFunDO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012216","FILTRO GALVANIZADO TIPO NOLD PARA POÇO PROFunDO, DIÂMETRO 6´ (150 MM)","m",null,500.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012228","PERFURAÇÃO ROTATIVA PARA POÇO PROFunDO EM ALUVIÃO, ARENITO, OU SOLOS SEDIMENTADOS EM GERAL, DIÂMETRO DE 14´ (350 MM)","m",null,383.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012230","PERFURAÇÃO ROTATIVA PARA POÇO PROFunDO EM ALUVIÃO, ARENITO, OU SOLOS SEDIMENTADOS EM GERAL, DIÂMETRO DE 16´ (400 MM)","m",null,431.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012234","PERFURAÇÃO ROTATIVA PARA POÇO PROFunDO EM ROCHA ALTERADA (BASALTO ALTERADO), DIÂMETRO DE 8´ (200 MM)","m",null,187.96,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012250","REVESTIMENTO DA BOCA DE POÇO PROFunDO TUBO CHAPA 3/16´, DIÂMETRO 14´","m",null,605,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012269","PERFILAGEM ÓTICA","m",null,55.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012272","PERFURAÇÃO ROTO-PNEUMÁTICA PARA POÇO PROFunDO EM ROCHA METASSEDIMENTAR EM GERAL, DIÂMETRO DE 12,25´ (311,15 MM)","m",null,950,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012280","REVESTIMENTO DA BOCA DE POÇO PROFunDO TUBO CHAPA 3/16´, DIÂMETRO 20´","m",null,890,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TRATAMENTO, RECUPERAÇÃO E TRABALHOS ESPECIAIS EM CONCRETO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012302","LIMPEZA DE ARMADURA COM ESCOVA DE AÇO","m²",null,3.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012319","FURAÇÃO DE 2 1/2´ EM CONCRETO ARMADO","m",null,135.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012346","FURAÇÃO DE 1´ EM CONCRETO ARMADO","m",null,117.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"012347","FURAÇÃO DE 3´ EM CONCRETO ARMADO","m",null,164.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CONTAINER",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"020210","CONTAINER GUARITA SIMPLES - MÍNIMO 1,0 M²","unxmês",null,178.61,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"020309","FECHAMENTO DEFINITIVO DE VÃOS EM CHAPA DE MADEIRA COMPENSADA","m²",null,19.81,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"020320","LOCAÇÃO DE QUADROS METÁLICOS PARA PLATAFORMA DE PROTEÇÃO, INCLUSIVE O MADEIRAMENTO","m²xmês",null,15.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"020503","ANDAIME TUBULAR FACHADEIRO","m²xmês",null,8.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"020802","PLACA DE IDENTIFICAÇÃO PARA OBRA","m²",null,354.49,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"LIMPEZA DE TERRENO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"020904","LIMPEZA MECANIZADA DO TERRENO, INCLUSIVE TRONCOS ATÉ 15 CM DE DIÂMETRO, COM CAMINHÃO À DISPOSIÇÃO, DENTRO E FORA DA OBRA, COM TRANSPORTE NO RAIO DE ATÉ 1,0 KM","m²",null,2.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"021002","LOCAÇÃO DE OBRA DE EDIFICAÇÃO","m²",null,6.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"030104","DEMOLIÇÃO MANUAL DE CONCRETO ARMADO","m³",null,194.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"030204","DEMOLIÇÃO MANUAL DE ALVENARIA DE ELEVAÇÃO OU ELEMENTO VAZADO, INCLUINDO REVESTIMENTO","m³",null,38.84,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"DEMOLIÇÃO DE REVESTIMENTO EM PEDRA E BLOCOS MACIÇOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"030606","DESMONTE (LEVANTAMENTO) MECANIZADO DE PAVIMENTO EM PARALELEPÍPEDO OU LAJOTA DE CONCRETO, INCLUSIVE ACOMODAÇÃO DO MATERIAL","m²",null,5.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"DEMOLIÇÃO DE REVESTIMENTO ASFÁLTICO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"030707","FRESAGEM DE PAVIMENTO ASFÁLTICO COM ESPESSURA ATÉ 5 CM, INCLUSIVE ACOMODAÇÃO DO MATERIAL","m²",null,3.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"030904","DEMOLIÇÃO MANUAL DE ARGAMASSA REGULARIZANTE, ISOLANTE OU PROTETORA E PAPEL KRAFT","m²",null,9.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REMOÇÃO PINTURA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"031010","REMOÇÃO DE PINTURA EM SUPERFÍCIES DE MADEIRA E/OU METÁLICAS COM LIXAMENTO","m²",null,3.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"031014","REMOÇÃO DE PINTURA EM MASSA COM LIXAMENTO","m²",null,2.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"040108","RETIRADA DE FECHAMENTO EM PLACAS PRÉ-MOLDADAS, INCLUSIVE PILARES","m²",null,1.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"040214","RETIRADA DE ESTRUTURA METÁLICA","kg",null,1.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"040502","RETIRADA DE PISO EM TACOS DE MADEIRA","m²",null,5.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"RETIRADA DE FORRO, BRISES E FACHADAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"RETIRADA DE ESQUADRIA E ELEMENTOS METÁLICOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"040910","RETIRADA DE GUARDA-CORPO OU GRADIL EM GERAL","m²",null,15.03,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"040912","RETIRADA DE ESCADA DE MARINHEIRO COM OU SEM GUARDA-CORPO","m",null,17.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"040916","RETIRADA DE ENTELAMENTO METÁLICO EM GERAL","m²",null,2.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041114","RETIRADA DE SIFÃO OU METAIS SANITÁRIOS DIVERSOS","un",null,5.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041204","RETIRADA DE MOTOR DE BOMBA DE RECALQUE","un",null,34.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041302","RETIRADA DE ISOLAMENTO TÉRMICO COM MATERIAL MONOLÍTICO","m²",null,2.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041402","RETIRADA DE VIDRO OU ESPELHO COM RASPAGEM DA MASSA OU RETIRADA DE BAGUETE","m²",null,7.03,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041704","REMOÇÃO DE APARELHO DE ILUMINAÇÃO OU PROJETOR FIXO EM POSTE OU BRAÇO","un",null,34.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041710","REMOÇÃO DE BASE DE DISJunTOR TIPO QUIK-LAG","un",null,3.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041716","REMOÇÃO DE BASE OU CHAVE PARA FUSÍVEL NH TIPO TRIPOLAR","un",null,11.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041802","REMOÇÃO DE CABEÇOTE EM REDE DE TELEFONIA","un",null,5.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041806","REMOÇÃO DE CAIXA DE ENTRADA DE ENERGIA PADRÃO MEDIÇÃO INDIRETA COMPLETA","un",null,113.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041808","REMOÇÃO DE CAIXA DE ENTRADA TELEFÔNICA COMPLETA","un",null,45.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041814","REMOÇÃO DE CAIXA PARA TRANSFORMADOR DE CORRENTE","un",null,25.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041818","REMOÇÃO DE CANTONEIRA METÁLICA","m",null,5.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041834","REMOÇÃO DE CONDULETE","un",null,9.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041839","REMOÇÃO DE CONDUTOR EMBUTIDO DIÂMETRO EXTERNO ATÉ 6,5 MM","m",null,1.1400000000000001,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041846","REMOÇÃO DE CRUZETA DE FERRO PARA FIXAÇÃO DE PROJETORES","un",null,34.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"RETIRADA EM INSTALAÇÃO ELÉTRICA - LETRA D ATÉ I",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041906","REMOÇÃO DE DISJunTOR TERMO-MAGNÉTICO","un",null,5.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"041910","REMOÇÃO DE GANCHO DE SUSTENTAÇÃO DE LUMINÁRIA EM PERFILADO","un",null,4.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042002","REMOÇÃO DE JANELA DE VENTILAÇÃO, ILUMINAÇÃO OU VENTILAÇÃO E ILUMINAÇÃO PADRÃO","un",null,16.07,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042012","REMOÇÃO DE TERMINAL MODULAR (MUFLA) TRIPOLAR OU unIPOLAR","un",null,32.14,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042106","REMOÇÃO DE PERFILADO","m",null,9.1,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042121","REMOÇÃO DE REATOR PARA LÂMPADA FIXO EM POSTE","un",null,45.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042130","REMOÇÃO DE SUPORTE DE TRANSFORMADOR EM POSTE SINGELO OU ESTALEIRO","un",null,15.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042204","REMOÇÃO DE TRANSFORMADOR DE POTÊNCIA EM CABINE PRIMÁRIA","un",null,159.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"042211","REMOÇÃO DE TUBULAÇÃO ELÉTRICA APARENTE DIÂMETRO EXTERNO ATÉ 50 MM","m",null,5.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"043505","RETIRADA DE APARELHO DE AR CONDICIONADO PORTÁTIL","un",null,10.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"051003","TRANSPORTE DE SOLO BREJOSO POR CAMINHÃO ATÉ O 2° KM","m³",null,5.97,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"051007","TRANSPORTE DE SOLO BREJOSO POR CAMINHÃO PARA DISTÂNCIAS SUPERIORES AO 3° KM ATÉ O 5° KM","m³",null,8.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"051008","TRANSPORTE DE SOLO DE 1ª E 2ª CATEGORIA POR CAMINHÃO PARA DISTÂNCIAS SUPERIORES AO 5° KM ATÉ O 10° KM","m³",null,7.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"051011","TRANSPORTE DE SOLO BREJOSO POR CAMINHÃO PARA DISTÂNCIAS SUPERIORES AO 10° KM ATÉ O 15° KM","m³",null,16.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"051015","TRANSPORTE DE SOLO BREJOSO POR CAMINHÃO PARA DISTÂNCIAS SUPERIORES AO 20° KM","m³xkm",null,1.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"SERVIÇO EM SOLO E ROCHA, MANUAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"061102","REATERRO MANUAL PARA SIMPLES REGULARIZAÇÃO SEM COMPACTAÇÃO","m³",null,4.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"061106","REATERRO MANUAL COM ADIÇÃO DE 2% DE CIMENTO","m³",null,44.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CARGA / CARREGAMENTO E DESCARGA MANUAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"SERVIÇO EM SOLO E ROCHA, MECANIZADO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"070106","ESCAVAÇÃO E CARGA MECANIZADA EM SOLO DE 2ª CATEGORIA, EM CAMPO ABERTO","m³",null,13.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESCAVAÇÃO MECANIZADA DE VALAS E BURACOS EM SOLO, EXCETO ROCHA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESCAVAÇÃO MECANIZADA EM SOLO BREJOSO OU TURFA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"071201","COMPACTAÇÃO DE ATERRO MECANIZADO MÍNIMO DE 95% PN, SEM FORNECIMENTO DE SOLO EM ÁREAS FECHADAS","m³",null,6.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"071204","ATERRO MECANIZADO POR COMPENSAÇÃO, SOLO DE 1ª CATEGORIA EM CAMPO ABERTO, SEM COMPACTAÇÃO DO ATERRO","m³",null,7.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESCORAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"080206","MONTAGEM E DESMONTAGEM DE CIMBRAMENTO TUBULAR METÁLICO","m³",null,7.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"080502","MANTA GEOTÊXTIL DE 200 G/M²","m²",null,9.21,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"080709","ESGOTAMENTO DE ÁGUAS SUPERFICIAIS COM BOMBA DE SUPERFÍCIE OU SUBMERSA","HPxh",null,2.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"081011","GABIÃO EM TELA GALVANIZADA COM MALHA DE 8/10 CM, FIO DIÂMETRO 2,4 MM, INDEPENDENTE DO FORMATO OU UTILIZAÇÃO","m³",null,358.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"090202","FORMA PLANA EM COMPENSADO PARA ESTRUTURA CONVENCIONAL","m²",null,75.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"090401","FORMA EM TUBO DE PAPELÃO COM DIÂMETRO DE 20 CM","m",null,64.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"100106","ARMADURA EM BARRA DE AÇO CA-60 (A OU B) FYK= 600 MPA","kg",null,4.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"100202","ARMADURA EM TELA SOLDADA DE AÇO","kg",null,5.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"110119","CONCRETO USINADO, FCK = 40,0 MPA","m³",null,324.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"110129","CONCRETO USINADO, FCK = 25,0 MPA - PARA BOMBEAMENTO","m³",null,319.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"110151","CONCRETO USINADO, FCK = 20,0 MPA - PARA BOMBEAMENTO EM ESTACA HÉLICE CONTÍNUA","m³",null,335.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CONCRETO USINADO NÃO ESTRUTURAL - FORNECIMENTO DO MATERIAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CONCRETO E ARGAMASSA ESPECIAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"110504","ARGAMASSA GRAUTE","m³",null,229.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"111622","NIVELAMENTO DE PISO EM CONCRETO COM ACABADORA DE SUPERFÍCIE","m²",null,12.24,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"111807","ENCHIMENTO DE LAJE COM CONCRETO CELULAR COM DENSIDADE DE 1.200 KG/M³","m³",null,347.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"111814","LASTRO E/OU FunDAÇÃO EM RACHÃO MECANIZADO","m³",null,104.03,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"112012","REPARO SUPERFICIAL COM ARGAMASSA POLIMÉRICA (TIXOTRÓPICA), BICOMPONENTE","m³",null,5453.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"BROCA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120106","BROCA EM CONCRETO ARMADO DIÂMETRO DE 30 CM - COMPLETA","m",null,48.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120402","ESTACA PRÉ-MOLDADA DE CONCRETO ATÉ 20 T","m",null,67.16,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120404","ESTACA PRÉ-MOLDADA DE CONCRETO ATÉ 40 T","m",null,89.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120502","ESTACA ESCAVADA MECANICAMENTE, DIÂMETRO DE 25 CM ATÉ 20 T","m",null,30.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120504","ESTACA ESCAVADA MECANICAMENTE, DIÂMETRO DE 35 CM ATÉ 40 T","m",null,54.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120601","TAXA DE MOBILIZAÇÃO PARA ESTACA TIPO STRAUSS","tx",null,1464,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120604","ESTACA TIPO STRAUSS, DIÂMETRO DE 38 CM ATÉ 40 T","m",null,78.72,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESTACA TIPO RAIZ",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120709","ESTACA TIPO RAIZ, DIÂMETRO DE 20 CM PARA 50 T, EM SOLO","m",null,243.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120910","ABERTURA DE FUSTE MANUAL DIÂMETRO DE 120 CM","m",null,226.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"120950","ALARGAMENTO DE BASE A CÉU ABERTO","m³",null,259.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"121204","ESTACA TIPO HÉLICE CONTÍNUA, DIÂMETRO DE 30 CM EM SOLO","m",null,41.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"121207","ESTACA TIPO HÉLICE CONTÍNUA, DIÂMETRO DE 50 CM EM SOLO","m",null,70.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"121210","ESTACA TIPO HÉLICE CONTÍNUA, DIÂMETRO DE 80 CM EM SOLO","m",null,126.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"LAJE PRÉ-FABRICADA MISTA EM VIGOTAS PROTENDIDAS E LAJOTAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"130204","LAJE PRÉ-FABRICADA MISTA VIGOTA PROTENDIDA/LAJOTA CERÂMICA - LP 12 (8+4) E CAPA COM CONCRETO DE 20MPA","m²",null,90.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"130212","LAJE PRÉ-FABRICADA MISTA VIGOTA PROTENDIDA/LAJOTA CERÂMICA - LP 10 (7+3) E CAPA COM CONCRETO DE 25MPA","m²",null,89.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"130507","PRÉ-LAJE EM PAINEL PRÉ-FABRICADO TRELIÇADO, COM EPS, H= 12 CM","m²",null,73.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"130515","PRÉ-LAJE EM PAINEL PRÉ-FABRICADO TRELIÇADO, H= 16 CM","m²",null,71.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"140104","ALVENARIA DE EMBASAMENTO EM BLOCO DE CONCRETO COM 9 CM","m²",null,43.09,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ALVENARIA COM TIJOLO MACIÇO COMUM OU ESPECIAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"140421","ALVENARIA DE BLOCO CERÂMICO DE VEDAÇÃO, USO REVESTIDO, DE 14 CM","m²",null,43.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"140505","ALVENARIA DE BLOCO CERÂMICO ESTRUTURAL, USO REVESTIDO, DE 14 CM","m²",null,50.58,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ALVENARIA COM BLOCO DE CONCRETO DE VEDAÇÃO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"141012","ALVENARIA DE BLOCO DE CONCRETO DE VEDAÇÃO, USO REVESTIDO, DE 19 CM","m²",null,52.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"141015","ALVENARIA DE BLOCO DE CONCRETO DE VEDAÇÃO, USO APARENTE, DE 19 CM","m²",null,57.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"141122","ALVENARIA DE BLOCO DE CONCRETO ESTRUTURAL, USO REVESTIDO, DE 14 CM","m²",null,47.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"141125","ALVENARIA DE BLOCO DE CONCRETO ESTRUTURAL, USO APARENTE, DE 19 CM","m²",null,58.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"141506","ALVENARIA EM BLOCO DE CONCRETO CELULAR AUTOCLAVADO, USO REVESTIDO, DE 9/10 CM - CLASSE C 25","m²",null,51.44,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"141512","ALVENARIA EM BLOCO DE CONCRETO CELULAR AUTOCLAVADO, USO REVESTIDO, DE 14/15 CM - CLASSE C 25","m²",null,76.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"142002","CIMALHA EM CONCRETO COM PINGADEIRA","m",null,5.66,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"142806","ELEMENTO VAZADO EM CONCRETO, TIPO VENEZIANA - 39 X 10 X 10 CM","m²",null,187.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"142812","ELEMENTO VAZADO EM VIDRO TIPO VENEZIANA - 20 X 10 X 10 CM","m²",null,853.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"DIVISÓRIA E FECHAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"143004","DIVISÓRIA EM PLACAS DE ARDÓSIA COM ESPESSURA DE 2 CM","m²",null,258.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"143027","FECHAMENTO E DIVISÓRIA EM PLACAS DE GESSO ACARTONADO, RESISTÊNCIA AO FOGO 30 MINUTOS, ESPESSURA TOTAL DE 7,3 CM, COM MIOLO EM LÃ DE ROCHA","m²",null,104.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"143041","FECHAMENTO/DIVISÓRIA EM PLACAS DE GESSO ACARTONADO, RESISTÊNCIA A UMIDADE, RESISTÊNCIA AO FOGO 30 MINUTOS, ESPESSURA TOTAL DE 10 CM, COM MIOLO EM LÃ DE ROCHA","m²",null,154.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"150121","ESTRUTURA PONTALETADA PARA TELHAS DE BARRO","m²",null,62.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"150530","MOBILIÁRIO EM CONCRETO ARMADO PRÉ-MOLDADO - FCK= 40 MPA","m³",null,1652.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"150553","PLACAS, VIGAS E PILARES EM CONCRETO ARMADO, PRÉ-MOLDADO - FCK= 25 MPA","m³",null,1269.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"152006","RECOLOCAÇÃO DE PEÇAS LINEARES EM MADEIRA COM SEÇÃO SUPERIOR A 60 CM²","m",null,7.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"160206","TELHA DE BARRO TIPO PLAN","m²",null,60.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"160227","ESPIGÃO DE BARRO EMBOÇADO","m",null,16.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"160301","TELHAMENTO EM CIMENTO REFORÇADO COM FIO SINTÉTICO CRFS - PERFIL ONDULADO DE 6 MM","m²",null,27.97,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"160330","CUMEEIRA NORMAL EM CIMENTO REFORÇADO COM FIO SINTÉTICO CRFS - PERFIL ONDULADO","m",null,36.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"160332","CUMEEIRA NORMAL EM CIMENTO REFORÇADO COM FIO SINTÉTICO CRFS - PERFIL TRAPEZOIDAL 44 CM","m",null,45.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"161002","TELHA EM FIBRA VEGETAL, PERFIL ONDULADO COM ESPESSURA DE 3 MM","m²",null,42.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TELHAMENTO METÁLICO COMUM",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"161205","TELHAMENTO EM CHAPA DE AÇO PRÉ-PINTADA COM EPÓXI E POLIÉSTER, PERFIL TRAPEZOIDAL, COM ESPESSURA DE 0,80 MM E ALTURA DE 100 MM","m²",null,66.89,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"161222","CUMEEIRA EM CHAPA DE AÇO PRÉ-PINTADA COM EPÓXI E POLIÉSTER, PERFIL ONDULADO, COM ESPESSURA DE 0,50 MM","m",null,37.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"161306","TELHAMENTO EM CHAPA DE AÇO PRÉ-PINTADA COM EPÓXI E POLIÉSTER, TIPO SANDUICHE, ESPESSURA DE 0,50 MM, COM LÃ DE ROCHA","m²",null,92.72,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"161616","TELHA EM POLIÉSTER REFORÇADO COM FIBRAS DE VIDRO, PERFIL TRAPEZOIDAL 49","m²",null,68.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"161618","TELHA EM POLIÉSTER REFORÇADO COM FIBRAS DE VIDRO, PERFIL TRAPEZOIDAL 90","m²",null,82.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"163213","COBERTURA CURVA EM POLICARBONATO ALVEOLAR BRONZE 10 MM","m²",null,140.96,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"163302","CALHA, RUFO, AFINS EM CHAPA GALVANIZADA Nº 24 - CORTE 0,33 M","m",null,43.07,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"163310","CALHA, RUFO, AFINS EM CHAPA GALVANIZADA Nº 26 - CORTE 0,50 M","m",null,54.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"163341","RUFO PRÉ-MOLDADO EM CONCRETO, DE 20 X 50 X 26 CM","un",null,8.29,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"164012","RECOLOCAÇÃO DE TELHAS DE BARRO TIPO FRANCESA","m²",null,15.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"164015","RECOLOCAÇÃO DE TELHA EM FIBROCIMENTO OU CRFS, PERFIL MODULADO, TRAPEZOIDAL OU MAXPLAC","m²",null,11.71,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"170105","REGULARIZAÇÃO DE PISO COM NATA DE CIMENTO","m²",null,14.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"170212","EMBOÇO COMUM","m²",null,10.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REVESTIMENTO EM CIMENTADO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"170320","DEGRAU EM CIMENTADO","m",null,28.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"170333","RODAPÉ EM CIMENTADO DESEMPENADO E ALISADO COM ALTURA 15 CM","m",null,12.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"170507","PISO COM REQUADRO EM CONCRETO SIMPLES COM CONTROLE DE FCK= 20 MPA","m³",null,512.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"172005","FRISO PARA JunTA DE DILATAÇÃO EM REVESTIMENTO DE GRANITO LAVADO TIPO FULGET","m",null,4.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"172014","REVESTIMENTO TEXTURIZADO ACRÍLICO COM MICROAGREGADOS MINERAIS","m²",null,13.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS E CONSERVAÇÕES EM MASSA E CONCRETO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"174005","REPAROS EM PEITORIL DE GRANILITE - ESTUCAMENTO E POLIMENTO","m",null,12.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REVESTIMENTO CERÂMICO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PISOS EM PLACAS CERÂMICAS ESMALTADAS PRENSADAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180607","RODAPÉ CERÂMICO ESMALTADO COM TEXTURA SEMI-RUGOSA PEI-5 RESISTÊNCIA QUÍMICA A, PARA ÁREAS INTERNAS, ASSENTADO COM ARGAMASSA MISTA","m",null,19.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180617","PISO CERÂMICO ESMALTADO RÚSTICO PEI-5 RESISTÊNCIA QUÍMICA B, PARA ÁREAS INTERNAS COM SAÍDA PARA O EXTERIOR, ASSENTADO COM ARGAMASSA MISTA","m²",null,69.66,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180642","REJunTAMENTO DE PISO EM PLACAS CERÂMICAS (40-43 X 40-43 CM) COM CIMENTO BRANCO, JunTAS ACIMA 5 ATÉ 10 MM","m²",null,5.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180651","REJunTAMENTO DE RODAPÉ EM PLACAS CERÂMICAS ATÉ 10 CM DE ALTURA COM ARGAMASSA INDUSTRIALIZADA PARA REJunTE, JunTAS ACIMA DE 3 ATÉ 5 MM","m",null,0.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180709","CANTO DE RODAPÉ CERÂMICO NÃO ESMALTADO EXTRUDADO ALTA RESISTÊNCIA QUÍMICA E MECÂNICA, ALTURA DE 10 CM ASSENTADO COM ARGAMASSA DE CIMENTO E AREIA","un",null,3.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180721","REJunTAMENTO DE PISO CERÂMICO EXTRUDADO ANTIÁCIDO DE 9 MM, COM ARGAMASSA INDUSTRIALIZADA À BASE DE RESINA EPÓXI, JunTAS ACIMA DE 3 ATÉ 6 MM","m²",null,17.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180724","REJunTAMENTO DE REVESTIMENTO CERÂMICO EXTRUDADO ANTIÁCIDO DE 9 MM, COM ARGAMASSA INDUSTRIALIZADA À BASE DE RESINA EPÓXI, JunTAS ACIMA DE 3 ATÉ 6 MM","m²",null,17.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180731","REJunTAMENTO DE RODAPÉ CERÂMICO EXTRUDADO ANTIÁCIDO DE 9 MM, COM ARGAMASSA INDUSTRIALIZADA À BASE DE RESINA EPÓXI, JunTAS ACIMA DE 3 ATÉ 6 MM","m",null,1.72,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"180814","RODAPÉ EM PORCELANATO TÉCNICO ANTIÁCIDO, GRUPO DE ABSORÇÃO BI-A, REJunTADO COM RESINA EPÓXI","m",null,21.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"181120","REJunTAMENTO DE PLACA CERÂMICA DE 15 X 15 CM COM CIMENTO BRANCO, JunTAS ATÉ 3 MM","m²",null,5.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"181122","REJunTAMENTO DE CERÂMICA ESMALTADA DE 20 X 20 CM COM CIMENTO BRANCO, JunTAS ATÉ 3 MM","m²",null,5.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"181220","REVESTIMENTO EM PASTILHA DE PORCELANA NATURAL OU ESMALTADA DE 2,5 X 2,5 CM, ASSENTADO E REJunTADO COM ARGAMASSA COLANTE INDUSTRIALIZADA, FAIXAS ATÉ 40 CM","m",null,60.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REVESTIMENTO EM PLACAS CERÂMICAS NÃO ESMALTADAS EXTRUDADAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"181301","REVESTIMENTO DE PLACA CERÂMICA NÃO ESMALTADA EXTRUDADA ALTA RESISTÊNCIA QUÍMICA E MECÂNICA, ESPESSURA DE 9 MM, ASSENTADO COM ARGAMASSA COLANTE INDUSTRIALIZADA","m²",null,74.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"190101","RODAPÉ EM GRANITO COM 7 CM DE ALTURA","m",null,78.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"190102","REVESTIMENTO EM GRANITO COM 2 CM DE ESPESSURA, ASSENTE COM MASSA","m²",null,173.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"190132","RODAPÉ EM GRANITO COM ALTURA DE 7,1 A 10 CM","m",null,83.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"190202","REVESTIMENTO EM MÁRMORE BRANCO DE 2 CM, ASSENTE COM MASSA","m²",null,401.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PEDRA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"190309","REVESTIMENTO EM PEDRA MIRACEMA","m²",null,59.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"190327","RODAPÉ EM PEDRA ARDÓSIA COM 7 CM DE ALTURA","m",null,8.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"200104","LAMBRIL EM MADEIRA MACHO/FÊMEA TARUGADO, EXCETO PINUS","m²",null,63.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"201004","RODAPÉ DE MADEIRA DE 7 X 1,5 CM","m",null,18.26,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"202002","RECOLOCAÇÃO DE SOALHO EM MADEIRA","m²",null,4.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"210110","REVESTIMENTO EM BORRACHA SINTÉTICA PRETA DE 4,0 MM - COLADO","m²",null,45.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REVESTIMENTO VINÍLICO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"210228","REVESTIMENTO VINÍLICO EM MANTA CALANDRADA HOMOGÊNEA FLEXÍVEL COM ESPESSURA DE 2MM","m²",null,109.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"210410","REVESTIMENTO COM CARPETE PARA TRÁFEGO MODERADO, USO COMERCIAL, TIPO BOUCLÊ DE 5,4 ATÉ 8 MM","m²",null,70.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"211006","RODAPÉ VINÍLICO DE 5,0 CM, COM IMPERMEABILIZANTE ACRÍLICO","m",null,19.49,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"211105","DEGRAU (PISO E ESPELHO) EM BORRACHA SINTÉTICA PRETA COM TESTEIRA - COLADO","m",null,57.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"FORRO DE MADEIRA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"220121","TESTEIRA EM TÁBUA APARELHADA, COM LARGURA DE ATÉ 20 CM","m",null,17.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"220203","FORRO EM PAINÉIS DE GESSO ACARTONADO, COM ESPESSURA DE 12,5 MM, FIXO","m²",null,50.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"220302","FORRO EM LÃ DE VIDRO REVESTIDO EM PVC, ESPESSURA DE 20 MM","m²",null,56.24,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"BRISE-SOLÉIL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"220609","TERMOBRISE EM ALUZINC PRÉ-PINTADO, COM INJEÇÃO DE POLIURETANO EXPANDIDO, LARGURA 335 MM","m²",null,604.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"220614","BRISE EM PLACA CIMENTÍCIA COM ESPESSURA DE 12MM","m²",null,182.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230203","PORTA MACHO E FÊMEA COM BATENTE DE MADEIRA - 72 X 210 CM","un",null,665.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230253","PORTA MACHO E FÊMEA COM BATENTE METÁLICO - 82 X 210 CM","un",null,757.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230413","PORTA EM LAMINADO FENÓLICO MELAMÍNICO COM ACABAMENTO LISO, BATENTE DE MADEIRA SEM REVESTIMENTO - 144 X 210 CM","un",null,1194.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230460","PORTA EM LAMINADO FENÓLICO MELAMÍNICO COM ACABAMENTO LISO, BATENTE METÁLICO - 82 X 210 CM","un",null,740.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230802","FAIXA/BATEDOR DE PROTEÇÃO EM MADEIRA APARELHADA NATURAL 10 X 2,5 CM","m",null,25.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230817","LOUSA EM LAMINADO MELAMÍNICO, BRANCO - LINHA COMERCIAL","m²",null,126.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230822","ARMÁRIO SOB MEDIDA EM COMPENSADO DE MADEIRA TOTALMENTE REVESTIDO EM LAMINADO MELAMÍNICO TEXTURIZADO, COMPLETO","m²",null,998.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230824","PORTA LISA DE CORRER, EM MADEIRA","m²",null,575.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230902","PORTA LISA COM BATENTE MADEIRA - 62 X 210 CM","un",null,226.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230905","PORTA LISA COM BATENTE MADEIRA - 92 X 210 CM","un",null,236.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230950","ACRÉSCIMO DE BANDEIRA - PORTA LISA COMUM COM BATENTE METÁLICO","m²",null,144.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230953","PORTA LISA COM BATENTE METÁLICO - 82 X 160 CM","un",null,215.01,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230956","PORTA LISA COM BATENTE METÁLICO - 92 X 210 CM","un",null,321.72,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"230959","PORTA LISA COM BATENTE METÁLICO - 164 X 210 CM","un",null,425.1,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"231101","ACRÉSCIMO DE BANDEIRA - PORTA LISA PARA ACABAMENTO EM VERNIZ, COM BATENTE DE MADEIRA","m²",null,122.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"231104","PORTA LISA PARA ACABAMENTO EM VERNIZ, COM BATENTE DE MADEIRA - 82 X 210 CM","un",null,246.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"232014","ACRÉSCIMO DE VISOR COMPLETO EM PORTA DE MADEIRA","un",null,127.21,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"232022","FOLHA DE PORTA MACHO E FÊMEA, 72 X 210 CM","un",null,538.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"232033","FOLHA DE PORTA LISA COMUM, 82 X 210 CM","un",null,100.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"232046","FOLHA DE PORTA EM LAMINADO FENÓLICO MELAMÍNICO COM ACABAMENTO LISO, 92 X 210 CM","un",null,548.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240103","CAIXILHO EM FERRO BASCULANTE, SOB MEDIDA","m²",null,384.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240107","CAIXILHO EM FERRO DE CORRER, SOB MEDIDA","m²",null,447.21,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240109","CAIXILHO EM FERRO COM VENTILAÇÃO PERMANENTE, SOB MEDIDA","m²",null,300.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240112","CAIXILHO TIPO VENEZIANA INDUSTRIAL COM MONTANTES EM AÇO GALVANIZADO E ALETAS EM FIBRA DE VIDRO","m²",null,158.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240120","CAIXILHO FIXO EM AÇO SAE 1010/1020 PARA VIDRO À PROVA DE BALA, SOB MEDIDA","m²",null,559.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240128","CAIXILHO TIPO GUICHÊ EM CHAPA DE AÇO","m²",null,744.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240201","PORTA EM FERRO DE ABRIR, PARA RECEBER VIDRO, SOB MEDIDA","m²",null,653,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240205","PORTA CORTA-FOGO CLASSE P.90 DE 90 X 210 CM, COMPLETA, COM MAÇANETA TIPO ALAVANCA","un",null,567.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240207","PORTA DE FERRO DE ABRIR TIPO VENEZIANA, LINHA COMERCIAL","m²",null,250.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240227","PORTÃO DE 2 FOLHAS, TUBULAR EM TELA DE AÇO GALVANIZADO ACIMA DE 2,50 M DE ALTURA, COMPLETO","m²",null,398.92,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240247","PORTINHOLA DE CORRER EM CHAPA, PARA ´PASSA PACOTE´, COMPLETA, SOB MEDIDA","m²",null,911.21,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240249","GRADE EM BARRA CHATA SOLDADA DE 1 1/2´ X 1/4´, SOB MEDIDA","m²",null,772.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240290","PORTA DE ABRIR EM CHAPA DUPLA COM VISOR, BATENTE ENVOLVENTE, COMPLETA","m²",null,1229.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240292","PORTA CORTA-FOGO CLASSE P.120 DE 90 X 210 CM, COM UMA FOLHA DE ABRIR","un",null,1539.29,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240310","ALÇAPÃO/TAMPA EM CHAPA DE FERRO COM PORTA CADEADO","m²",null,858.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240396","CORRIMÃO EM TUBO DE AÇO INOXIDÁVEL ESCOVADO, COM DIÂMETRO DE 1 1/2´ E MONTANTES COM DIÂMETRO DE 2´","m",null,708.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240422","GRADE DE SEGURANÇA EM AÇO SAE 1045, DIÂMETRO 1´, SEM TÊMPERA E REVENIMENTO","m²",null,698.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240430","GRADE DE SEGURANÇA EM AÇO SAE 1045, DIÂMETRO 1´, COM TÊMPERA E REVENIMENTO","m²",null,796.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240432","GRADE DE SEGURANÇA EM AÇO SAE 1045 CHAPEADA, DIÂMETRO 1´, COM TÊMPERA E REVENIMENTO","m²",null,1221.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240437","PORTÃO DE SEGURANÇA DE ABRIR, PARA MURALHA, EM GRADE COM AÇO SAE 1045 CHAPEADO, DIÂMETRO 1´, COMPLETO, COM TÊMPERA E REVENIMENTO","m²",null,1580.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240442","PORTA DE SEGURANÇA DE CORRER EM GRADE DE AÇO SAE 1045 CHAPEADA, DIÂMETRO DE 1´, COMPLETA, SEM TÊMPERA E REVENIMENTO","m²",null,1512.09,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESQUADRIA, SERRALHERIA DE SEGURANÇA - PADRÃO FunDAÇÃO CASA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240504","PORTÃO DE SEGURANÇA DE ABRIR, PARA MURALHA, EM CHAPA DE AÇO GALVANIZADO, COMPLETO - PADRÃO FunDAÇÃO CASA","m²",null,980.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"240512","GAIOLA DE SEGURANÇA, COMPLETA - PADRÃO FunDAÇÃO CASA","cj",null,17059.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"242009","SOLDA MIG EM ESQUADRIAS METÁLICAS","m",null,25.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250105","CAIXILHO EM ALUMÍNIO MAXIMAR, COM VIDRO, LINHA COMERCIAL","m²",null,346.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250111","CAIXILHO GUILHOTINA EM ALUMÍNIO ANODIZADO, SOB MEDIDA","m²",null,801.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250143","CAIXILHO EM ALUMÍNIO FIXO, TIPO FACHADA","m²",null,483.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250146","GRADIL EM ALUMINIO NATURAL, SOB MEDIDA","m²",null,630.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250150","CAIXILHO EM ALUMÍNIO ANODIZADO FIXO, SOB MEDIDA - BRONZE/PRETO","m²",null,241.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250201","PORTA DE ENTRADA DE ABRIR EM ALUMÍNIO COM VIDRO, LINHA COMERCIAL","m²",null,531.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250206","PORTA/PORTINHOLA EM ALUMÍNIO, SOB MEDIDA","m²",null,506.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250223","PORTA EM ALUMÍNIO ANODIZADO DE ABRIR, SOB MEDIDA - BRONZE/PRETO","m²",null,332.71,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"250226","PORTINHOLA EM ALUMÍNIO ANODIZADO DE CORRER, TIPO VENEZIANA, SOB MEDIDA - BRONZE/PRETO","m²",null,504.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESQUADRIA E ELEMENTO EM VIDRO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"260102","VIDRO LISO TRANSPARENTE DE 3 MM","m²",null,53.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"260123","VIDRO FANTASIA DE 3/4 MM","m²",null,57.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"260135","VIDRO LISO LAMINADO DE ALTA SEGURANÇA","m²",null,3468.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"VIDROS TEMPERADOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"260206","VIDRO TEMPERADO INCOLOR DE 10 MM","m²",null,201.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"260214","VIDRO TEMPERADO CINZA OU BRONZE DE 8 MM","m²",null,208.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"262001","MASSA PARA VIDRO","m",null,2.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"262006","FURAÇÃO EM VIDRO","un",null,38.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"270201","CHAPA DE POLICARBONATO COMPACTA CRISTAL 6 MM","m²",null,312,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"270402","CAIXILHO DE ABRIR COM FECHAMENTO EM CHAPA DE PVC E REQUADRO EM CANTONEIRA DE AÇO CARBONO","m²",null,290.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"270403","CAIXILHO DE CORRER EM PVC","m²",null,360.92,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280109","FERRAGEM ADICIONAL PARA PORTA VÃO DUPLO EM DIVISÓRIA","cj",null,270.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280125","VISOR TIPO OLHO MÁGICO","un",null,20.17,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280128","FECHADURA DE SEGURANÇA PARA CELA TIPO GORGES, COM CLIC E ABERTURA DE UM LADO, EMBUTIDA EM CAIXA","cj",null,545.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280136","FERRAGEM COMPLETA COM MAÇANETA TIPO ALAVANCA, ACABAMENTO EM ALUMÍNIO, PARA PORTA EXTERNA COM 1 FOLHA","cj",null,240.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280137","FERRAGEM COMPLETA COM MAÇANETA TIPO ALAVANCA, ACABAMENTO EM ALUMÍNIO, PARA SANITÁRIO COM 1 FOLHA","cj",null,188.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280144","FERRAGEM COMPLETA COM MAÇANETA TIPO ALAVANCA, ACABAMENTO EM ALUMÍNIO, PARA PORTA EXTERNA COM 2 FOLHAS","cj",null,388.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"280506","CADEADO DE LATÃO COM CILÍNDRO - TRAVA DUPLA - 50MM","un",null,21.39,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282003","BARRA ANTIPÂNICO DE SOBREPOR PARA PORTA DE 1 FOLHA","un",null,493.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282017","BRETE PARA INSTALAÇÃO SUPERIOR EM PORTA CHAPA/GRADE DE SEGURANÇA","cj",null,1659.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282023","DOBRADIÇA SUPERIOR PARA PORTA DE VIDRO TEMPERADO","un",null,75.26,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282036","SUPORTE DUPLO PARA VIDRO TEMPERADO FIXADO EM ALVENARIA","un",null,93.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282059","CONTRA FECHADURA DE CENTRO PARA PORTA EM VIDRO TEMPERADO","un",null,27.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282071","SUPORTE DUPLO OU CENTRAL SEM NÚCLEO PARA VIDRO TEMPERADO","un",null,20.29,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282076","ESPELHO PARA TRINCO DE PISO PARA PORTA EM VIDRO TEMPERADO","un",null,21.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"282078","FECHADURA EXTERNA COM MAÇANETA TIPO ALAVANCA E CILINDRO, ACABAMENTO COR PRATA","un",null,168.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"290102","CANTONEIRA EM ALUMÍNIO PERFIL SEXTAVADO","m",null,10.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"292003","ALUMÍNIO LISO PARA COMPLEMENTOS E REPAROS","kg",null,27.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"300109","BARRA DE APOIO, EM ÂNGULO DE 90°, PARA PESSOAS COM MOBILIDADE REDUZIDA, EM TUBO DE ALUMÍNIO DE 800 X 800 MM, ACABAMENTO COM PINTURA EPÓXI","un",null,220.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"300110","BARRA DE APOIO RETA, PARA PESSOAS COM MOBILIDADE REDUZIDA, EM TUBO DE ALUMÍNIO, COMPRIMENTO DE 900 MM, ACABAMENTO COM PINTURA EPÓXI","un",null,106.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"APARELHOS ELÉTRICOS, HIDRÁULICOS E A GÁS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"300406","REVESTIMENTO EM CHAPA DE AÇO INOXIDÁVEL PARA PROTEÇÃO DE PORTAS, ALTURA DE 40 CM","m",null,235.49,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"300411","REVESTIMENTO EM PORCELANATO ANTIDERRAPANTE DE ALERTA / DIRECIONAL, GRUPO DE ABSORÇÃO BI-A, REJunTADO","m²",null,356.21,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"301001","FECHADURA COM MAÇANETA PARA PESSOAS COM MOBILIDADE REDUZIDA, EM ALUMÍNIO","un",null,587.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"301401","ELEVADOR DE USO RESTRITO A PESSOAS COM MOBILIDADE REDUZIDA COM 02 PARADAS - USO INTERNO EM ALVENARIA","cj",null,53000,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ISOLAMENTOS TÉRMICOS / ACÚSTICOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"320704","JunTA PLÁSTICA DE 3/4´ X 1/8´","m",null,4.17,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"320711","JunTA A BASE DE ASFALTO OXIDADO A QUENTE","cm³",null,0.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"320803","JunTA ESTRUTURAL COM POLIESTIRENO EXPANDIDO DE ALTA DENSIDADE P-III, ESPESSURA DE 20 MM","m²",null,11.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"320811","JunTA ESTRUTURAL COM PERFIL ELASTOMÉRICO E LÁBIOS POLIMÉRICOS PARA OBRAS DE ARTE, MOVIMENTAÇÃO MÁXIMA 40 MM","m",null,440.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"320904","APOIO EM PLACA DE NEOPRENE FRETADO","dm³",null,88.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321011","PROTEÇÃO ANTICORROSIVA, COM FITA ADESIVA, PARA RAMAIS SOB A TERRA, COM DN ACIMA DE 2´ ATÉ 3´","m",null,27.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321014","PROTEÇÃO ANTICORROSIVA, COM FITA ADESIVA, PARA RAMAIS SOB A TERRA, COM DN ACIMA DE 5´ ATÉ 6´","m",null,52.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321130","ISOLAMENTO TÉRMICO EM ESPUMA ELASTOMÉRICA, ESPESSURA DE 9 A 12 MM, PARA TUBULAÇÃO DE 1´ (COBRE)","m",null,9.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321132","ISOLAMENTO TÉRMICO EM ESPUMA ELASTOMÉRICA, ESPESSURA DE 19 A 26 MM, PARA TUBULAÇÃO DE 1 1/8´ (COBRE) OU 3/4´ (FERRO)","m",null,16.1,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321134","ISOLAMENTO TÉRMICO EM ESPUMA ELASTOMÉRICA, ESPESSURA DE 19 A 26 MM, PARA TUBULAÇÃO DE 1 5/8´ (COBRE) OU 1 1/4´ (FERRO)","m",null,20.15,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321138","ISOLAMENTO TÉRMICO EM ESPUMA ELASTOMÉRICA, ESPESSURA DE 19 A 26 MM, PARA TUBULAÇÃO DE 3 1/2´ (COBRE) OU 3´ (FERRO)","m",null,33.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321140","ISOLAMENTO TÉRMICO EM ESPUMA ELASTOMÉRICA, ESPESSURA DE 19 A 26 MM, PARA TUBULAÇÃO DE 5´ (FERRO)","m",null,51.89,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321503","IMPERMEABILIZAÇÃO EM MANTA ASFÁLTICA COM ARMADURA, TIPO III-B, ESPESSURA DE 3 MM","m²",null,36.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321601","IMPERMEABILIZAÇÃO EM PINTURA DE ASFALTO OXIDADO COM SOLVENTES ORGÂNICOS, SOBRE MASSA","m²",null,7.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321603","IMPERMEABILIZAÇÃO EM MEMBRANA DE ASFALTO MODIFICADO COM ELASTÔMEROS, NA COR PRETA","m²",null,24.98,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321605","IMPERMEABILIZAÇÃO EM MEMBRANA À BASE DE POLÍMEROS ACRÍLICOS, NA COR BRANCA","m²",null,28.21,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"321704","IMPERMEABILIZAÇÃO EM ARGAMASSA POLIMÉRICA COM REFORÇO EM TELA POLIÉSTER PARA PRESSÃO HIDROSTÁTICA POSITIVA","m²",null,25.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"322002","APLICAÇÃO DE PAPEL KRAFT","m²",null,3.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330135","PREPARO DE BASE PARA SUPERFÍCIE METÁLICA COM FunDO ANTI-OXIDANTE","m²",null,7.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330206","MASSA CORRIDA A BASE DE PVA","m²",null,6.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330212","MASSA CORRIDA A ÓLEO EM SUPERFÍCIE REBOCADA","m²",null,13.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330375","VERNIZ ACRÍLICO","m²",null,16.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330378","VERNIZ DE PROTEÇÃO ANTIPICHAÇÃO","m²",null,21.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330512","ESMALTE EM RODAPÉS, BAGUETES OU MOLDURAS DE MADEIRA","m",null,2.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PINTURA EM ESTRUTURAS METÁLICAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PINTURA DE SINALIZAÇÃO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"330902","BORRACHA CLORADA PARA FAIXAS DEMARCATÓRIAS","m",null,1.97,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"331003","TINTA ACRÍLICA ANTIMOFO EM MASSA, INCLUSIVE PREPARO","m²",null,14.26,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"331102","ESMALTE EM SUPERFÍCIE METÁLICA, INCLUSIVE PREPARO","m²",null,20.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PINTURA EM SUPERFÍCIE DE MADEIRA, INCLUSIVE PREPARO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PAISAGISMO E FECHAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340207","FORRAÇÃO COM LÍRIO AMARELO, MÍNIMO 18 MUDAS / M² - H= 0,50 M","m²",null,42.2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340209","FORRAÇÃO COM HERA INGLESA, MÍNIMO 18 MUDAS / M² - H= 0,15 M","m²",null,23.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340240","PLANTIO DE GRAMA PELO PROCESSO HIDROSSEMEADURA","m²",null,2.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340315","ARBUSTO CURCÚLIGO - H= 0,60 A 0,80 M","un",null,20.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340436","ÁRVORE ORNAMENTAL TIPO COQUEIRO JERIVÁ - H= 4,00 M","un",null,156.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340502","CERCA EM ARAME FARPADO COM MOURÕES DE CONCRETO","m",null,29.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340535","PORTÃO DE ABRIR EM GRADIL ELETROFunDIDO, MALHA 5 X 15 CM","m²",null,702.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340537","FECHAMENTO DE DIVISA - MOURÃO COM PLACAS PRÉ MOLDADAS","m",null,99.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"340778","ÁRVORE TIPO AROEIRA SALSA - H= 2,00 M","un",null,108.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"350117","POSTE OFICIAL COMPLETO COM REDE PARA VOLEIBOL","cj",null,737.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"350155","PISO EM FIBRA DE POLIPROPILENO CORRUGADO PARA QUADRA DE ESPORTES, INCLUSIVE PINTURA","m²",null,70.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"350413","BANCO DE MADEIRA SOBRE ALVENARIA","m²",null,104.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"350520","CENTRO DE ATIVIDADES EM MADEIRA RÚSTICA","cj",null,2750.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"350703","PLATAFORMA COM 3 MASTROS GALVANIZADOS, H= 9,00 M","cj",null,3327.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360306","CAIXA DE MEDIÇÃO EXTERNA TIPO ´M´ (900 X 1200 X 270) MM, PADRÃO ELETROPAULO","un",null,768.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360313","CAIXA DE PROTEÇÃO DOS BORNES DO MEDIDOR, (300 X 250 X 90) MM, PADRÃO CPFL","un",null,76.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360316","CAIXA BASE LATERAL TIPO ´N´ (130 X 40 X 25) CM","un",null,346.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360403","SUPORTE PARA 2 ISOLADORES DE BAIXA TENSÃO","un",null,22.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360502","ISOLADOR TIPO CASTANHA INCLUINDO GRAMPO DE SUSTENTAÇÃO","un",null,10.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360511","ISOLADOR PEDESTAL PARA 25 KV","un",null,69.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360601","TERMINAL MODULAR (MUFLA) unIPOLAR INTERNO PARA CABO ATÉ 120 MM²/25 KV","cj",null,270.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360603","TERMINAL MODULAR (MUFLA) unIPOLAR EXTERNO PARA CABO ATÉ 70 MM²/25 KV","cj",null,279.1,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360829","GRUPO GERADOR COM POTÊNCIA DE 563/513 KVA, 220/127 V OU 380/220V, COMPLETO, INCLUSIVE CONJunTO DE BATERIAS","un",null,183187.07,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMADOR DE ENTRADA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360917","TRANSFORMADOR DE POTÊNCIA TRIFÁSICO DE 300 KVA, CLASSE 15 KV, A ÓLEO","un",null,15103.15,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"360970","TRANSFORMADOR DE POTÊNCIA TRIFÁSICO DE 500 KVA, CLASSE 25KV, ENCAPSULADO A VÁCUO EM RESINA EPÓXI","un",null,39596.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"362018","LUVA ISOLANTE DE BORRACHA, ACIMA DE 10 ATÉ 20 KV","par",null,499.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"362020","MÃO FRANCESA DE 700 MM","un",null,34.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"362024","ÓLEO PARA DISJunTOR","l",null,9.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"362034","SELA PARA CRUZETA DE MADEIRA","un",null,38.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"362039","ESTRADO DE BORRACHA DE 100 X 100 CM, ISOLANTE ATÉ 68 KV","un",null,256.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"QUADRO PARA TELEFONIA EMBUTIR, PROTEÇÃO IP40 CHAPA Nº 16MSG",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"370116","QUADRO TELEBRÁS DE EMBUTIR DE 800 X 800 X 120 MM","un",null,268.96,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"QUADRO DISTRIBUIÇÃO DE LUZ E FORÇA DE EMBUTIR unIVERSAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"370323","QUADRO DE DISTRIBUIÇÃO unIVERSAL DE EMBUTIR, PARA DISJunTORES 44 DIN / 32 BOLT-ON - 150 A - SEM COMPONENTES","un",null,337.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"370425","QUADRO DE DISTRIBUIÇÃO unIVERSAL DE SOBREPOR, PARA DISJunTORES 16 DIN / 12 BOLT-ON - 150 A - SEM COMPONENTES","un",null,261.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"370428","QUADRO DE DISTRIBUIÇÃO unIVERSAL DE SOBREPOR, PARA DISJunTORES 44 DIN / 32 BOLT-ON - 150 A - SEM COMPONENTES","un",null,389.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"370429","QUADRO DE DISTRIBUIÇÃO unIVERSAL DE SOBREPOR, PARA DISJunTORES 56 DIN / 40 BOLT-ON - 225 A - SEM COMPONENTES","un",null,515.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"BARRAMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"BASES",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371112","BASE DE FUSÍVEL TRIPOLAR DE 15 KV","un",null,478.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371210","FUSÍVEL TIPO NH 4 DE 800 A ATÉ 1250 A","un",null,250.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371214","FUSÍVEL TIPO HH PARA 15 KV DE 60 A ATÉ 100 A","un",null,271.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371222","FUSÍVEL DIAZED RETARDADO DE 35 A ATÉ 63 A","un",null,6.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371352","DISJunTOR A SECO ABERTO TRIFÁSICO, 600 V DE 800 A, 50/60 HZ, COM ACESSÓRIOS","un",null,12957.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371361","DISJunTOR TERMOMAGNÉTICO, unIPOLAR 127/220 V, CORRENTE DE 35 A ATÉ 50 A","un",null,17.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371364","DISJunTOR TERMOMAGNÉTICO, BIPOLAR 220/380 V, CORRENTE DE 60 A ATÉ 100 A","un",null,66.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371378","DISJunTOR EM CAIXA MOLDADA, TÉRMICO E MAGNÉTICO AJUSTÁVEIS, TRIPOLAR 1600 A/690 V, FAIXA DE AJUSTE DE 1000 ATÉ 1600 A","un",null,10593.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371386","MINI-DISJunTOR TERMOMAGNÉTICO, BIPOLAR 220/380 V, CORRENTE DE 63 A","un",null,40.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371391","MINI-DISJunTOR TERMOMAGNÉTICO, TRIPOLAR 400 V, CORRENTE DE 80 A ATÉ 125 A","un",null,592.89,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371433","CHAVE SECCIONADORA SOB CARGA, TRIPOLAR, ACIONAMENTO ROTATIVO, COM PROLONGADOR, SEM PORTA-FUSÍVEL, DE 630 A","un",null,1119.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371442","CHAVE SECCIONADORA SOB CARGA, TRIPOLAR, ACIONAMENTO ROTATIVO, COM PROLONGADOR E PORTA-FUSÍVEL ATÉ NH-00-160 A - SEM FUSÍVEIS","un",null,868.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371444","CHAVE SECCIONADORA SOB CARGA, TRIPOLAR, ACIONAMENTO ROTATIVO, COM PROLONGADOR E PORTA-FUSÍVEL ATÉ NH-2-400 A - SEM FUSÍVEIS","un",null,1658.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371482","BARRA DE CONTATO PARA CHAVE SECCIONADORA TIPO NH2-400 A","un",null,25.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371512","CHAVE SECCIONADORA TRIPOLAR SOB CARGA PARA 400 A - 15 KV - COM PROLONGADOR","un",null,1127.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371706","DISPOSITIVO DIFERENCIAL RESIDUAL DE 25 A X 30 MA - 2 PÓLOS","un",null,103.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TRANSFORMADOR DE POTENCIAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371804","TRANSFORMADOR DE POTENCIAL MONOFÁSICO ATÉ 1000 VA CLASSE 25 KV, A SECO, COM FUSÍVEIS","un",null,1928.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371903","TRANSFORMADOR DE CORRENTE 1000-5 A ATÉ 1500-5 A, JANELA","un",null,276.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"371906","TRANSFORMADOR DE CORRENTE 50-5 A ATÉ 150-5 A, JANELA","un",null,114.97,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"372004","PALHETA PLÁSTICA PARA DISJunTORES FALTANTES","un",null,1.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"372404","SUPRESSOR DE SURTO MONOFÁSICO, NEUTRO-TERRA, IN > OU = 20 KA, IMAX. DE SURTO DE 65 ATÉ 80 KA","un",null,134.76,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"372521","DISJunTOR EM CAIXA MOLDADA BIPOLAR, TÉRMICO E MAGNÉTICO FIXOS - 600V - DE 150A PARA 120/240VCA - 25 KA E PARA 380/440VCA - 18 KA","un",null,430.03,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"380416","ELETRODUTO DE FERRO GALVANIZADO, MÉDIO DE 3´ - COM ACESSÓRIOS","m",null,59.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"380502","ELETRODUTO DE FERRO GALVANIZADO, PESADO DE 1/2´ - COM ACESSÓRIOS","m",null,16.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"380509","ELETRODUTO DE FERRO GALVANIZADO, PESADO DE 1 1/4´ - COM ACESSÓRIOS","m",null,31.97,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"380618","ELETRODUTO DE FERRO GALVANIZADO A QUENTE, PESADO DE 4´ - COM ACESSÓRIOS","m",null,95.71,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"DUTO FECHADO DE PISO E ACESSÓRIOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381007","CAIXA DE TOMADA E TAMPA BASCULANTE COM REBAIXO DE 3 X (25 X 70 MM)","un",null,91.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ELETRODUTO EM POLIETILENO DE ALTA DENSIDADE",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381303","ELETRODUTO CORRUGADO EM POLIETILENO DE ALTA DENSIDADE, DN= 75 MM, COM ACESSÓRIOS","m",null,14.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381306","ELETRODUTO CORRUGADO EM POLIETILENO DE ALTA DENSIDADE, DN= 150 MM, COM ACESSÓRIOS","m",null,47.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381511","TERMINAL MACHO FIXO EM LATÃO ZINCADO DE 3/4´","un",null,8.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381514","TERMINAL MACHO FIXO EM LATÃO ZINCADO DE 2´","un",null,33.78,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381533","TERMINAL MACHO GIRATÓRIO EM LATÃO ZINCADO DE 1 1/2´","un",null,29.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381611","CAIXA DE DERIVAÇÃO EMBUTIDA OU EXTERNA COM PINTURA ELETROSTÁTICA, PARA RODAPÉ TÉCNICO TRIPLO","un",null,36.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381620","CURVA HORIZONTAL DUPLA DE 90°, INTERNA OU EXTERNA, E TAMPA COM PINTURA ELETROSTÁTICA","un",null,26.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"381922","ELETRODUTO DE PVC CORRUGADO FLEXÍVEL REFORÇADO, DIÂMETRO EXTERNO DE 32 MM","m",null,9.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ELETROCALHA E ACESSÓRIOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382113","ELETROCALHA LISA GALVANIZADA A FOGO, 150 X 50 MM, COM ACESSÓRIOS","m",null,37.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382134","ELETROCALHA LISA GALVANIZADA A FOGO, 250 X 100 MM, COM ACESSÓRIOS","m",null,64.76,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382195","ELETROCALHA PERFURADA GALVANIZADA A FOGO, 250 X 50 MM, COM ACESSÓRIOS","m",null,51.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382212","ELETROCALHA PERFURADA GALVANIZADA A FOGO, 150X100MM, COM ACESSÓRIOS","m",null,57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382214","ELETROCALHA PERFURADA GALVANIZADA A FOGO, 250X100MM, COM ACESSÓRIOS","m",null,68.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382263","TAMPA DE ENCAIXE PARA ELETROCALHA, GALVANIZADA A FOGO, L= 150MM","m",null,19.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ELETROCALHA E ACESSÓRIOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382303","SUPORTE PARA ELETROCALHA, GALVANIZADO A FOGO, 150X50MM","un",null,9.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382317","SUPORTE PARA ELETROCALHA, GALVANIZADO A FOGO, 500X100MM","un",null,16.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382322","MÃO FRANCESA SIMPLES, GALVANIZADA A FOGO, L= 300MM","un",null,14.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382332","MÃO FRANCESA DUPLA, GALVANIZADA A FOGO, L= 400MM","un",null,28.84,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"382335","MÃO FRANCESA DUPLA, GALVANIZADA A FOGO, L= 700MM","un",null,42.28,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CONDUTOR E ENFIAÇÃO DE ENERGIA ELÉTRICA E TELEFONIA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390203","CABO DE COBRE DE 6 MM², ISOLAMENTO 750 V - ISOLAÇÃO EM PVC 70°C","m",null,3.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390208","CABO DE COBRE DE 50 MM², ISOLAMENTO 750 V - ISOLAÇÃO EM PVC 70°C","m",null,21.14,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390305","CABO DE COBRE DE 16 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EM PVC 70°C","m",null,7.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390313","CABO DE COBRE DE 185 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EM PVC 70°C","m",null,76.5,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390406","CABO DE COBRE NU, TÊMPERA MOLE, CLASSE 2, DE 25 MM²","m",null,9.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390418","CABO DE COBRE NU, TÊMPERA MOLE, CLASSE 2, DE 185 MM²","m",null,72.96,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390506","CABO DE COBRE DE 3X25 MM², TENSÃO DE ISOLAMENTO 8,7/15 KV - ISOLAÇÃO EPR 90°C","m",null,97.76,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CABO DE COBRE unIPOLAR, ISOLAMENTO 8,7/15 KV, ISOLAÇÃO EPR 90°C",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390602","CABO DE COBRE DE 70 MM², TENSÃO DE ISOLAMENTO 8,7/15 KV - ISOLAÇÃO EPR 90°C","m",null,63.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390703","CABO DE COBRE DE 4 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EPR 90°C","m",null,2.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390707","CABO DE COBRE DE 25 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EPR 90°C","m",null,11.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390709","CABO DE COBRE DE 50 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EPR 90°C","m",null,22.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390714","CABO DE COBRE DE 185 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EPR 90°C","m",null,74.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390808","CABO DE COBRE DE 3X35 MM², ISOLAMENTO 0,6/1 KV - ISOLAÇÃO EPR 90°C","m",null,46.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390904","CONECTOR SPLIT-BOLT PARA CABO DE 35 MM², LATÃO, SIMPLES","un",null,5.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"390916","CONECTOR SPLIT-BOLT PARA CABO DE 70 MM², LATÃO, COM RABICHO","un",null,11.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391001","TERMINAL DE PRESSÃO/COMPRESSÃO PARA CABO DE 300 MM²","un",null,24.96,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391006","TERMINAL DE PRESSÃO/COMPRESSÃO PARA CABO DE 6 ATÉ 10 MM²","un",null,5.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"FIOS E CABOS TELEFÔNICOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391104","CABO TELEFÔNICO CI, COM 20 PARES DE 0,50 MM, PARA CENTRAIS TELEFÔNICAS, EQUIPAMENTOS E REDE INTERNA","m",null,8.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391205","CABO DE COBRE FLEXÍVEL ´PP´ 3X2,5 MM², ISOLAMENTO 750 V - ISOLAÇÃO EM PVC 70°C","m",null,6.6,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391206","CABO DE COBRE FLEXÍVEL ´PP´ 3X4 MM², ISOLAMENTO 750 V - ISOLAÇÃO EM PVC 70°C","m",null,9.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391507","CABO DE ALUMÍNIO NU SEM ALMA DE AÇO CA, 2/0 AWG - ASTER","m",null,6.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"391811","CABO COAXIAL TIPO RGC 06","m",null,4.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392003","RECOLOCAÇÃO DE CONDUTOR APARENTE COM DIÂMETRO EXTERNO ACIMA DE 6,5 MM","m",null,6.78,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392601","CABO DE COBRE FLEXÍVEL DE 1,5 MM², ISOLAMENTO 0,6/1 KV - 90°C - BAIXA EMISSÃO DE FUMAÇA E GASES","m",null,1.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392602","CABO DE COBRE FLEXÍVEL DE 2,5 MM², ISOLAMENTO 0,6/1 KV - 90°C - BAIXA EMISSÃO DE FUMAÇA E GASES","m",null,2.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392605","CABO DE COBRE FLEXÍVEL DE 10 MM², ISOLAMENTO 0,6/1 KV - 90°C - BAIXA EMISSÃO DE FUMAÇA E GASES","m",null,6.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392607","CABO DE COBRE FLEXÍVEL DE 25 MM², ISOLAMENTO 0,6/1 KV - 90°C - BAIXA EMISSÃO DE FUMAÇA E GASES","m",null,12.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392614","CABO DE COBRE FLEXÍVEL DE 185 MM², ISOLAMENTO 0,6/1 KV - 90°C - BAIXA EMISSÃO DE FUMAÇA E GASES","m",null,80.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392703","CABO ÓPTICO MULTIMODO, 6 FIBRAS, 50/125 µM - USO INTERNO/EXTERNO","m",null,7.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"392712","CABO ÓPTICO MULTIMODO, NÚCLEO GELEADO, 6 FIBRAS, 50/125 µM - USO EXTERNO","m",null,7.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400202","CAIXA DE PASSAGEM EM CHAPA, COM TAMPA PARAFUSADA, 100 X 100 X 80 MM","un",null,15.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400208","CAIXA DE PASSAGEM EM CHAPA, COM TAMPA PARAFUSADA, 300 X 300 X 120 MM","un",null,52.28,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400244","CAIXA EM ALUMÍNIO FunDIDO À PROVA DE TEMPO, UMIDADE, GASES, VAPORES E PÓ, 150 X 150 X 150 MM","un",null,106.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400260","CAIXA DE PASSAGEM EM ALUMÍNIO FunDIDO À PROVA DE TEMPO, 100 X 100 MM","un",null,16.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400262","CAIXA DE PASSAGEM EM ALUMÍNIO FunDIDO À PROVA DE TEMPO, 300 X 300 MM","un",null,80.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400414","TOMADA 3P+T DE 32 A, BLINDADA INDUSTRIAL DE SOBREPOR NEGATIVA","cj",null,40.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400435","TOMADA RJ 45 PARA REDE DE DADOS, COM PLACA","un",null,31.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400446","TOMADA 2P+T DE 20 A - 250 V, COMPLETA","cj",null,14.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400501","MINUTERIA INDIVIDUAL 110/220 V, PARA LÂMPADAS INCANDESCENTES, COM PULSADOR LUMINOSO E PLACA","cj",null,141.76,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400504","INTERRUPTOR COM 2 TECLAS SIMPLES E PLACA","cj",null,15.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400510","INTERRUPTOR COM 2 TECLAS PARALELO E PLACA","cj",null,17.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400516","INTERRUPTOR COM 3 TECLAS, 1 SIMPLES, 2 PARALELO E PLACA","cj",null,22.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400606","CONDULETE METÁLICO DE 1´","cj",null,28.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400608","CONDULETE METÁLICO DE 1 1/4´","cj",null,36.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"400617","CONDULETE METÁLICO DE 4´","cj",null,170.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401002","CONTATOR DE POTÊNCIA 9 A - 2NA+2NF","un",null,106.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401004","CONTATOR DE POTÊNCIA 12 A - 2NA+2NF","un",null,116.14,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401015","CONTATOR DE POTÊNCIA DE 220 A - 2NA + 2NF","un",null,2301.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401106","RELÉ DE TEMPO ELETRÔNICO DE 0,6 ATÉ 6 SEG. - 220V - 50/60 HZ","un",null,72.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401107","RELÉ SUPERVISOR TRIFÁSICO CONTRA FALTA DE FASE, INVERSÃO DE FASE E MÍNIMA TENSÃO","un",null,1077.15,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401124","RELÉ DE TEMPO ELETRÔNICO DE 3 - 30SEG 220V 50/60HZ","un",null,74.49,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401220","CHAVE COMUTADORA/SELETORA COM 1 PÓLO E 2 POSIÇÕES PARA 25 A","un",null,69.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"401403","VOLTÍMETRO DE FERRO MÓVEL DE 96 X 96 MM, ESCALAS VARIÁVEIS DE 0/150 V, 0/250 V, 0/300 V, 0/500 V E 0/600 V","un",null,136.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"402002","PLUGUE COM 3P+T DE 63 A, 220/240 V, INDUSTRIAL","un",null,87.17,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"402007","BOTÃO DE COMANDO DUPLO COM SINALIZADOR","un",null,74.39,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"402011","ALARME SONORO BITONAL 220 V PARA PAINEL DE COMANDO","un",null,205.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"402033","PLACA/ESPELHO EM LATÃO ESCOVADO 4´ X 4´, PARA TOMADA DE LÓGICA RJ-45","un",null,24.5,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410524","LÂMPADA DE VAPOR DE SÓDIO ELIPSOIDAL OU TUBULAR, BASE E40 DE 250 W","un",null,25.28,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410533","LÂMPADA DE VAPOR DE SÓDIO TUBULAR STANDBY, BASE E40 DE 400 W","un",null,33.89,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410563","LÂMPADA DE VAPOR METÁLICO TUBULAR, BASE E40 DE 2000 W","un",null,378.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410610","LÂMPADA HALÓGENA REFLETORA PAR20, BASE E27 DE 50 W - 220 V","un",null,12.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410703","LÂMPADA FLUORESCENTE TUBULAR, BASE BIPINO BILATERAL DE 16 W","un",null,4.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410712","LÂMPADA FLUORESCENTE TUBULAR, BASE BIPINO BILATERAL DE 54 W","un",null,12.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410740","LÂMPADA FLUORESCENTE COMPACTA ELETRÔNICA ´2U´, BASE E27 DE 9 W - 110 OU 220 V","un",null,7.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410807","TRANSFORMADOR 300 W - 220 V/12 V PARA ATÉ 05 MINI REFLETORES DE USO SUBMERSO","un",null,234.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410827","REATOR ELETROMAGNÉTICO DE ALTO FATOR DE POTÊNCIA, PARA LÂMPADA VAPOR DE SÓDIO 400 W / 220 V","un",null,83.84,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410842","REATOR ELETROMAGNÉTICO DE ALTO FATOR DE POTÊNCIA, PARA LÂMPADA VAPOR METÁLICO 70 W / 220 V","un",null,50.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410845","REATOR ELETROMAGNÉTICO DE ALTO FATOR DE POTÊNCIA, PARA LÂMPADA VAPOR METÁLICO 250 W / 220 V","un",null,60.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410917","REATOR ELETROMAGNÉTICO DE ALTO FATOR DE POTÊNCIA COM PARTIDA RÁPIDA, PARA DUAS LÂMPADAS FLUORESCENTES TUBULARES ´HO´, BASE BIPINO BILATERAL, 110 W - 220 V","un",null,90.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410961","REATOR ELETRÔNICO DE ALTO FATOR DE POTÊNCIA COM PARTIDA INSTANTÂNEA, PARA DUAS LÂMPADAS FLUORESCENTES TUBULARES, BASE BIPINO BILATERAL, 28 W - 220 V","un",null,41.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"410972","REATOR ELETRÔNICO DE ALTO FATOR DE POTÊNCIA COM PARTIDA INSTANTÂNEA, PARA DUAS LÂMPADAS FLUORESCENTES TUBULARES, BASE BIPINO BILATERAL, 16 W - 127 V / 220 V","un",null,23.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"POSTES E ACESSÓRIOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411007","CRUZETA REFORÇADA EM FERRO GALVANIZADO PARA FIXAÇÃO DE QUATRO LUMINÁRIAS","un",null,274.01,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411026","POSTE TELECÔNICO CURVO EM AÇO SAE 1010/1020 GALVANIZADO A FOGO, ALTURA DE 8,00 M","un",null,1066.61,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411032","POSTE TELECÔNICO RETO EM AÇO SAE 1010/1020 GALVANIZADO A FOGO, ALTURA DE 15,00 M","un",null,2147.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411044","POSTE TUBULAR RETO EM AÇO SAE 1010/1020, SEÇÃO QUADRADA, ALTURA DE 7,50 M","un",null,338.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411111","LUMINÁRIA RETANGULAR FECHADA PARA ILUMINAÇÃO EXTERNA EM POSTE, TIPO PÉTALA PEQUENA","un",null,205.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411206","PROJETOR RETANGULAR FECHADO, PARA LÂMPADAS VAPOR DE SÓDIO 1000 W E VAPOR METÁLICO 2000 W","un",null,623.16,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411208","PROJETOR RETANGULAR FECHADO, PARA LÂMPADAS VAPOR METÁLICO E SÓDIO 250/400W","un",null,213.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411219","PROJETOR DE SOBREPOR COM FOCO ORIENTÁVEL, PARA LÂMPADA VALOR METÁLICO OU VAPOR DE SÓDIO 250/400 W","un",null,386.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"APARELHO DE ILUMINAÇÃO COMERCIAL E INDUSTRIAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411418","LUMINÁRIA INDUSTRIAL PENDENTE PARA INSTALAÇÃO EM PERFILADO COM REFLETOR ACRÍLICO REDONDO, PARA 1 LÂMPADA VAPOR METÁLICO ATÉ 400W","un",null,256.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411428","LUMINÁRIA DE SOBREPOR EM CALHA ABERTA COM CABECEIRAS PARA 2 LÂMPADAS FLUORESCENTES 32/36W","un",null,60.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411432","LUMINÁRIA DE SOBREPOR, TIPO SPOT ORIENTÁVEL RETANGULAR PARA 1 LÂMPADA DE VAPOR METÁLICO DE 70/150W","un",null,163.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411443","LUMINÁRIA DE EMBUTIR EM CALHA COM REFLETOR E ALETA PARABÓLICAS, COM ACABAMENTO ALTO BRILHO, PARA 4 LÂMPADAS FLUORESCENTES DE 16 W","un",null,112.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411455","LUMINÁRIA DE EMBUTIR EM CALHA COM ALETAS DUPLO PARABÓLICAS PARA 2 LÂMPADAS FLUORESCENTES DE 28 W","un",null,106.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"411506","LUMINÁRIA DE EMBUTIR EM FORRO, MÉDIA PARA 1 LÂMPADA INCANDESCENTE ATÉ 100W","un",null,41.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"LUMINÁRIA E ACESSÓRIOS ESPECIAIS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420106","LUVA DE REDUÇÃO GALVANIZADA DE 2´ X 3/4´","un",null,26.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420302","ISOLADOR GALVANIZADO PARA MASTRO DE DIÂMETRO 2´, SIMPLES COM 1 DESCIDA","un",null,10.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420404","APOIO PARA MASTRO DE DIÂMETRO 2´","un",null,11.44,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420412","MASTRO SIMPLES GALVANIZADO DE DIÂMETRO 2´","m",null,39.92,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420416","SUPORTE PORTA BANDEIRA REFORÇADO PARA MASTRO DE DIÂMETRO 2´","un",null,19.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420501","SINALIZADOR DE OBSTÁCULO SIMPLES, SEM CÉLULA FOTOELÉTRICA","un",null,23.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420514","CONECTOR OLHAL CABO/HASTE DE 3/4´","un",null,5.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420541","SUPORTE PARA FIXAÇÃO DE TERMINAL AÉREO E/OU DE CABO DE COBRE NU, COM BASE ONDULADA","un",null,8.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420545","CONECTOR COM RABICHO E PORCA EM LATÃO PARA CABO DE 16 A 35 MM²","un",null,9.81,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420551","SUPORTE PARA FIXAÇÃO DE FITA DE ALUMÍNIO 7/8´ X 1/8´  E/OU CABO DE COBRE NÚ, COM BASE ONDULADA","un",null,8.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420552","SUPORTE PARA FIXAÇÃO DE FITA DE ALUMÍNIO 7/8´ X 1/8´ , COM BASE PLANA","un",null,7.98,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"420558","TERMINAL ESTANHADO COM 1 FURO E 1 COMPRESSÃO - 35 MM²","un",null,7.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"422005","SOLDA EXOTÉRMICA TIPO ´RR´ CABO-BARRA","un",null,21.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"422012","SOLDA EXOTÉRMICA CONEXÃO CABO-CABO HORIZONTAL EM X SOBREPOSTO, BITOLA DO CABO DE 35-35MM² A 50-35MM²","un",null,20.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"422016","SOLDA EXOTÉRMICA CONEXÃO CABO-CABO HORIZONTAL EM T, BITOLA DO CABO DE 50-50MM² A 95-50MM²","un",null,19.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"422017","SOLDA EXOTÉRMICA CONEXÃO CABO-CABO HORIZONTAL RETO, BITOLA DO CABO DE 16MM² A 70MM²","un",null,16.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"422020","SOLDA EXOTÉRMICA CONEXÃO CABO-HASTE EM X SOBREPOSTO, BITOLA DO CABO DE 70MM² A 95MM² PARA HASTE DE 5/8 E 3/4","un",null,26.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"422031","SOLDA EXOTÉRMICA CONEXÃO CABO-SUPERFÍCIE DE AÇO, BITOLA DO CABO DE 16MM² A 35MM²","un",null,16.58,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"APARELHOS ELÉTRICOS, HIDRÁULICOS E A GÁS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"BEBEDOUROS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"430207","CHUVEIRO, COM VÁLVULA DE ACIONAMENTO, ANTIVANDALISMO, DN= 3/4´","cj",null,377.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"430214","CHUVEIRO ELÉTRICO DE 5500 W / 220 V EM PVC","un",null,59.5,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"430303","AQUECEDOR A GÁS, CAPACIDADE 2.000 L, POTÊNCIA DE 60.000 KCAL/H","un",null,16707.58,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"430313","AQUECEDOR A GÁS DE ACUMULAÇÃO, CAPACIDADE 500 L","un",null,6398.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"430321","AQUECEDOR DE PASSAGEM ELÉTRICO INDIVIDUAL, BAIXA PRESSÃO, 5.100 W / 127 V OU 5.200 W / 220 V","un",null,674.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"EMISSORES DE SOM",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"BOMBAS CENTRÍFUGAS - USO GERAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431005","CONJunTO MOTOR-BOMBA (CENTRÍFUGA) 10 CV MONOESTÁGIO, HMAN= 24 A 36 MCA,Q= 53 A 45 M³/H","un",null,3808.49,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431009","CONJunTO MOTOR-BOMBA (CENTRÍFUGA) 20 CV MONOESTÁGIO, HMAN= 40 A 70 MCA, Q= 76 A 28 M³/H","un",null,6389,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431013","CONJunTO MOTOR-BOMBA (CENTRÍFUGA) 3/4 CV MONOESTÁGIO, HMAN= 10 A 16 MCA, Q= 12,7 A 8 M³/H","un",null,1065.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431021","CONJunTO MOTOR-BOMBA (CENTRÍFUGA) 60 CV MONOESTÁGIO, HMAN= 90 A 125 MCA, Q= 115 A 50 M³/H","un",null,19198.07,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431023","CONJunTO MOTOR-BOMBA (CENTRÍFUGA) 2 CV MONOESTÁGIO, HMAN= 12 A 27 MCA, Q= 25 A 8 M³/H","un",null,1261.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431104","CONJunTO MOTOR-BOMBA SUBMERSÍVEL PARA POÇO PROFunDO DE 6´, Q= 5 A 13 M³/H, HMAN= 279 A 153 MCA, 12,5 HP","un",null,6370.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431108","CONJunTO MOTOR-BOMBA SUBMERSÍVEL PARA POÇO PROFunDO DE 6´, Q= 10 A 20M³/H, HMAN= 164 A 98 MCA, 12,5 HP","un",null,5737.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431110","CONJunTO MOTOR-BOMBA SUBMERSÍVEL PARA POÇO PROFunDO DE 6´, Q= 10 A 20M³/H, HMAN= 274 A 170 MCA, 20 HP","un",null,8407.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431136","CONJunTO MOTOR-BOMBA SUBMERSÍVEL VERTICAL PARA ÁGUAS RESIDUAIS, Q= 2 A16 M³/H, HMAN= 12 A 2 MCA, POTÊNCIA DE 0,5 CV","un",null,1361.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431140","CONJunTO MOTOR-BOMBA SUBMERSÍVEL VERTICAL PARA ESGOTO, Q= 3,4 A 86,3 M³/H, HMAN= 14 A 5 MCA, POTÊNCIA 5 CV","un",null,7903.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431208","BOMBA DOSADORA TIPO DIAFRAGMA COM SENSOR DE NÍVEL, VAZÃO ATÉ 1,5 L/H PARA PRESSÃO MÁXIMA 12 BAR","un",null,1029.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431210","BOMBA DOSADORA TIPO DIAFRAGMA COM SENSOR DE NÍVEL, VAZÃO ATÉ 8,0 L/H PARA PRESSÃO MÁXIMA 10 BAR","un",null,1374.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"431212","BOMBA DOSADORA TIPO DIAFRAGMA COM SENSOR DE NÍVEL, VAZÃO ATÉ 15,0 L/H PARA PRESSÃO MÁXIMA 4 BAR","un",null,1885.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440110","LAVATÓRIO DE LOUÇA SEM COLUNA","un",null,77.96,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440117","LAVATÓRIO EM POLIPROPILENO","un",null,30.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440127","CUBA DE LOUÇA DE EMBUTIR OVAL","un",null,70.1,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440134","TANQUE SIMPLES EM CONCRETO PRÉ-MOLDADO","un",null,62.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440170","BANHEIRA EM FIBRA DE VIDRO SEM HIDROMASSAGEM","un",null,994.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440210","TAMPO/BANCADA EM MÁRMORE NACIONAL ESPESSURA DE 3 CM","m²",null,816.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440321","DUCHA CROMADA SIMPLES","un",null,55.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440331","TORNEIRA DE MESA PARA LAVATÓRIO, ACIONAMENTO HIDROMECÂNICO, COM REGISTRO INTEGRADO REGULADOR DE VAZÃO, EM LATÃO CROMADO, DN= 1/2´","un",null,430.29,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440343","TORNEIRA CURTA SEM ROSCA PARA USO GERAL, EM LATÃO FunDIDO CROMADO, DN= 1/2´","un",null,22.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440359","TORNEIRA DE MESA PARA PIA COM BICA MÓVEL E AREJADOR EM LATÃO FunDIDO CROMADO","un",null,112.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440387","DUCHA HIGIÊNICA BRANCA DE PVC","un",null,64.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440393","DESVIADOR PARA DUCHA ELÉTRICA","un",null,45.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440403","PRATELEIRA EM GRANITO COM ESPESSURA DE 2 CM","m²",null,304.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440631","CUBA EM AÇO INOXIDÁVEL SIMPLES DE 465X300X140MM","un",null,141.89,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440640","CUBA EM AÇO INOXIDÁVEL SIMPLES DE 500X400X300MM","un",null,443.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"440651","CUBA EM AÇO INOXIDÁVEL SIMPLES DE 600X400X400MM","un",null,630.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"442002","RECOLOCAÇÃO DE TORNEIRAS","un",null,11.98,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"442015","ACABAMENTO CROMADO PARA REGISTRO","un",null,25.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"442024","SIFÃO PLÁSTICO COM COPO, RÍGIDO, DE 1´ X 1 1/2´","un",null,19.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"442030","BOLSA PARA BACIA SANITÁRIA","un",null,6.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"442062","VÁLVULA AMERICANA","un",null,25.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"442070","ESPARGIDOR DE FERRO GALVANIZADO PARA MICTÓRIO TIPO COCHO","m",null,36.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"450104","ENTRADA COMPLETA DE ÁGUA COM ABRIGO E REGISTRO DE GAVETA, DN= 1´","un",null,693.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"450106","ENTRADA COMPLETA DE ÁGUA COM ABRIGO E REGISTRO DE GAVETA, DN= 1 1/2´","un",null,1671.81,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ENTRADA DE GÁS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"450202","ENTRADA COMPLETA DE GÁS GLP DOMICILIAR COM 2 BUJÕES DE 13 KG","un",null,1144.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"450302","HIDRÔMETRO EM FERRO FunDIDO, DIÂMETRO 80 MM (3´)","un",null,2286.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"450310","HIDRÔMETRO EM BRONZE, DIÂMETRO DE 25 MM (1´)","cj",null,419.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"450321","FILTRO TIPO CESTO PARA HIDRÔMETRO DE 80 MM (3´)","un",null,1400.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460103","TUBO DE PVC RÍGIDO, DN= 32 MM, (1´), INCLUSIVE CONEXÕES","m",null,21.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460109","TUBO DE PVC RÍGIDO, DN= 110 MM, (4´), INCLUSIVE CONEXÕES","m",null,77.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460401","TUBO DE PVC RÍGIDO TIPO PBA CLASSE 15, DN= 50MM, (DE= 60MM), INCLUSIVE CONEXÕES","m",null,16.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460505","TUBO PVC RÍGIDO, JunTA ELÁSTICA, TIPO VINILFORT, DN= 200 MM, INCLUSIVE CONEXÕES","m",null,54.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460509","TUBO PVC RÍGIDO, JunTA ELÁSTICA, TIPO VINILFORT, DN= 400 MM, INCLUSIVE CONEXÕES","m",null,177.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460703","TUBO DE FERRO GALVANIZADO DN= 1´, INCLUSIVE CONEXÕES","m",null,53.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460810","TUBO AÇO GALVANIZADO SEM COSTURA SCHEDULE 40, DN= 4´, INCLUSIVE CONEXÕES","m",null,227.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460913","JOELHO 87° 30´ EM FERRO FunDIDO, LINHA PREDIAL TRADICIONAL, DN= 150 MM","un",null,196.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460921","PLACA CEGA EM FERRO FunDIDO, LINHA PREDIAL TRADICIONAL, DN= 100 MM","un",null,38.98,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460924","JunÇÃO 45° EM FERRO FunDIDO, LINHA PREDIAL TRADICIONAL, DN= 75 X 50 MM","un",null,111.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460928","JunÇÃO 45° EM FERRO FunDIDO, LINHA PREDIAL TRADICIONAL, DN= 100 X 100 MM","un",null,169.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"460930","JunÇÃO DUPLA 45° EM FERRO FunDIDO, LINHA PREDIAL TRADICIONAL, DN= 100 MM","un",null,191.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461005","TUBO DE COBRE CLASSE A, DN= 42MM (1 1/2´), INCLUSIVE CONEXÕES","m",null,92.07,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461020","TUBO DE COBRE CLASSE E, DN= 22MM (3/4´), INCLUSIVE CONEXÕES","m",null,36.58,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461023","TUBO DE COBRE CLASSE E, DN= 42MM (1 1/2´), INCLUSIVE CONEXÕES","m",null,70.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461202","TUBO DE CONCRETO (PS-1), DN= 400MM","m",null,61.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461205","TUBO DE CONCRETO (PS-2), DN= 300MM","m",null,55.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461211","TUBO DE CONCRETO (PA-1), DN= 900MM","m",null,254.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461217","TUBO DE CONCRETO (PA-2), DN= 1000MM","m",null,317.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461219","TUBO DE CONCRETO (PA-3), DN= 800MM","m",null,276.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461229","TUBO DE CONCRETO (PA-2), DN= 700MM","m",null,221.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461232","TUBO DE CONCRETO (PA-1), DN= 300MM","m",null,76.89,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461305","TUBO EM POLIETILENO DE ALTA DENSIDADE CORRUGADO PERFURADO, DN= 6´, INCLUSIVE CONEXÕES","m",null,27.98,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461306","TUBO EM POLIETILENO DE ALTA DENSIDADE CORRUGADO PERFURADO, DN= 12´, INCLUSIVE CONEXÕES","m",null,64.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TUBULAÇÃO E CONEXÕES FLANGEADAS EM FERRO DÚCTIL PARA REDES SANEAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461803","TUBO EM FERRO FunDIDO COM PONTA E PONTA TCLA - DN= 150MM, SEM JunTAS E CONEXÕES","m",null,351.5,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461808","TUBO EM FERRO FunDIDO COM PONTA E PONTA TCLA - DN= 400MM, SEM JunTAS E CONEXÕES","m",null,921.42,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461815","FLANGE AVULSO EM FERRO FunDIDO, CLASSE PN-10, DN= 350MM","un",null,377.44,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461819","CURVA DE 90° EM FERRO FunDIDO, COM FLANGES, CLASSE PN-10, DN= 150MM","un",null,310.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TUBULAÇÃO E CONEXÕES FLANGEADAS EM FERRO DÚCTIL PARA REDES SANEAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461930","CURVA DE 90° EM FERRO FunDIDO COM FLANGES, CLASSE PN-10, DN= 50MM","un",null,129.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461950","REDUÇÃO EXCÊNTRICA EM FERRO FunDIDO, COM FLANGES, CLASSE PN-10, DN= 100MM X 80MM","un",null,359.67,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"461953","REDUÇÃO EXCÊNTRICA EM FERRO FunDIDO, COM FLANGES, CLASSE PN-10, DN= 250MM X 150/200MM","un",null,709.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TUBULAÇÃO COM CONEXÕES EM AÇO PRETO CLASSE SCHEDULE",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462106","TUBO DE AÇO CARBONO PRETO SEM COSTURA SCHEDULE 40, DN= 3´ - INCLUSIVE CONEXÕES","m",null,142.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462110","TUBO DE AÇO CARBONO PRETO SEM COSTURA SCHEDULE 40, DN= 6´ - INCLUSIVE CONEXÕES","m",null,289.72,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462113","TUBO DE AÇO CARBONO PRETO SEM COSTURA SCHEDULE 40, DN= 3 1/2´ - INCLUSIVE CONEXÕES","m",null,166.6,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462158","TUBO DE AÇO CARBONO PRETO COM COSTURA SCHEDULE 40, DN= 10´ - INCLUSIVE CONEXÕES","m",null,449.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462305","TUBO DE CONCRETO CLASSE EA-2, DN= 800 MM","m",null,327.98,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462315","TUBO DE CONCRETO CLASSE EA-3, DN= 800 MM","m",null,373.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462316","TUBO DE CONCRETO CLASSE EA-3, DN= 900 MM","m",null,433.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462610","JunTA DE unIÃO EM AÇO INOXIDÁVEL COM PARAFUSO DE AÇO ZINCADO, PARA TUBO EM FERRO FunDIDO PREDIAL SMU, DN= 200 MM","un",null,107.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462643","JOELHO 45° EM FERRO FunDIDO, PREDIAL SMU, DN= 150 MM","un",null,205.14,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462647","JOELHO 88° EM FERRO FunDIDO, PREDIAL SMU, DN= 75 MM","un",null,107.78,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462652","JunÇÃO 45° EM FERRO FunDIDO, PREDIAL SMU, DN= 75 X 75 MM","un",null,175.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462653","JunÇÃO 45° EM FERRO FunDIDO, PREDIAL SMU, DN= 75 X 50 MM","un",null,165.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462680","ABRAÇADEIRA DENTADA PARA TRAVAMENTO EM AÇO INOXIDÁVEL, COM PARAFUSO DE AÇO ZINCADO, PARA TUBO EM FERRO FunDIDO PREDIAL SMU, DN= 50 MM","un",null,244.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"462682","ABRAÇADEIRA DENTADA PARA TRAVAMENTO EM AÇO INOXIDÁVEL, COM PARAFUSO DE AÇO ZINCADO, PARA TUBO EM FERRO FunDIDO PREDIAL SMU, DN= 100 MM","un",null,310.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TUBULAÇÃO COM CONEXÕES EM COBRE, PARA SISTEMA DE AR CONDICIONADO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470101","REGISTRO DE GAVETA EM LATÃO FunDIDO SEM ACABAMENTO, DN= 1/2´","un",null,30.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470109","REGISTRO DE GAVETA EM LATÃO FunDIDO SEM ACABAMENTO, DN= 4´","un",null,585.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470204","REGISTRO DE GAVETA EM LATÃO FunDIDO CROMADO COM CANOPLA, DN= 1 1/4´ - LINHA ESPECIAL","un",null,96.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470210","REGISTRO DE PRESSÃO EM LATÃO FunDIDO CROMADO COM CANOPLA, DN= 1/2´ - LINHA ESPECIAL","un",null,60.84,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470220","REGISTRO REGULADOR DE VAZÃO PARA CHUVEIRO E DUCHA EM LATÃO CROMADO COM CANOPLA, DN= 1/2´","un",null,51.44,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470403","VÁLVULA DE DESCARGA COM REGISTRO PRÓPRIO, DN= 1 1/4´","un",null,176.25,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470408","VÁLVULA DE DESCARGA EXTERNA, TIPO ALAVANCA COM REGISTRO PRÓPRIO, DN= 1 1/4´ E DN= 1 1/2´","un",null,376.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470503","VÁLVULA DE RETENÇÃO HORIZONTAL EM BRONZE, DN= 1 1/4´","un",null,85.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470509","VÁLVULA DE RETENÇÃO VERTICAL EM BRONZE, DN= 3/4´","un",null,46.29,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470514","VÁLVULA DE RETENÇÃO VERTICAL EM BRONZE, DN= 2 1/2´","un",null,179.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470520","VÁLVULA DE RETENÇÃO DE PÉ COM CRIVO EM BRONZE, DN= 2´","un",null,95.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470523","VÁLVULA DE GAVETA EM BRONZE, CLASSE 125 LIBRAS PARA VAPOR E CLASSE 200 LIBRAS PARA ÁGUA, ÓLEO E GÁS, DN= 2´","un",null,107.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470526","VÁLVULA DE RETENÇÃO DE PÉ COM CRIVO EM BRONZE, DN= 3´","un",null,209.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470542","VÁLVULA DE GAVETA EM BRONZE, CLASSE 125 LIBRAS PARA VAPOR E CLASSE 200 LIBRAS PARA ÁGUA, ÓLEO E GÁS, DN= 2 1/2´","un",null,201.95,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470544","VÁLVULA GLOBO EM BRONZE, CLASSE 150 LIBRAS PARA VAPOR SATURADO E 300 LIBRAS PARA ÁGUA, ÓLEO E GÁS, DN= 3´","un",null,752.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470557","VÁLVULA DE GAVETA EM BRONZE, HASTE ASCENDENTE, CLASSE 150 LIBRAS PARA VAPOR SATURADO E 300 LIBRAS PARA ÁGUA, ÓLEO E GÁS, DN= 4´","un",null,2164.6,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REGISTRO E / OU VÁLVULA EM FERRO FunDIDO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470607","VÁLVULA DE GAVETA EM FERRO FunDIDO COM BOLSA, DN= 200 MM","un",null,1496.09,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470632","VÁLVULA DE GOVERNO (RETENÇÃO E ALARME) COMPLETA, CORPO EM FERRO FunDIDO, CLASSE 125 LIBRAS, DN= 4´","cj",null,4056.28,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470634","VÁLVULA DE GAVETA EM FERRO FunDIDO, HASTE ASCENDENTE COM FLANGE, CLASSE 125 LIBRAS, DN= 6´","un",null,1298.66,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470710","VÁLVULA ESFERA EM AÇO CARBONO FunDIDO, PASSAGEM REDUZIDA, CLASSE 150 LIBRAS PARA VAPOR E CLASSE 600 LIBRAS PARA ÁGUA, ÓLEO E GÁS, DN= 1/2´","un",null,43.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"470903","VÁLVULA GLOBO EM AÇO CARBONO FORJADO, CLASSE 800 LIBRAS PARA VAPOR E CLASSE 2000 LIBRAS PARA ÁGUA, ÓLEO E GÁS, DN= 1 1/2´","un",null,410.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"471110","MANÔMETRO COM MOSTRADOR DE 4´, ESCALAS: 0-4 / 0-7 / 0-10 / 0-17 / 0-21 / 0-28 KG/CM²","un",null,79.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"471227","VÁLVULA DE GAVETA EM FERRO DÚCTIL COM FLANGES, CLASSE PN-10, DN= 80MM","un",null,588.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"472002","FILTRO ´Y´ EM BRONZE PARA GÁS COMBUSTÍVEL, DN= 2´","un",null,195.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"472008","REGULADOR DE PRIMEIRO ESTÁGIO DE ALTA PRESSÃO ATÉ 2KGF/CM², VAZÃO DE 90KG GLP/HORA","un",null,363.61,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"472030","CHAVE DE FLUXO DE ÁGUA COM RETARDO PARA TUBULAÇÕES COM DIÂMETRO NOMINAL DE 1´ A 6´ - CONEXÃO BSP","un",null,273.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"480201","RESERVATÓRIO DE FIBRA DE VIDRO - CAPACIDADE DE 15.000 LITROS","un",null,3763.61,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"480230","RESERVATÓRIO EM POLIETILENO DE ALTA DENSIDADE (CISTERNA) COM ANTIOXIDANTE E PROTEÇÃO CONTRA RAIOS ULTRAVIOLETA (UV) - CAPACIDADE DE 5.000 LITROS","cj",null,5496.38,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"RESERVATÓRIO METÁLICO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"480502","TORNEIRA DE BÓIA, DN= 1´","un",null,55.26,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"480505","TORNEIRA DE BÓIA, DN= 2´","un",null,117.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"482002","LIMPEZA DE CAIXA D´ÁGUA ATÉ 1.000 LITROS","un",null,29.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CAIXA, RALO, GRELHA E ACESSÓRIO HIDRÁULICO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CAIXAS SIFONADAS DE PVC RÍGIDO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"490104","CAIXA SIFONADA DE PVC RÍGIDO DE 150 X 185 X 75 MM, COM GRELHA","un",null,47.81,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"490614","GRELHA REDONDA COM DISCO ROTATIVO EM AÇO INOXIDÁVEL DE 15 CM","un",null,11.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"491210","CAIXA COLETORA EM CONCRETO ARMADO 0,30 X 0,70 X 1,00 M","un",null,430.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"491303","FILTRO BIOLÓGICO ANAERÓBIO COM ANÉIS PRÉ-MOLDADOS DE CONCRETO DIÂMETRO DE 2,40 M - H= 2,00 M","un",null,7403.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500106","ABRIGO PARA HIDRANTE/MANGUEIRA (EMBUTIR E EXTERNO)","un",null,262.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500120","TAMPÃO DE ENGATE RÁPIDO EM LATÃO, DN= 1 1/2´, COM CORRENTE","un",null,32.81,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500202","BICO DE SPRINKLER CROMADO PENDENTE COM ROMPIMENTO DA AMPOLA A 68°C","un",null,23.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500506","CENTRAL DE ILUMINAÇÃO DE EMERGÊNCIA, COMPLETA, PARA ATÉ 6.000 W","un",null,9014.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500516","MÓDULO PARA ADAPTAÇÃO DE LUMINÁRIA DE EMERGÊNCIA, AUTONOMIA 90 MINUTOS PARA LÂMPADA FLUORESCENTE DE 32 W","un",null,147.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500526","BLOCO AUTÔNOMO DE ILUMINAÇÃO DE EMERGÊNCIA COM AUTONOMIA MÍNIMA DE 1 HORA, EQUIPADO COM 2 LÂMPADAS DE 11 W","un",null,165.49,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500531","BLOCO AUTÔNOMO DE ILUMINAÇÃO DE EMERGÊNCIA COM AUTONOMIA MÍNIMA DE 3 HORAS, EQUIPADO COM 2 FARÓIS DE LÂMPADAS DE 21/55 W","un",null,360.03,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500543","DETECTOR ÓPTICO DE FUMAÇA COM BASE - ENDEREÇÁVEL","un",null,136.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"500544","PAINEL REPETIDOR DE DETECÇÃO E ALARME DE INCÊNDIO TIPO ENDEREÇÁVEL","un",null,921.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"501011","EXTINTOR MANUAL DE PÓ QUÍMICO SECO ABC - CAPACIDADE DE 4 KG","un",null,128.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"501012","EXTINTOR MANUAL DE PÓ QUÍMICO SECO ABC - CAPACIDADE DE 6 KG","un",null,140.66,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"501022","SUPORTE PARA EXTINTOR DE PISO EM AÇO INOX","un",null,212.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PAVIMENTAÇÃO E PASSEIO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540103","ABERTURA E PREPARO DE CAIXA ATÉ 40 CM, COMPACTAÇÃO DO SUBLEITO MÍNIMO DE 95% DO PN E TRANSPORTE ATÉ O RAIO DE 1,0 KM","m²",null,11.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540120","BASE DE MACADAME HIDRÁULICO","m³",null,156.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540323","IMPRIMAÇÃO BETUMINOSA LIGANTE","m²",null,2,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540326","REVESTIMENTO DE PRÉ-MISTURADO A FRIO","m³",null,422.26,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540403","PAVIMENTAÇÃO EM PARALELEPÍPEDO, SEM REJunTE","m²",null,104.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540602","GUIA PRÉ-MOLDADA CURVA TIPO PMSP 100 - FCK 25 MPA","m",null,36.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540616","SARJETA OU SARJETÃO MOLDADO NO LOCAL, TIPO PMSP EM CONCRETO COM FCK 20 MPA","m³",null,405.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540712","PISO EM LADRILHO HIDRÁULICO VÁRIAS CORES 20 X 20 CM, ASSENTADO COM ARGAMASSA MISTA","m²",null,81.44,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"540721","REJunTAMENTO DE PISO EM LADRILHO HIDRÁULICO (20 X 20 X 1,8 CM) COM ARGAMASSA INDUSTRIALIZADA PARA REJunTE, JunTAS DE 2 MM","m²",null,6.43,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"542011","REASSENTAMENTO DE PARALELEPÍPEDOS, SEM REJunTE","m²",null,19.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"542013","REASSENTAMENTO DE PAVIMENTAÇÃO EM LAJOTA DE CONCRETO, ESPESSURA 8 CM, COM REJunTE EM AREIA","m²",null,13.8,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"550107","LIMPEZA COMPLEMENTAR E ESPECIAL DE PISO COM PRODUTOS QUÍMICOS","m²",null,2.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"550113","LIMPEZA E LAVAGEM DE SUPERFÍCIE REVESTIDA COM MATERIAL CERÂMICO OU PASTILHAS POR HIDROJATEAMENTO COM REJunTAMENTO","m²",null,6.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"550204","LIMPEZA E DESOBSTRUÇÃO DE BOCA DE LOBO","un",null,10.04,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"610176","ELEVADOR PARA PASSAGEIROS, USO INTERNO COM CAPACIDADE MÍNIMA DE 600 KG PARA QUATRO PARADAS, PORTAS BILATERAIS","cj",null,105250,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"612013","LIGAÇÃO TÍPICA, (CAVALETE), PARA AR CONDICIONADO ´FANCOIL´, DIÂMETRO DE 1 1/4´","cj",null,1246.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"612045","DUTO EM CHAPA DE AÇO GALVANIZADO","kg",null,22.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"COZINHA, REFEITÓRIO, LAVANDERIA INDUSTRIAL, EQUIPAMENTO E ACESSÓRIOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"MOBILIÁRIO E ACESSÓRIOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"620406","TANQUE DUPLO COM PÉS EM AÇO INOXIDÁVEL DE 1600 X 700 X 850 MM","un",null,2811.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"620407","MESA EM AÇO INOXIDÁVEL, LARGURA ATÉ 700 MM","m",null,1150.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"620409","MESA LATERAL EM AÇO INOXIDÁVEL COM PRATELEIRA INFERIOR, LARGURA ATÉ 700 MM","m",null,1898.36,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"622033","COIFA EM AÇO INOXIDÁVEL COM FILTRO E EXAUSTOR AXIAL - ÁREA ATÉ 3,00 M²","m²",null,7285.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"622034","COIFA EM AÇO INOXIDÁVEL COM FILTRO E EXAUSTOR AXIAL - ÁREA DE 3,01 ATÉ 7,50 M²","m²",null,5363.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"622035","COIFA EM AÇO INOXIDÁVEL COM FILTRO E EXAUSTOR AXIAL - ÁREA DE 7,51 ATÉ 16,00 M²","m²",null,2819.99,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"RESFRIAMENTO E CONSERVAÇÃO DE MATERIAL PERECIVEL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CÂMARA FRIGORÍFICA PARA RESFRIADO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"650121","CÂMARA FRIGORÍFICA PARA RESFRIADOS","m²",null,1999.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CÂMARA FRIGORÍFICA PARA CONGELADO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"650210","CÂMARA FRIGORÍFICA PARA CONGELADOS","m²",null,2400.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"SEGURANÇA, VIGILÂNCIA E CONTROLE, EQUIPAMENTOS E SISTEMA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CONTROLE DE ACESSOS E ALARME",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660206","REPETIDORA DE SINAIS DE OCORRÊNCIAS, DO PAINEL SINÓPTICO DA CENTRAL DE ALARME","un",null,734.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660209","DETECTOR DE METAIS, TIPO PORTAL, MICROPROCESSADO","un",null,5603.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660213","PORTEIRO ELETRÔNICO COM UM INTERFONE","cj",null,144.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660224","SISTEMA ELETRÔNICO DE AUTOMATIZAÇÃO DE PORTÃO DESLIZANTE, ESFORÇO ATÉ 1400 KG","cj",null,2755.54,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660246","VÍDEO PORTEIRO ELETRÔNICO COLORIDO, COM UM INTERFONE E FECHADURA ELÉTRICA","cj",null,1092.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660250","CENTRAL DE ALARME MICROPROCESSADA, PARA ATÉ 125 ZONAS","un",null,1423.09,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"EQUIPAMENTOS PARA SISTEMA DE SEGURANÇA, VIGILÂNCIA E CONTROLE",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660803","unIDADE GERENCIADORA DE VÍDEO LOCAL - DVR","un",null,33756.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660806","MANIPULADOR OU TECLADO PARA AS CÂMERAS MÓVEIS","un",null,5195.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660807","RACK FECHADO DE PISO PADRÃO METÁLICO, 19 X 44US X 770 MM","un",null,1992.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660808","GABINETE DE COMANDO E VISUALIZAÇÃO, COM MESA DE APOIO PARA ATÉ 3 MONITORES DE 17´ E 3 MONITORES DE 20´","un",null,11544.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660810","RACK FECHADO PADRÃO METÁLICO, 19 X 12 US X 470 MM","un",null,699.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660811","RACK FECHADO PADRÃO METÁLICO, 19 X 20 US X 470 MM","un",null,1187.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660812","MONITOR LCD COLORIDO TELA PLANA DE 17´","un",null,533.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660813","MONITOR LCD COLORIDO TELA PLANA DE 20´","un",null,715.34,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660816","LENTE COM DIÂMETRO DE 1/3´, COM FOCO VARIÁVEL ENTRE 3,5 MM A 8,0 MM","un",null,218.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660819","RACK FECHADO DE PISO PADRÃO METÁLICO, 19 X 24 US X 570 MM","un",null,1110.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660823","GRAVADOR E REPRODUTOR DE DVD","un",null,1281.01,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660824","FILTRO E MISTURADOR DE SINAIS","un",null,25.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660825","RECEPTOR DE SINAIS VIA SATÉLITE PARA 8 CANAIS (RACK)","un",null,2292.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660826","MODULADOR DE CANAIS","un",null,176.44,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"660827","AMPLIFICADOR DE LINHA VHF + UHF COM CONECTOR DE F50 DB","un",null,360.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662015","GUIA ORGANIZADORA DE CABOS PARA RACK, 19´ 1 U","un",null,20.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662016","SWITCH 24 PORTAS COM CAPACIDADE DE 10/100/1000/MBPS","cj",null,1495.85,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662017","GUIA ORGANIZADORA DE CABOS PARA RACK, 19´ 2 U","un",null,28.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662018","CAIXA DE PROTEÇÃO COM SUPORTE PARA CÂMERA FIXA INTERNA OU EXTERNA","un",null,58.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662019","SUPORTE PARA CÂMERA DOME","un",null,226.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662020","INSTALAÇÃO DE CÂMERA FIXA, PARA CFTV","un",null,398.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"662021","INSTALAÇÃO DE CÂMERA MÓVEL, PARA CFTV","un",null,796.92,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"CAPTAÇÃO, ADUÇÃO E TRATAMENTO DE ÁGUA E ESGOTO, EQUIPAMENTOS E SISTEMA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TRATAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670204","MEDIDOR DE VAZÃO TIPO CALHA PARSHALL COM GARGANTA W= 6´","un",null,1270.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670216","MEDIDOR DE VAZÃO TIPO CALHA PARSHALL COM GARGANTA W= 3´","un",null,808.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670218","GRADE FINA EM AÇO CARBONO, ESPAÇAMENTO DE 3 CM, COM BARRAS CHATAS DE 1´X 1/4´","m²",null,854.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670219","GRADE GROSSA EM AÇO CARBONO, ESPAÇAMENTO DE 5 CM, COM BARRAS CHATAS DE 1´ X 1/4´","m²",null,659.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670221","TELA GALVANIZADA REVESTIDA EM POLIAMIDA, MALHA DE 10 MM","m²",null,392.18,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670223","GRADE FINA EM AÇO CARBONO, ESPAÇAMENTO 1 CM COM BARRAS CHATAS DE 1´ X 3/8´","m²",null,1381.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670224","GRADE MÉDIA EM AÇO CARBONO, ESPAÇAMENTO 2 CM COM BARRAS CHATAS DE 1´ X 3/8´","m²",null,833.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670225","GRADE GROSSA EM AÇO CARBONO, ESPAÇAMENTO 4 CM COM BARRAS CHATAS DE 1´ X 3/8´","m²",null,726.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670228","CESTO EM CHAPA DE AÇO INOXIDÁVEL COM ESPESSURA DE 1,5 MM E FUROS DE 1/2´","un",null,502.41,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670229","ESTAÇÃO DE TRATAMENTO DE ESGOTO COMPACTA, VAZÃO MÁXIMA HORÁRIA 12,0 L/S, PARA OBRAS DE SEGURANÇA","gl",null,1208337.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"670232","COMPORTA EM FIBRA DE VIDRO (STOP LOG) - ESPESSURA DE 10 MM","m²",null,780.58,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ELETRIFICAÇÃO, EQUIPAMENTOS E SISTEMA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"POSTEAMENTO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680101","POSTE DE CONCRETO DUPLO ´T´ - 10/150","un",null,910.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680102","POSTE DE CONCRETO DUPLO ´T´ - 10/300","un",null,1066.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680103","POSTE DE CONCRETO DUPLO ´T´ - 10/600","un",null,1255,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680104","POSTE DE CONCRETO DUPLO ´T´ - 11/600","un",null,1417.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680110","POSTE DE CONCRETO TUBULAR CÔNICO - 11/200","un",null,1091.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680111","POSTE DE CONCRETO TUBULAR CÔNICO - 11/400","un",null,1302.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680112","POSTE DE CONCRETO TUBULAR CÔNICO - 11/600","un",null,1570.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680113","POSTE DE CONCRETO TUBULAR CÔNICO - 12/400","un",null,1452.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680114","POSTE DE CONCRETO TUBULAR CÔNICO - 12/600","un",null,1708.72,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680115","POSTE DE CONCRETO TUBULAR CÔNICO - 12/1000","un",null,2456.92,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680116","POSTE DE CONCRETO TUBULAR CÔNICO - 12/200","un",null,1210.56,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680118","POSTE DE CONCRETO TUBULAR CÔNICO - 10/400","un",null,1222.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680124","POSTE DE CONCRETO DUPLO ´T´ - 6/200","un",null,707.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680125","POSTE DE CONCRETO DUPLO ´T´ - 6/300","un",null,757.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680126","POSTE DE CONCRETO DUPLO ´T´ - 7,5/200","un",null,749.81,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680127","POSTE DE CONCRETO DUPLO ´T´ - 7,5/300","un",null,850.64,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680128","POSTE DE CONCRETO TUBULAR CÔNICO - 7/200","un",null,852.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680129","POSTE DE CONCRETO TUBULAR CÔNICO - 8/200","un",null,1049.58,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680130","POSTE DE CONCRETO TUBULAR CÔNICO - 10/200","un",null,1082.17,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESTRUTURA ESPECÍFICA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680201","ESTAI","un",null,285.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680202","ESTRUTURA TIPO M1","un",null,269.87,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680203","ESTRUTURA TIPO m²","un",null,463.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680204","ESTRUTURA TIPO N3","un",null,601.71,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680205","ESTRUTURA TIPO M1 - N3","un",null,720.5,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680206","ESTRUTURA TIPO M4","un",null,974.73,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680207","ESTRUTURA TIPO N2","un",null,554.68,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680209","ESTRUTURA TIPO N4","un",null,1013.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680210","ARMAÇÃO SECunDÁRIA TIPO 1C - 2R","un",null,108.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680211","ARMAÇÃO SECunDÁRIA TIPO 1C - 3R","un",null,111.59,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680212","ARMAÇÃO SECunDÁRIA TIPO 2C - 3R","un",null,155.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680213","ARMAÇÃO SECunDÁRIA TIPO 2C - 4R","un",null,158.01,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"680214","ARMAÇÃO SECunDÁRIA TIPO 4C - 6R","un",null,242.62,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"682001","RECOLOCAÇÃO DE POSTE DE MADEIRA","un",null,261.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"682004","BRAÇADEIRA CIRCULAR EM AÇO CARBONO GALVANIZADO, DIÂMETRO NOMINAL DE 140 ATÉ 300 MM","un",null,26.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"682005","CRUZETA EM AÇO CARBONO GALVANIZADO PERFIL ´L´ 75 X 75 X 8 MM, COMPRIMENTO 2500 MM","un",null,296.23,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"682012","BENGALA EM PVC PARA RAMAL DE ENTRADA, DIÂMETRO DE 32 MM","un",null,24.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TELEFONIA, LÓGICA E TRANSMISSÃO DE DADOS, EQUIPAMENTOS E SISTEMA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"DISTRIBUIÇÃO E COMANDO, CAIXAS E EQUIPAMENTOS ESPECÍFICOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690301","CONECTOR RJ-45 - FÊMEA - CATEGORIA 5","un",null,12.29,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690309","APARELHO TELEFÔNICO MULTIFREQUENCIAL, COM TECLAS ´FLASH´, ´HOOK´, ´PAUSE´, ´LND´, ´MODE´","un",null,41.65,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690313","CAIXA SUBTERRÂNEA DE ENTRADA DE TELEFONIA, TIPO R1 (60 X 35 X 50) CM, PADRÃO TELEBRÁS, COM TAMPA","un",null,230.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690314","CAIXA SUBTERRÂNEA DE ENTRADA DE TELEFONIA, TIPO R2 (107 X 52 X 50) CM, PADRÃO TELEBRÁS, COM TAMPA","un",null,452.06,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690325","CENTRAL DE TELEFONIA PARA 8 LINHAS E 24 RAMAIS","cj",null,3195.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690331","CAIXA DE TOMADA EM POLIAMIDA E TAMPA PARA PISO ELEVADO, COM 4 ALOJAMENTOS PARA ELÉTRICA E ATÉ 8 ALOJAMENTOS PARA TELEFONIA E DADOS","un",null,89.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690334","CONECTOR RJ-45 FÊMEA - CATEGORIA 6","un",null,23.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690336","CONECTOR RJ-45 FÊMEA - CATEGORIA 6A","un",null,69.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ESTABILIZAÇÃO DE TENSÃO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690501","ESTABILIZADOR ELETRÔNICO DE TENSÃO, MONOFÁSICO, COM POTÊNCIA DE 5 KVA","un",null,5106.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690503","ESTABILIZADOR ELETRÔNICO DE TENSÃO, MONOFÁSICO, COM POTÊNCIA DE 7,5 KVA","un",null,6122.16,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690504","ESTABILIZADOR ELETRÔNICO DE TENSÃO, MONOFÁSICO, COM POTÊNCIA DE 10 KVA","un",null,7382.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690505","ESTABILIZADOR ELETRÔNICO DE TENSÃO, MONOFÁSICO, COM POTÊNCIA DE 15 KVA","un",null,9564.39,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690506","ESTABILIZADOR ELETRÔNICO DE TENSÃO, MONOFÁSICO, COM POTÊNCIA DE 20 KVA","un",null,11274.13,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690515","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 15 KVA","un",null,12409.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690516","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 20 KVA","un",null,13724.47,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690517","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 10 KVA, TENSÃO DE ENTRADA 220 V E DE SAÍDA 110 V","un",null,9562.84,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690519","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 25 KVA","un",null,15825.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690522","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 30 KVA","un",null,17076.14,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690523","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 40 KVA","un",null,21259.91,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690528","ESTABILIZADOR ELETRÔNICO DE TENSÃO, TRIFÁSICO, COM POTÊNCIA DE 150 KVA, COM TRAFO ISOLADOR","un",null,60534.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"SISTEMAS ININTERRUPTOS DE ENERGIA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690601","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO ON LINE SENOIDAL DE 2,4 KVA (110 V/110 V), COM AUTONOMIA DE 15 MINUTOS","un",null,5981.28,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690602","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 10 KVA (220 V/220 V), COM AUTONOMIA DE 15 MINUTOS","un",null,26939.01,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690603","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 20 KVA (220 V/208 V-108 V), COM AUTONOMIA 15 MINUTOS","un",null,34888.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690604","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE SENOIDAL DE 15 KVA (208 V/110 V), COM AUTONOMIA DE 15 MINUTOS","un",null,37115.57,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690605","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO, COM POTÊNCIA DE 2 KVA","un",null,3306.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690608","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO ON LINE SENOIDAL DE 5 KVA (220 V/110 V), COM AUTONOMIA DE 15 MINUTOS","un",null,10191.03,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690610","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO, COM POTÊNCIA ENTRE 5 A 7,5 KVA","un",null,12447.37,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690611","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO DE 600 VA (127 V/127 V), COM AUTONOMIA DE 10 A 15 MINUTOS","un",null,457.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690612","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE SENOIDAL DE 10 KVA (220 V/110 V), COM AUTONOMIA DE 2 HORAS","un",null,35999.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690613","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO ON LINE SENOIDAL DE 10 KVA (110 V/110 V), COM AUTONOMIA DE 30 MINUTOS","un",null,17616.11,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690614","SISTEMA ININTERRUPTO DE ENERGIA, MONOFÁSICO ON LINE SENOIDAL DE 15 KVA (127/127 V) COM AUTONOMIA DE 30 MINUTOS","un",null,22258.53,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690620","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 20 KVA (220/127 V), COM AUTONOMIA DE 15 MINUTOS","un",null,36011.94,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690621","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 60 KVA (220/127 V), COM AUTONOMIA DE 15 MINUTOS","un",null,84403.19,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690622","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 80 KVA (220/127 V), COM AUTONOMIA DE 15 MINUTOS","un",null,107551.32,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690623","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 20 KVA (380/380 V), COM AUTONOMIA DE 15 MINUTOS","un",null,34869.12,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690624","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE DE 20 KVA (380/220 V), COM AUTONOMIA DE 15 MINUTOS","un",null,35708.48,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690628","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE SENOIDAL DE 5 KVA (220/110 V), COM AUTONOMIA DE 15 MINUTOS","un",null,17617.63,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690629","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE SENOIDAL DE 10 KVA (220/110 V), COM AUTONOMIA DE 10 A 15 MINUTOS","un",null,26806.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690630","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE SENOIDAL DE 50 KVA (220/110 V), COM AUTONOMIA DE 15 MINUTOS","un",null,69891.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690632","SISTEMA ININTERRUPTO DE ENERGIA, TRIFÁSICO ON LINE SENOIDAL DE 7,5 KVA (220/110 V), COM AUTONOMIA DE 15 MINUTOS","un",null,21107.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"EQUIPAMENTOS PARA INFORMÁTICA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690801","DISTRIBUIDOR INTERNO ÓPTICO - 1 U PARA ATÉ 24 FIBRAS","un",null,481.93,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"SISTEMA DE REDE",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690925","PATCH CORDS DE 1,50 OU 3,00 M - RJ-45 / RJ-45 - CATEGORIA 6","un",null,28.3,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690926","PATCH PANEL DE 24 PORTAS - CATEGORIA 6","un",null,521.09,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690930","VOICE PANEL DE 50 PORTAS - CATEGORIA 3","cj",null,390.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"690936","PATCH CORDS DE 2,00 OU 3,00 M - RJ-45 / RJ-45 - CATEGORIA 6A","un",null,105.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"TELECOMunICAÇÕES",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"691013","AMPLIFICADOR DE POTÊNCIA PARA VHF E CATV-50 DB, FREQUENCIA 40 A 550 MHZ","un",null,356.14,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"691014","ANTENA PARABÓLICA COM CAPTADOR DE SINAIS E MODULADOR DE ÁUDIO E VÍDEO","cj",null,602.86,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692001","ARAME DE ESPINAR EM AÇO INOXIDÁVEL NU, PADRÃO TELESP","m",null,2.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692002","BRAÇADEIRA AJUSTÁVEL PARA POSTE TUBULAR, TIPO BAP 2, PADRÃO TELEBRÁS","un",null,9.84,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692003","SUPORTE PARA ISOLADOR ROLDANA TIPO SIR, PADRÃO TELEBRÁS","un",null,10.22,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692004","ISOLADOR ROLDANA EM PORCELANA DE 72 X 72 MM","un",null,6.79,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692005","SUPORTE PARA ISOLADOR ROLDANA TIPO DM, PADRÃO TELEBRÁS","un",null,5.51,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692007","FITA EM AÇO INOXIDÁVEL PARA POSTE DE 0,50 M X 19 MM, COM FECHO EM AÇO INOXIDÁVEL","un",null,5.83,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692010","TAMPA PARA CAIXA R1, PADRÃO TELEBRÁS","un",null,157.27,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692011","TAMPA PARA CAIXA R2, PADRÃO TELEBRÁS","un",null,306.24,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692013","BLOCO DE LIGAÇÃO INTERNA PARA 10 PARES, BLI-10","un",null,10.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692014","BLOCO DE LIGAÇÃO ENGATE RÁPIDO PARA 10 PARES, BER-10","un",null,19.28,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692017","CALHA DE AÇO PARA 4 TOMADAS 2P+T - 250 V, COM CABO","un",null,59.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692018","CORDÃO ÓPTICO DUPLEX, MULTIMODO COM CONECTOR LC/LC - 2,5 M","un",null,86.31,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692019","EXTENSÃO ÓPTICO SIMPLEX COM CONECTOR LC","un",null,32.74,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692020","BANDEJA FIXA PARA RACK, 19´ X 500 MM","un",null,58.9,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692021","BANDEJA FIXA PARA RACK, 19´ X 800 MM","un",null,97.55,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692022","BANDEJA DESLIZANTE PARA RACK, 19´ X 800 MM","un",null,201.05,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692023","CALHA DE AÇO COM 8 TOMADAS 2P+T - 250 V, COM CABO","un",null,63.77,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692024","CALHA DE AÇO COM 12 TOMADAS 2P+T - 250 V, COM CABO","un",null,88.45,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692025","PAINEL FRONTAL CEGO, 19´ X 2 U","un",null,11.35,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692026","PROTETOR DE SURTO HÍBRIDO PARA REDE DE TELECOMunICAÇÕES","un",null,36.07,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692027","DIVISOR INTERNO COM 1 ENTRADA E 2 SAÍDAS - 75 OHMS","un",null,10.17,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692028","DIVISOR INTERNO COM 1 ENTRADA E 4 SAÍDAS - 75 OHMS","un",null,12.7,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692029","TOMADA BLINDADA PARA VHF/UHF, CATV E FM, FREQUÊNCIA 5 MHZ A 1 GHZ","un",null,10.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692030","BLOCO DE DISTRIBUIÇÃO COM PROTETOR DE SURTOS, PARA 10 PARES, BTDG-10","un",null,41.82,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692034","TOMADA PARA TV, TIPO PINO JACK, COM PLACA","cj",null,10.33,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"692035","CAIXA DE EMENDA VENTILADA EM POLIPROPILENO, PARA ATÉ 200 PARES","un",null,54.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"COMunICAÇÃO VISUAL",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ADESIVOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970101","ADESIVO VINÍLICO, PADRÃO REGULAMENTADO, PARA SINALIZAÇÃO DE INCÊNDIO","un",null,15.69,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PLACAS, PÓRTICOS E OBELISCOS ARQUITETÔNICOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970203","PLACA COMEMORATIVA EM AÇO INOXIDÁVEL ESCOVADO","m²",null,2804.39,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970219","PLACA DE IDENTIFICAÇÃO EM ACRÍLICO COM TEXTO EM VINIL","m²",null,638.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970221","PLACA DE SINALIZAÇÃO EM PVC PARA AMBIENTES","un",null,99.88,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PINTURA DE LETRAS E PICTOGRAMAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970301","SINALIZAÇÃO COM PICTOGRAMA EM TINTA ACRÍLICA","un",null,29.46,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PINTURA DE SINALIZAÇÃO VIÁRIA",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970401","SINALIZAÇÃO HORIZONTAL COM TINTA VINÍLICA OU ACRÍLICA","m²",null,15.52,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970402","SINALIZAÇÃO HORIZONTAL COM TERMOPLÁSTICO TIPO HOT-SPRAY","m²",null,35.02,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"PLACAS, PÓRTICOS E SINALEIRAS VIÁRIAS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970510","SINALIZAÇÃO VERTICAL EM PLACA DE AÇO GALVANIZADA COM PINTURA EM ESMALTE SINTÉTICO","m²",null,550.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970513","COLOCAÇÃO DE PLACA EM SUPORTE DE MADEIRA / METÁLICO - SOLO","m²",null,32.4,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"970514","SUPORTE DE PERFIL METÁLICO GALVANIZADO","kg",null,14.08,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"ARQUITETURA DE INTERIORES",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"MOBILIÁRIO",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"980221","BANCO DE MADEIRA COM ENCOSTO E PÉS EM FERRO FunDIDO PINTADO","un",null,251.75,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,"REPAROS, CONSERVAÇÕES E COMPLEMENTOS",null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CPOS"]
[null,null,null,null,null,null,null,null,null,null,"982002","CAPACHO EM FIBRA NATURAL","m²",null,156.88,"CPOS"]

{"sheet":"Reparo Profundo","index":1,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["REPARO PROFUNDO",316.11,"m²","espessura (m)"]
["CONCRETO ASFALTICO GRADUACAO I",15.805500000000002,"m³",0.05]
["CONC.ASF.US.QUENTE - BINDER GRAD.A C/DOP",31.611000000000004,"m³",0.1]
["CONCRETO FCK 15 MPA",63.22200000000001,"m³",0.2]
["DEMOLIÇÃO",110.63850000000002,"m³",0.35000000000000003]
["IMPRIMAÇÃO IMPERMEABILIZANTE",316.11,"m²",1]
["IMPRIMAÇÃO LIGANTE",632.22,"m²",2]

{"sheet":"Plan3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}